DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20171 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Utility Fail (20171)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Utility Fail (20171)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Indicates that the utility input power is not within predetermined limits. This could be, but is not limited to, over voltage, under voltage, over frequency, under frequency or over current.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20172 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Utility Fail Cleared (20172)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Utility Fail Cleared (20172)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Indicates that the utility input power is within predetermined limits.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20181 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Utility Not Present (20181)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Utility Not Present (20181)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Indicates that the utility input is not present. This differs from alarm #57 in that the detected voltage is zero in this case.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20182 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Utility Not Present Cleared (20182)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Utility Not Present Cleared (20182)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Indicates that the utility input is present.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20191 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Bypass Manual Turned On (20191)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Bypass Manual Turned On (20191)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The bypass has been given a manual turn on command.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20192 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Bypass Manual Turned Off (20192)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Bypass Manual Turned Off (20192)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The bypass has been given a manual turn off command.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20201 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Site Wiring Fault (20201)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Site Wiring Fault (20201)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a fault in the input wiring, other than Phase Rotation: e.g., Ground/Neutral reversed. Recommendations: 1. Contact an electrician.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20202 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Site Wiring Fault Cleared (20202)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Site Wiring Fault Cleared (20202)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a fault in the input wiring, other than Phase Rotation: e.g., Ground/Neutral reversed. Recommendations: 1. Contact an electrician.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21060 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS is no longer on manual bypass (21060)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS is no longer on manual bypass (21060)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is operating in manual bypass mode. Recommendations: 1. In bypass mode, the UPS cannot support devices if there is a power failure. 2. Once maintenance has been performed return the UPS to normal mode.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21059 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS is on manual bypass (21059)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS is on manual bypass (21059)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is operating in manual bypass mode. Recommendations: 1. In bypass mode, the UPS cannot support devices if there is a power failure. 2. Once maintenance has been performed return the UPS to normal mode.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20152 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Utility power has been restored (20152)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Utility power has been restored (20152)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device has been started while on battery power. AC input power is not present. Recommendations: 1. Check to make sure the UPS is plugged into an outlet supplied with utility power. If the UPS remains on battery for an extended time it'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='will not be able to sustain the output load!  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 20151 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS was started without utility power (20151)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS was started without utility power (20151)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device has been started while on battery power. AC input power is not present. Recommendations: 1. Check to make sure the UPS is plugged into an outlet supplied with utility power. If the UPS remains on battery for an extended time it'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='will not be able to sustain the output load.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21022 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Input voltage is normal (21022)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Input voltage is normal (21022)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting input voltage is out of range. Recommendations: 1. Check to make sure the UPS is plugged into an outlet supplied with utility power. 2. If the UPS remains on battery for an extended period of time it will not be able'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='to sustain the load.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21021 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Input voltage is out of range (21021)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Input voltage is out of range (21021)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting input voltage is out of range. Recommendations: 1. Check to make sure the UPS is plugged into an outlet supplied with utility power. 2. If the UPS remains on battery for an extended period of time it will not be able'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='to sustain the load.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21007 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS temperature out of range (21007)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS temperature out of range (21007)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting temperature is out of range. Recommendations: 1. Check to make sure the UPS is in a well ventilated area. 2. Lower the ambient temperature in the area where the UPS is located.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21008 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS temperature has returned to normal (21008)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS temperature has returned to normal (21008)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting temperature is out of range. Recommendations: 1. Check to make sure the UPS is in a well ventilated area. 2. Lower the ambient temperature in the area where the UPS is located.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21047 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS is on automatic bypass (21047)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS is on automatic bypass (21047)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is operating in auto bypass mode. Recommendations: 1. In bypass mode, the UPS cannot support devices if there is a power failure. 2. Once maintenance has been performed return the UPS to normal mode.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21048 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS is no longer on auto bypass (21048)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS is no longer on auto bypass (21048)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is operating in auto bypass mode. Recommendations: 1. In bypass mode, the UPS cannot support devices if there is a power failure. 2. Once maintenance has been performed return the UPS to normal mode.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21019 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Output voltage is out of range (21019)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Output voltage is out of range (21019)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting output voltage is out of Range. Recommendations: 1. Initiate a UPS self test. 2. If this error persists contact technical support.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21053 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - One or more UPS batteries have been disconnected. (21053)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - One or more UPS batteries have been disconnected. (21053)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting batteries are not connected to the UPS. Recomendations: 1. Connect the UPS Batteries. The UPS will not be capable of supporting it s load if the utility power fails!'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21054 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - All UPS batteries have been reconnected. (21054)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - All UPS batteries have been reconnected. (21054)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting batteries are not connected to the UPS. Recomendations: 1. Connect the UPS Batteries. The UPS will not be capable of supporting it s load if the utility power fails!'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21057 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS batteries are in a discharged condition. (21057)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS batteries are in a discharged condition. (21057)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting batteries are completely discharged. Recommendations: 1. Connect the UPS to utility power to charge the batteries. The UPS will not be able to support it s load if the utility power fails!'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21058 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS batteries are in a discharged condition. (21058)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS batteries are in a discharged condition. (21058)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting batteries are completely discharged. Recommendations: 1. Connect the UPS to utility power to charge the batteries. The UPS will not be able to support it s load if the utility power fails!'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21041 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - A UPS circuit breaker needs attention. (21041)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - A UPS circuit breaker needs attention. (21041)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting an output Breaker or Relay has failed or may be stuck open or closed with this alarm. Recommendations: 1. Check all breakers on the UPS. 2. If this error persists contact technical support.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21042 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - All breakers are functioning normally. (21042)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - All breakers are functioning normally. (21042)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting an output Breaker or Relay has failed or may be stuck open or closed with this alarm. Recommendations: 1. Check all breakers on the UPS. 2. If this error persists contact technical support.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21037 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Emergency Power Off activated (21037)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Emergency Power Off activated (21037)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting an Emergency Power Off (EPO) command has been received to shutdown the UPS immediately with out delay. This command may come from a local control panel or from a remote source. Recommendations: 1. Turn the UPS on to'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='reapply power to attached equipment.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21033 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS output has been manually turned off. (21033)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS output has been manually turned off. (21033)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The UPS has been powered off with user interaction.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21034 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - UPS output has been restored (21034)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - UPS output has been restored (21034)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The UPS has been powered off with user interaction.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21045 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - A cover panel has been removed. (21045)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - A cover panel has been removed. (21045)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a cover panel has been removed while utility power is present. Recommendations: 1. Reinstall all panels. 2. If this error persists contact technical support.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21046 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - A cover panel has been replaced. (21046)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - A cover panel has been replaced. (21046)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a cover panel has been removed while utility power is present. Recommendations: 1. Reinstall all panels. 2. If this error persists contact technical support.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21035 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS has encountered an fan failure. (21035)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS has encountered an fan failure. (21035)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a fan failure has occurred. Recommendations: 1. If this error persists contact technical support.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21036 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS fan failure has cleared. (21036)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS fan failure has cleared. (21036)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a fan failure has occurred. Recommendations: 1. If this error persists contact technical support.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21023 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS N+1 load has been exceeded (21023)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS N+1 load has been exceeded (21023)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a loss of redundancy due to one of the following. 1. One or more of the Electronics Modules has failed 2. One or more of the electronics modules has been manually removed. 3. The amount of load on the UPS has'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='increased to the point that the UPS is no longer able to support an N+1 configuration. Recommendations: 1. Check the UPS to see if one of the modules has failed. 2. Make sure that all modules are securely plugged in. 3. Reduce the load to  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='return the N+1 configuration. 4. If the amount of load is now going to exceed and N+1 configuration permanently, change the configuration on the front panel of the UPS to Capacity instead of Parallel N+1." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21024 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Loss of redundancy cleared or configuration has changed from N+1 to Capacity (21024)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Loss of redundancy cleared or configuration has changed from N+1 to Capacity (21024)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a loss of redundancy due to one of the following. 1. One or more of the Electronics Modules has failed 2. One or more of the electronics modules has been manually removed. 3. The amount of load on the UPS has'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='increased to the point that the UPS is no longer able to support an N+1 configuration. Recommendations: 1. Check the UPS to see if one of the modules has failed. 2. Make sure that all modules are securely plugged in. 3. Reduce the load to  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='return the N+1 configuration. 4. If the amount of load is now going to exceed and N+1 configuration permanently, change the configuration on the front panel of the UPS to Capacity instead of Parallel N+1." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21013 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - A UPS shutdown is imminent. (21013)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - A UPS shutdown is imminent. (21013)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a shutdown imminent condition. Recommendations: 1. Immediately restore power to the UPS. The UPS will not continue to supply power to devices following the shutdown!'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21014 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS is no longer in an imminent shutdown state. (21014)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS is no longer in an imminent shutdown state. (21014)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a shutdown imminent condition. Recommendations: 1. Immediately restore power to the UPS. The UPS will not continue to supply power to devices following the shutdown!'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21011 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - A UPS shutdown is pending. (21011)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - A UPS shutdown is pending. (21011)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting shutdown pending condition. Recommendations: 1. Immediately restore power to the UPS. The UPS will not continue to supply power to devices following the shutdown!'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 21012 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - The UPS is no longer pending shutdown. (21012)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - The UPS is no longer pending shutdown. (21012)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting shutdown pending condition. Recommendations: 1. Immediately restore power to the UPS. The UPS will not continue to supply power to devices following the shutdown!'

