DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7875 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Read EEPROM failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Read EEPROM failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to read the EEPROM (FRUID) on the System Backplane failed'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7877 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Read command on System Backplane I2C bus failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Read command on System Backplane I2C bus failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A read command on the system backplane I2C bus failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7878 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Write command on System Backplane I2C bus failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Write command on System Backplane I2C bus failed: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A write command on the system backplane I2C bus failed. The type of command that failed can be identified by the activity status field (last byte) of the encoded field. B = RC Cable Configuration Register write C = Backplane Voltage Margin'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Register write 9 = Flex circuit configuration register write  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7879 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Syatem Backplane Power Fault'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Syatem Backplane Power Fault: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Local Power Monitor on the named System Backplane has detected a power fault. The failing Backplane Power Board status is read from the Backplane LPM I2C interface register and the value is placed in the data field of the event (bits'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='15-8).  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7880 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System Backplane voltage margin failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System Backplane voltage margin failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Margining voltage to the System Backplane has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7891 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure to write data to FRUID EEPROM'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure to write data to FRUID EEPROM: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to write data to the FRUID EEPROM by the MFG level MP command WF failed. The FRU handle of the failing FRUID is embedded in the two uppermost bytes of the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7892 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU fan failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU fan failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The fan on a CPU is not operating in a manner that provides enough air flow to cool the processor'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7893 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU fan failing'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU fan failing: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The fan on a CPU is operating in a manner that provides enough air flow to cool the processor but is not at normal operation'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7894 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CC chip fan failed'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CC chip fan failed: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The fan on a CC chip is not operating in a manner that provides enough air flow to cool the processor'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7895 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CC chip fan failing'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CC chip fan failing: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The fan on a CC chip is operating in a manner that provides enough air flow to cool the processor but is not at normal operation'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7902 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDH Controller firmware version is not supported with this version of MP FW'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDH Controller firmware version is not supported with this version of MP FW: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The MP checked the FW revision of the PDHC identified in the physical location data field and discovered that it did not recognize the revision as one that it has been qualed with. This is an unsupported configuration.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7903 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Power fault on cell board'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Power fault on cell board: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The local Power Monitor is reporting a fault with the named Cell Power Board.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7938 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The CPU Node reported a problem initializing its node in the device tree'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The CPU Node reported a problem initializing its node in the device tree: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The CPU node retuned an error when calling its initialize node function. The specific status is displayed in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7939 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The ExecuteCommand function failed on a CPU.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The ExecuteCommand function failed on a CPU.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='ExecuteCommand issues commands that execute on remote CPUs via IPI interrupts. If the command failed to execute, this event is printed and the data field contains the status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7940 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A remote CPU is not prepared to receive a command'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A remote CPU is not prepared to receive a command: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A remote CPU is in a state where it cannot receive and execute a new command. The current status of the CPU is provided in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7948 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was encountered when executing a PAL_PROC'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was encountered when executing a PAL_PROC: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error was encountered when executing a PAL_PROC. This code will be emitted in pairs. The Proc INDEX will be in the data of the first chassis code. The status is in the second data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7953 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPUs loaded in wrong order'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPUs loaded in wrong order: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='CPUs not loaded in correct order. Correct loading order is CPU 0, 1, 2, 3.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7963 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XBC SBE and LPE errors were not cleared properly'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XBC SBE and LPE errors were not cleared properly: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The XBC logged a SBE or LPE after they should have been cleared. Either the clear failed, or a new error was logged immediately. Data field: XBC number (32:43), port number (44:55), port status information (0:31)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7964 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The CC to XBC link pattern test failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The CC to XBC link pattern test failed.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The CC to XBC Link pattern test failed. Data Field: This event will be emitted three times 1st event: XBC number (32:43), port number (44:55) 2nd event: expected pattern (0:63) 3rd event: actual data read (0:63)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7965 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error Reading a platform storage variable from the PDHC/MP'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error Reading a platform storage variable from the PDHC/MP: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware was unable to complete a platform storage read command from the utilities system. The exact status printed in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7966 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error was returned on a Platform Storage Write Command to the PDHC/MP'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error was returned on a Platform Storage Write Command to the PDHC/MP: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware was unable to complete a platform storage write command. The actual status is returned in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7973 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The Sequencer was unable to find/use a needed tree node'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The Sequencer was unable to find/use a needed tree node: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Sequencer was unable to find the tree node it needed to complete an operation. The tree node is in the ascii in the data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7974 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware encountered an error in processing the partition variables'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware encountered an error in processing the partition variables: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware atempted to read a partition variable from the GSP and store it in options. An error was encountered during this process. The data field contains the partition variable element ID that was being processed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7975 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A non-critical cell power fault has occurred'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A non-critical cell power fault has occurred: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='One or more power converter on the Cell or Cell Power Board has reported a fault. However, because of redundancy in the power system, the power to the Cell is still good. The data field contains detailed power fault location information (see'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Cell ERS for more information). Data Byte[0]: bit0 - Power_Fault status, bit1 - Power_Good status Data Byte[1]: Contents of Power Board Converter Status register. Data Byte[2]: Contents of Cell Converter Status register. Data Byte[3]: Contents  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='of CPU Module Power Status register." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8009 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPUProcConfigValue in /options is not compatible with the current PAL/CPU'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPUProcConfigValue in /options is not compatible with the current PAL/CPU: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='CPUProcConfigValue setting in options as been compared with what is reported by PAL as settable and CPUProcConfigValue is specifying at least one bit that is not supported by this version of PAL using the Get Processor Dependent Features. This'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='chassis code is emmitted in pairs, the first data field contains the PAL expected values; the second data field contains the requested setting from options.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8010 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware was unable to determine the Processor Dependent Features'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware was unable to determine the Processor Dependent Features: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System firmware was unable to successfully issue the PAL_GET_PROC_FEATURES PAL proc. The data field is unused'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8127 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Data field contains data meant for firmware debug only.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Data field contains data meant for firmware debug only.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This event is a tool to aid in the debugging and testing of firmware.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8128 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The CLU has encountered an undefined case'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The CLU has encountered an undefined case: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The CLU has encountered an undefined case in its control flow.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8130 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unknown Cell voltage margin has been detected.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unknown Cell voltage margin has been detected.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The Cell voltage margin settings do not match the Normal, +5%, or -5% values.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8131 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The run-time verification of a programming assumption has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The run-time verification of a programming assumption has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='For debug purposes, many assumptions made by the PDHC developer(s) are checked at run-time. If this event log is seen, it will either indicate that the hardware is in a unknown state that is not handled by the PDHC, or that a programming bug'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='has been found. For developer debug purposes, the data field describes where in the code that the error was detected. Data Bytes[0-1]: The line number within the source code file where the error was detected. Data Bytes[2-7]: The first 6  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='characters of the source code file name." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8132 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unknown error has been detected by the PDHC firmware.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unknown error has been detected by the PDHC firmware.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An unknown error has been detected by the PDHC firmware. For developer debug purposes, the data field describes where in the code that the error was detected. Data Bytes[0-1]: The line number within the source code file where the error was'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='detected. Data Bytes[2-7]: The first 6 characters of the source code file name.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8133 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An attempt to write to a device on the PDHCs I2C bus has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An attempt to write to a device on the PDHCs I2C bus has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to write to a device on the PDHC s I2C bus has failed. The devices on the I2C bus are the Cell s FRU EEPROM, the Cell Power Board s FRU EEPROM, the voltage margining D-to-A converters, and, if they are accessible, the CPU Module'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Power Pods  FRU EEPROMs. The Data field information contains information that can identify the exact device that has failed. Refer to the Cell ERS for a mapping of I2C device addresses to devices. Data Bytes[0-1]: Reserved Data Bytes[2-3]: I2C  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='Device Address Data Bytes[4-5]: Starting Word Address Data Bytes[6-7]: Size of attempted access (in bytes)." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8134 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An attempt to read from a device on the PDHC s I2C bus has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An attempt to read from a device on the PDHC s I2C bus has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to read from a device on the PDHC s I2C bus has failed. The devices on the I2C bus are the Cell s FRU EEPROM, the Cell Power Board s FRU EEPROM, the voltage margining D-to-A converters, and, if they are accessible, the CPU Module'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Power Pods  FRU EEPROMs. The Data field information contains information that can identify the exact device that has failed. Refer to the Cell ERS for a mapping of I2C device addresses to devices. Data Bytes[0-1]: Reserved Data Bytes[2-3]: I2C  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='Device Address Data Bytes[4-5]: Starting Word Address Data Bytes[6-7]: Size of attempted access (in bytes)." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8135 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An attempt to write to a device on the PDHC s SM bus has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An attempt to write to a device on the PDHC s SM bus has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to write to a device on the PDHC s SM bus has failed. The devices on the SM bus are the CPU modules  FRU EEPROMs, the CPU modules  Processor Information ROMs, and the CPU modules  thermal sensors. The Data field information contains'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='information that can identify the exact device that has failed. Refer to the Cell ERS for a mapping of SM Bus device addresses to devices. Data Bytes[0-1]: Reserved Data Bytes[2-3]: SM bus Device Address Data Bytes[4-5]: Starting Word Address  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='Data Bytes[6-7]: Size of attempted access (in bytes)." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8136 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An attempt to read from a device on the PDHC s SM bus has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An attempt to read from a device on the PDHC s SM bus has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An attempt to read from a device on the PDHC s SM bus has failed. The devices on the SM bus are the CPU modules  FRU EEPROMs, the CPU modules  Processor Information ROMs, and the CPU modules  thermal sensors. The Data field information'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='contains information that can identify the exact device that has failed. Refer to the Cell ERS for a mapping of SM Bus device addresses to devices. Data Bytes[0-1]: Reserved Data Bytes[2-3]: SM bus Device Address Data Bytes[4-5]: Starting Word  '
DEFine MSGACTion Name=(*,40)
ACTION=ANNOTATE TEXT='Address Data Bytes[6-7]: Size of attempted access (in bytes)." '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8137 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Cell boot has been disabled due to a failure setting the frequency registers.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Cell boot has been disabled due to a failure setting the frequency registers.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The PDHC did not read valid frequency information from the CPU modules  or Cell s FRU EEPROMs, or the frequency registers would not update properly. Following this event, the Cell will not boot until the problem is corrected and Cell Power has'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='been turned off, then on again, using the PE command.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 8138 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error has occurred while updating System FW.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error has occurred while updating System FW.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error has occurred while updating System FW. More details about the update failure may be available as displayed by the Firmware Update Utility (FWUU).'

