DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5836 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI unable to write privilege level during security initialization'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI unable to write privilege level during security initialization: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='As part of normal security initialization, EFI attempted to record the current privilege level. This attempt failed. EFI is unable to initialize the security system. Data Field: Return status from internal EFI function.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5837 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event EFI was denied permission to write the privilege level during security init'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event EFI was denied permission to write the privilege level during security init: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='As part of normal security initialization, EFI attempted to record the current privilege level. This attempt failed with a privilege violation error. EFI is unable to initialize the security system. Data Field: Return status from internal EFI'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='function.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5853 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event OS dump, error writing image area to disk (E055)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event OS dump, error writing image area to disk (E055): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='OS dump, error writing image area to disk (E055)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 5896 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Coherency controller (CC) registers indicate a Deadlock Recovery Reset'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Coherency controller (CC) registers indicate a Deadlock Recovery Reset: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Early in bootstrap, the coherency controller (CC) registers are checked for Deadlock Recovery Reset. This chassis code indicates that CC logs will be stored to NVRAM.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 6074 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A DIMM loading order error has occurred'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A DIMM loading order error has occurred: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The loading order of the DIMMs is incorrect. The cell is halted.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 6146 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Refresh Control Error Timeout'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Refresh Control Error Timeout: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Timeout Waiting for SDRAM parts to become ready - mem_status[0] Refresh Control Register'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 6180 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event memory extender/baseboard FRU mismatch'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event memory extender/baseboard FRU mismatch: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The version of Memory extender installed in the system has not been qualified to work with the version of the baseboard installed in the system.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 6730 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fabric topology mismatch with XBCs in complex'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fabric topology mismatch with XBCs in complex: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There is a fabric topology mismatch with the XBCs in the complex. Data Field: (Topology of XBC << 32) | Topology of destination XBC 0x00 Topology not yet determined 0x30 Domelight 0x40 U-Turn (Left cabinet) 0x41 U-Turn (Right cabinet) 0x42'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='Cross-Flex 0x43 U-Turn  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 6795 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An invalid XBC to XBC port was found.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An invalid XBC to XBC port was found.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='While routing the XBC to XBC ports, an invalid port was encountered. The data field is the crossbar number (32:43) and the port number (44:55).'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7652 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not get neighbor information.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not get neighbor information.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The XBC could not get neighbor information. Data Field: XBC # << 32 | internal port attempting to access neighbor'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7653 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XBC s routing state was marked as in ERROR'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XBC s routing state was marked as in ERROR: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='For the XBC being routed, routing has already been attempted, but an error occurred. Inspect chassis codes from other cells for more details regarding the nature of the problem. The data field consists of the XBC number (32:63)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7655 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event It indicates that there is no NVM error space left for logging an Error Event.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event It indicates that there is no NVM error space left for logging an Error Event.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This means that the error event log cannot be logged to the persistent storage. The data field gives the event type that was supposed to be logged.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7657 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An XBC port found to have an unexpected error.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An XBC port found to have an unexpected error.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An XBC port was found to have an unexpected error. The data field consists of the crossbar number (32:63) and the current port errors (0:31)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7658 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A XBC port route around has occurred'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A XBC port route around has occurred: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During fabric routing a port on a XBC was found in error or had been previously marked as in error. PDC will route around this XBC port. Data Field: XBC number (32:63) and external XBC port number (0:31)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7660 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event During routing a crossbar is found to be in an uexpected routing state.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event During routing a crossbar is found to be in an uexpected routing state.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Data field: the unexpected forward progress state (0:31) XBC number (32:44) Cell number (56:63)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7661 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An unexpected XBC forward progress state was continually found until timing out.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An unexpected XBC forward progress state was continually found until timing out.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A crossbar was found to be in an unexpected forward progress state during fabric routing. This crossbar stayed in the unexpected state until Fabric Discovery timed out. Data fied: unexpected forward progress (0:31) XBC number (32:44) Cell'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='number (56:63)  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7663 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event During remote routing, the current port s neighbor is not healthy.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event During remote routing, the current port s neighbor is not healthy.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An XBC port was found that is not healthy. This indicates at least one of the following about the port: - Hardware link is not okay - Presence detect is false - Fatal error detected - SBE detected - LPE detected - Port landmined The data field'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='of the chassis code indicates which port is unhealthy, as well as the fabric routing state before the problem was encountered.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7664 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The CC to XBC link is not viable.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The CC to XBC link is not viable.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The CC to XBC link is not viable.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7666 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Remote routing a crossbar failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Remote routing a crossbar failed.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='There was a problem performing remote routing on the local XBC. Chassis codes sent before this one may provide more details about the exact nature of the problem. The data field consists of the XBC number that failed routing (32:63)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7667 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Too many XBC-to-XBC were broken in the complex.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Too many XBC-to-XBC were broken in the complex.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Two or more XBC-XBC links were found to be broken. The data field is the XBC number (32:63) and a bit map of the ports broken (0:31)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7669 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event This cell did not get the XBC Global Semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event This cell did not get the XBC Global Semaphore.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='After unlocking the XBC Global Semaphore for a takeover, this cell did not get the semaphore.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7671 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Attempted an XBC SM4 takeover and timed out trying to unlock the SM4.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Attempted an XBC SM4 takeover and timed out trying to unlock the SM4.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='When a cell holds an XBC semaphore for an extended period of time, fabric will attempt to takeover the semaphore so that the rest of the cells will have access to it. Fabric will attempt to take the SM4 for a period of time. If it is unable to'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='unlock the SM4 within the timeout period, it will send this chassis code and halt the cell. Data field: XBC number (32:63) and current owner (cell) of the semaphore (0:31)  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7673 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Waiting for the XBC Global Semaphore has timed out.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Waiting for the XBC Global Semaphore has timed out.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During Fabric Discovery, the cell will wait until it gets the XBC s Global Semaphore. It waits for a very long time. This chassis code indicates that the wait has timed out.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7674 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A timeout occurred while attempting to release the XBC semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A timeout occurred while attempting to release the XBC semaphore.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The XBC Release Semaphore timeout is designed to fail last. The semaphore could not be released. Any other cell (even outside the PD) may be blocked because the XBC is a global resource. Data field: current semaphore owner (0:31) XBC number'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='(32:43) port number (44:55) cell number (56:63)  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7684 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Management Processor Firmware Battery Failure or NVRAM change'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Management Processor Firmware Battery Failure or NVRAM change: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Management Processor Firmware detected improper data in NVRAM (bad checksums.) Either the NVRAM layout changed, or the Management Processor Battery may not be maintaining the data through A/C power cycles.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7685 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Management Processor Firmware Software Error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Management Processor Firmware Software Error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Management Processor Firmware detected a software error and is logging an event. The data represents data associated with the error seen.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7686 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Management Processor detected an I2C Communication Error with BMC.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Management Processor detected an I2C Communication Error with BMC.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An I2C Communication failure with the Baseboard Management Controller was detected. Without I2C communication, the system cannot be powered on/off or reset.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7690 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A CRC error was discovered when verifying the ROM'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A CRC error was discovered when verifying the ROM: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A stored CRC value did not match the calculated CRC value for the specified address.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7718 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event (HWE) IO backplane type unknown'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event (HWE) IO backplane type unknown: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='See Summary.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7732 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU Revisions did not match'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU Revisions did not match: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='2 cpus in the system are reporting different revisions. This event will be emitted in greoups of 3 with the two revisions reported in the first 2 data fields and the cpu number in the 3rd data field.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7733 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event 2 cpus are running at mismatched frequencies.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event 2 cpus are running at mismatched frequencies.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='This chassis code will be emitted in pairs. 2 cpus are reporting that they are running at different frequencies. The two frequencies are reported in the data fields.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7734 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A cpu is being overclocked'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A cpu is being overclocked: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The rating for the cpu and the actual speed will be emitted in 2 sequencial event data fields.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7758 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Copy of complex profile on sub and cells don t match'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Copy of complex profile on sub and cells don t match: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The complex profile is stored in NVRAM on the MP and each cell. All copies must match. For this error to be generated, not only is the MP s copy of the complex profile invalid, but not all of the cell s copies match.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7760 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Duplicate cabinet number detected'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Duplicate cabinet number detected: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The MP detected 2 or more cabinets with the same cabinet number.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7767 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MP ID command must be run'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MP ID command must be run: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The complex identification information in group A of the complex profile is invalid. The MP (Managability Processor) command  ID  must be run. The SSKEY hardware is required.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7771 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event MP Battery is low'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event MP Battery is low: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The battery on the SBCH is below the safe threshold. The battery can be replaced online.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7773 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Partition being reset due to watchdog timeout expiring'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Partition being reset due to watchdog timeout expiring: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The partition is being reset because its watchdog timer expired and automatic restart is enabled.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 7774 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PDHC FW was reset by hardware due to firmware inactivity.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PDHC FW was reset by hardware due to firmware inactivity.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The processor dependent hardware controller (PDHC) on the cell board had its watchdog timer expire. The PDHC will reset the watchdog as the main program runs. If the watchdog does not get reset within 7 seconds the timer will expire, resetting'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='the PDHC.  '

