#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 1 * * * * 1*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: OTHER (Power Supply Bay: Other)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: OTHER (Power Supply Bay: Other)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 1 * * * * 2*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: NO UPS (Power Supply Bay: Other)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: NO UPS (Power Supply Bay: Other)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 1 * * * * 3*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: OK (Power Supply Bay: Other)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: OK (Power Supply Bay: Other)'
       SEVERITY=S
       ATTRIB=default
       COLOR=GREEN

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 1 * * * * 4*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: POWER FAILED (Power Supply Bay: Other)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: POWER FAILED (Power Supply Bay: Other)'
       SEVERITY=E
       ATTRIB=default
       COLOR=RED

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 1 * * * * 5*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: BATTERY LOW (Power Supply Bay: Other)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: BATTERY LOW (Power Supply Bay: Other)'
       SEVERITY=W
       ATTRIB=default
       COLOR=ORANGE




DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 2 * * * * 1*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: OTHER (Power Supply Bay: PowerBay1)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: OTHER (Power Supply Bay: PowerBay1)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 2 * * * * 2*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: NO UPS (Power Supply Bay: PowerBay1)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: NO UPS (Power Supply Bay: PowerBay1)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 2 * * * * 3*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: OK (Power Supply Bay: PowerBay1)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: OK (Power Supply Bay: PowerBay1)'
       SEVERITY=S
       ATTRIB=default
       COLOR=GREEN

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 2 * * * * 4*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: POWER FAILED (Power Supply Bay: PowerBay1)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: POWER FAILED (Power Supply Bay: PowerBay1)'
       SEVERITY=E
       ATTRIB=default
       COLOR=RED

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 2 * * * * 5*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: BATTERY LOW (Power Supply Bay: PowerBay1)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: BATTERY LOW (Power Supply Bay: PowerBay1)'
       SEVERITY=W
       ATTRIB=default
       COLOR=ORANGE




DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 3 * * * * 1*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: OTHER (Power Supply Bay: PowerBay2)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: OTHER (Power Supply Bay: PowerBay2)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 3 * * * * 2*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: NO UPS (Power Supply Bay: PowerBay2)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: NO UPS (Power Supply Bay: PowerBay2)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 3 * * * * 3*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: OK (Power Supply Bay: PowerBay2)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: OK (Power Supply Bay: PowerBay2)'
       SEVERITY=S
       ATTRIB=default
       COLOR=GREEN

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 3 * * * * 4*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: POWER FAILED (Power Supply Bay: PowerBay2)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: POWER FAILED (Power Supply Bay: PowerBay2)'
       SEVERITY=E
       ATTRIB=default
       COLOR=RED

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8018 * * * * * * * * * * * * * * * * * * * * * * * * * * 3 * * * * 5*'
       MSGNODE=*
       DEScription='HP - Power Supply UPS Status Change: BATTERY LOW (Power Supply Bay: PowerBay2)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Power Supply UPS Status Change: BATTERY LOW (Power Supply Bay: PowerBay2)'
       SEVERITY=W
       ATTRIB=default
       COLOR=ORANGE



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 1 * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: OTHER (Sensor Location: Other)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: OTHER (Sensor Location: Other - &46 degrees Celsius)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 1 * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: OK (Sensor Location: Other)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: OK (Sensor Location: Other - &46 degrees Celsius)'
       SEVERITY=S
       ATTRIB=default
       COLOR=GREEN

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 1 * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: DEGRADED (Sensor Location: Other)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: DEGRADED (Sensor Location: Other - &46 degrees Celsius)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 1 * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: FAILED (Sensor Location: Other)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: FAILED (Sensor Location: Other - &46 degrees Celsius)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 2 * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: OTHER (Sensor Location: Fan Bay)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: OTHER (Sensor Location: Fan Bay - &46 degrees Celsius)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 2 * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: OK (Sensor Location: Fan Bay)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: OK (Sensor Location: Fan Bay - &46 degrees Celsius)'
       SEVERITY=S
       ATTRIB=default
       COLOR=GREEN

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 2 * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: DEGRADED (Sensor Location: Fan Bay)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: DEGRADED (Sensor Location: Fan Bay - &46 degrees Celsius)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 2 * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: FAILED (Sensor Location: Fan Bay)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: FAILED (Sensor Location: Fan Bay - &46 degrees Celsius)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red





DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 3 * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: OTHER (Sensor Location: Backplane)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: OTHER (Sensor Location: Backplane - &46 degrees Celsius)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 3 * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: OK (Sensor Location: Backplane)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: OK (Sensor Location: Backplane - &46 degrees Celsius)'
       SEVERITY=S
       ATTRIB=default
       COLOR=GREEN

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 3 * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: DEGRADED (Sensor Location: Backplane)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: DEGRADED (Sensor Location: Backplane - &46 degrees Celsius)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8019 * * * * * * * * * * * * * * * * * * * * * * * * * * 3 * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Sensor Status: FAILED (Sensor Location: Backplane)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Sensor Status: FAILED (Sensor Location: Backplane - &46 degrees Celsius)'
       SEVERITY=E
       ATTRIB=default
       COLOR=RED
