DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9742 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Firmware detected a possible Cabinet Power Tiemout'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Firmware detected a possible Cabinet Power Tiemout: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='System Firmware detected a possible timeout waiting for the other cabinet to power on. System firmware queried the utilities system to see what cells are installed. This indicated that cells are installed in the other cabinet but none are'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='powered on. Firmware delayed fabric routing, waiting for the other cabinet cells to power on, but eventually timed out and went on.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9744 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error encountered while collecting PCI error logs'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error encountered while collecting PCI error logs: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9745 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error encountered while collecting SBA error logs'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error encountered while collecting SBA error logs: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error code'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9746 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fabric is unable to route the crossbar after multiple retry attempts'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fabric is unable to route the crossbar after multiple retry attempts: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='During fabric initialization, if a crossbar is found to be in an unexpected state, the number of retries is incremented. If the number of retries exceeds the maximum, then something is wrong and there is no way to initialize the fabric. Data'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='field: number of retries (0:31) crossbar number (32:63)  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9750 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Windows: Predictive Failure in Memory (Warning)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Windows: Predictive Failure in Memory (Warning): &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='ECC (Error Checking and Correcting) memory is designed to detect and correct single-bit errors that occasionally occur in computer systems. This memory module is currently correcting many single bit errors.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9751 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Windows: Predictive Failure in Memory (Critical)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Windows: Predictive Failure in Memory (Critical): &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='ECC (Error Checking and Correcting) memory is designed to detect and correct single-bit errors that occasionally occur in computer systems. This memory module is currently correcting many single bit errors.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9753 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event A rope parity error occurred'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event A rope parity error occurred: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A error occurred on the bus connecting the PCI card to the system bus.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9754 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI card inaccessible due to bus error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI card inaccessible due to bus error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A PCI card has been marked as  fatal  by the operating system due to a bus error. The LBA has been isolated by the operating system due to an error which occured in a device(s) connected to that LBA.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9755 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event PCI card inaccessible due to device error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event PCI card inaccessible due to device error: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A PCI card has been marked as  fatal  by the operating system due to a device error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9768 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event error reading bmc first boot token'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event error reading bmc first boot token: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware tried to read the first boot token an got a failure. The data field contains the token number that FW tried to read. This is a stop boot condition'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9769 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event a rendezvousing cell is non PA architecture and thus incompatible.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event a rendezvousing cell is non PA architecture and thus incompatible.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='monarch PA cell has detected that a cell it is attempting to rendezvous into its PD is not a PA cell and is thus incompatible.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9774 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event failed to write the XBC error log clear register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event failed to write the XBC error log clear register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A XBC error could not be cleared due to a write failure. The data field indicates the type of error: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9775 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error encounted while reading the XBC CSR Error Status Register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error encounted while reading the XBC CSR Error Status Register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to read the XBC Global CSR Error Status register. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9776 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XBC CSR Low Severity error was not cleared'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XBC CSR Low Severity error was not cleared: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The XBC CSR Low Severity error was not cleared or more errors remain. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | contents of the XBC CSR Error Status Register'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9777 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XBC CSR High Severity error was not cleared'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XBC CSR High Severity error was not cleared: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The XBC CSR High Severity error was not cleared or more errors remain. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | contents of the XBC CSR Error Status Register'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9778 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error encounted while reading the XBC Port Error Status Register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error encounted while reading the XBC Port Error Status Register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to read the XBC Port Error Status register. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9780 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC CSR Error Status register'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC CSR Error Status register: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to read the XBC Global CSR Error Status register. Data Field: (XBC Port Num << 56) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9781 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to copy the XBC CSR Error Symbol01 Block'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to copy the XBC CSR Error Symbol01 Block: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware failed to copy the XBC CSR Error symbol 01 registers into a data structure on the stack. Data Field: address where the register contents are being copied'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9782 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to copy the XBC CSR Error Symbol23 Block'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to copy the XBC CSR Error Symbol23 Block: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware failed to copy the XBC CSR Error symbol 23 registers into a data structure on the stack. Data Field: address where the register contents are being copied'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9783 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to reset the XBC Low Severity Error Log State'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to reset the XBC Low Severity Error Log State: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware was unable to reset the XBC CSR Low Severity error log state. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9784 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to clear the XBC Low Severity Log Symbol 01'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to clear the XBC Low Severity Log Symbol 01: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The XBC Low Severity error logs were not cleared. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | number of failed clear attempts'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9785 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not determine if there is a new XBC CSR Low Severity error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not determine if there is a new XBC CSR Low Severity error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Reading the XBC CSR Error Status register failed. Data field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9786 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC CSR Low Severity Error Log State'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC CSR Low Severity Error Log State: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to read a XBC Global scratch register that indicates if new, unlogged errors have been encountered. Data field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9787 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to reset the XBC Low Severity Error Log State'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to reset the XBC Low Severity Error Log State: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Firmware was unable to reset the XBC CSR Low Severity error log state. Data Field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9788 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Could not determine if there is a new XBC CSR High Severity error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Could not determine if there is a new XBC CSR High Severity error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Reading the XBC CSR Error Status register failed. Data field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9789 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC CSR High Severity Error Log State'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC CSR High Severity Error Log State: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to read a XBC Global scratch register that indicates if new, unlogged errors have been encountered. Data field: (XBC Port Num << 56) | (XBC Num << 32) | error status'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9801 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error occurred while enabling hashing in the platform cache'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error occurred while enabling hashing in the platform cache: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while enabling hashing in the platform cache. The data field contains the status.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9827 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The XBC CSR is not a valid CSR address'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The XBC CSR is not a valid CSR address: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A write to an invalid XBC CSR address was attempted. The write will not be allowed. The severity of this result will be determined by the calling function. Data Field: XBC CSR address that was attempted'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9832 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event It indicates loss of cell connectivity in the partition.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event It indicates loss of cell connectivity in the partition.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='It indicates loss of cell connectivity in the partition during a global MCA processing.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9849 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error building cell-level FW device tree'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error building cell-level FW device tree: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error status of building the cell-level firmware device tree'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9867 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured during FSB interface initialization'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured during FSB interface initialization: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error has occurred during CPU FSB interface initialization. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9868 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to error obtaining parameters from PAL'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to error obtaining parameters from PAL: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error has occurred while obtaining CPU parameters from the CPU abstraction layer. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9869 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to failure retrieving icache parameters from PAL'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to failure retrieving icache parameters from PAL: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while getting CPU icache parameters from the CPU abstraction layer. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured if this error occurs during system'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='boot.  '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9870 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured during initialization process'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured during initialization process: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while obtaining CPU dcache parameters from the CPU abstraction layer. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured if error occurs during system boot.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9871 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured during dcache init'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured during dcache init: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while initializing the CPU cache to a known state. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9872 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to internal error'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to internal error: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while enabling CPU cache error monitoring. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9873 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to machine check'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to machine check: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while enabling some machine error check traps on a CPU. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9874 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to error while disabling machine check'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to error while disabling machine check: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while disabling maching error check traps on a CPU. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 9875 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event CPU deconfigured due to failure in late self tests'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event CPU deconfigured due to failure in late self tests: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred during the serialized CPU late selftests. The datafield contains a 32-bit error number and 32-bits of additional error information. The CPU will be deconfigured.'

