--MibName=cpqRackInfo
-- ****************************************************************************
--
--                         Rack Information MIB
--         Management Information Base for SNMP Network Management
--
--
--      Copyright 2002,2003 Hewlett-Packard Development Company, L.P.
--
--      Hewlett-Packard Company shall not be liable for technical or
--      editorial errors or omissions contained herein. The information in
--      this document is provided "as is" without warranty of any kind and
--      is subject to change without notice. The warranties for HP products
--      are set forth in the express limited warranty statements
--      accompanying such products. Nothing herein should be construed as
--      constituting an additional warranty.
--
--      Confidential computer software. Valid license from HP required for
--      possession, use or copying. Consistent with FAR 12.211 and 12.212,
--      Commercial Computer Software, Computer Software Documentation, and
--      Technical Data for Commercial Items are licensed to the U.S.
--      Government under vendor's standard commercial license.
--
--      Refer to the READMIB.RDM file for more information about the
--      organization of the information in the Compaq Enterprise.
--
--      The Compaq Enterprise number is 232.
--      The ASN.1 prefix to, and including the Compaq Enterprise is:
--           1.3.6.1.4.1.232
--
-- ****************************************************************************

CPQRACK-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        compaq                         FROM CPQHOST-MIB
        DisplayString                  FROM RFC1213-MIB
        OBJECT-TYPE                    FROM RFC-1212
        sysName                        FROM RFC1213-MIB
        cpqHoTrapFlags                 FROM CPQHOST-MIB
        TRAP-TYPE                      FROM RFC-1215;

  compaq                             OBJECT IDENTIFIER ::= { enterprises 232 }
    cpqRackInfo                        OBJECT IDENTIFIER ::= { compaq 22 }
    cpqRackMibRev                      OBJECT IDENTIFIER ::= { cpqRackInfo 1 }
    cpqRackComponent                   OBJECT IDENTIFIER ::= { cpqRackInfo 2 }
    cpqRackSysObjID                    OBJECT IDENTIFIER ::= { cpqRackInfo 3 }

    cpqRackInterface                   OBJECT IDENTIFIER ::= { cpqRackComponent 1 }
    cpqRackAsset                       OBJECT IDENTIFIER ::= { cpqRackComponent 2 }
    cpqRackEnclosure                   OBJECT IDENTIFIER ::= { cpqRackComponent 3 }
    cpqRackServer                      OBJECT IDENTIFIER ::= { cpqRackComponent 4 }
    cpqRackPower                       OBJECT IDENTIFIER ::= { cpqRackComponent 5 }
    cpqRackNetwork                     OBJECT IDENTIFIER ::= { cpqRackComponent 6 }

    cpqRackOsCommon                    OBJECT IDENTIFIER ::= { cpqRackInterface 4 }

    cpqRackCommonEnclosure             OBJECT IDENTIFIER ::= { cpqRackEnclosure 1 }
    cpqRackServerEnclosure             OBJECT IDENTIFIER ::= { cpqRackEnclosure 2 }
    cpqRackPowerEnclosure              OBJECT IDENTIFIER ::= { cpqRackEnclosure 3 }

    cpqRackServerBlade                 OBJECT IDENTIFIER ::= { cpqRackServer 1 }

    cpqRackPowerSupply                 OBJECT IDENTIFIER ::= { cpqRackPower 1 }

    cpqRackNetConnector                OBJECT IDENTIFIER ::= { cpqRackNetwork 1 }

-- ****************************************************************************
--   Rack Information MIB Revision
--   =============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqRackInfo Group              (1.3.6.1.4.1.232.22)
--       cpqRackMibRev Group           (1.3.6.1.4.1.232.22.1)
--
--    Implementation of the MibRev group is mandatory for all Agents
--    supporting the Rack Information MIB.
--
--     An Agent conforming to this document will return a
--     cpqRackMibRevMajor of one (1) and a cpqRackMibRevMinor of three (3).
--
--
-- ****************************************************************************

    cpqRackMibRevMajor OBJECT-TYPE
        SYNTAX  INTEGER (1..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The major revision level of the MIB.

            A change in the major revision level represents a major change
            in the architecture of the MIB.  A change in the major revision
            level may indicate a significant change in the information
            supported and/or the meaning of the supported information,
            correct interpretation of data may require a MIB document with
            the same major revision level."
        ::= { cpqRackMibRev 1 }

    cpqRackMibRevMinor OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The minor revision level of the MIB.

            A change in the minor revision level may represent some minor
            additional support, no changes to any pre-existing information
            has occurred."
        ::= { cpqRackMibRev 2 }

    cpqRackMibCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),              -- default
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The overall condition.

            This object represents the overall status of the
            rack information represented by this MIB."
        ::= { cpqRackMibRev 3 }

-- ****************************************************************************
--   Rack Information Common
--   =======================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqRackInfo Group              (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group        (1.3.6.1.4.1.232.22.2)
--        cpqRackInterface Group       (1.3.6.1.4.1.232.22.2.1)
--         cpqRackOsCommon Group       (1.3.6.1.4.1.232.22.2.1.4)
--
--
--  Implementation of the cpqRackOsCommon group is mandatory for all
--  Agents that support the Rack Information MIB.
--
-- ****************************************************************************

    cpqRackOsCommonPollFreq OBJECT-TYPE
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The Management Agent's polling frequency.

            The frequency, in seconds, at which the Agent requests
            information from the device driver.  A frequency of zero (0)
            indicates that the Insight Agent retrieves the information upon
            request of a management station, it does not poll the device
            driver at a specific interval.

            If the poll frequency is zero (0) all attempts to write to this
            object will fail.  If the poll frequency is non-zero,
            setting this value will change the polling frequency of the
            Insight Agent.  Setting the poll frequency to zero (0) will
            always fail, an agent may also choose to fail any request to
            change the poll frequency to a value that would severely impact
            system performance."
        ::= { cpqRackOsCommon 1 }


-- ****************************************************************************
--   Rack Asset Group
--   ================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqRackInfo Group              (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group        (1.3.6.1.4.1.232.22.2)
--        cpqRackAsset Group           (1.3.6.1.4.1.232.22.2.2)
--
--  The cpqRackAsset group contains the serial numbers, names, etc. of any
--  Rack hardware that supports asset management.
--
--  Implementation of the cpqRackAsset group is mandatory for all
--  Agents that support the Rack Information MIB.
--
-- ****************************************************************************

-- ****************************************************************************
--   Rack Asset Table
--   ================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqRackInfo Group              (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group        (1.3.6.1.4.1.232.22.2)
--        cpqRackAsset Group           (1.3.6.1.4.1.232.22.2.2)
--         cpqRackAssetTable           (1.3.6.1.4.1.232.22.2.2.1)
--
-- ****************************************************************************

    cpqRackAssetTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqRackAssetEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of rack asset information."
        ::= { cpqRackAsset 1 }

    cpqRackAssetEntry OBJECT-TYPE
        SYNTAX  CpqRackAssetEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A rack asset description."
        INDEX   { cpqRackAssetIndex }
        ::= { cpqRackAssetTable 1 }

    CpqRackAssetEntry ::= SEQUENCE {
        cpqRackAssetIndex           INTEGER,
        cpqRackName                 DisplayString,
        cpqRackUid                  DisplayString,
        cpqRackSerialNum            DisplayString,
        cpqRackTrapSequenceNum      INTEGER,
        cpqRackHeight               INTEGER,
        cpqRackWidth                INTEGER,
        cpqRackDepth                INTEGER
    }

    cpqRackAssetIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this rack table entry."
        ::= { cpqRackAssetEntry 1 }

    cpqRackName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The customer changeable identifier used to identify the entire
            rack.

            The string will be empty if the system does not report this
            function."
        ::= { cpqRackAssetEntry 2 }

    cpqRackUid OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The rack unique identifier.

            The string will be empty if the rack does not report the
            UID or if it could not be determined."
        ::= { cpqRackAssetEntry 3 }

    cpqRackSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The rack serial number.

            The string will be empty if the rack does not report the
            serial number."
        ::= { cpqRackAssetEntry 4 }

    cpqRackTrapSequenceNum OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The trap sequence number for rack traps.

            This is used by the management application trap processing.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackAssetEntry 5 }

    cpqRackHeight OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The internal height dimension of the useable rack space expressed
            in millimeters.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackAssetEntry 6 }

    cpqRackWidth OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The internal width dimension of the useable rack space expressed
            in millimeters.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackAssetEntry 7 }

    cpqRackDepth OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The internal depth dimension of the useable rack space expressed
            in millimeters.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackAssetEntry 8 }


-- ****************************************************************************
--   Rack Enclosure Chassis Group
--   ============================
--
-- The compaq enterprise               (1.3.6.1.4.1.232)
--      cpqRackInfo Group              (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group        (1.3.6.1.4.1.232.22.2)
--        cpqRackEnclosure Group       (1.3.6.1.4.1.232.22.2.3)
--
--  The cpqRackEnclosure group contains the information about rack
--  enclosures.
--
-- ****************************************************************************

-- ****************************************************************************
--   Rack Common Enclosure Table
--   ===========================
--
-- The compaq enterprise                 (1.3.6.1.4.1.232)
--      cpqRackInfo Group                (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group          (1.3.6.1.4.1.232.22.2)
--        cpqRackEnclosure Group         (1.3.6.1.4.1.232.22.2.3)
--         cpqRackCommonEnclosure Group  (1.3.6.1.4.1.232.22.2.3.1)
--          cpqRackCommonEnclosureTable  (1.3.6.1.4.1.232.22.2.3.1.1)
--
-- ****************************************************************************

    cpqRackCommonEnclosureTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqRackCommonEnclosureEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of rack enclosure information."
        ::= { cpqRackCommonEnclosure 1 }

    cpqRackCommonEnclosureEntry OBJECT-TYPE
        SYNTAX  CpqRackCommonEnclosureEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A rack enclosure description."
        INDEX   { cpqRackCommonEnclosureRack,
                  cpqRackCommonEnclosureIndex }
        ::= { cpqRackCommonEnclosureTable 1 }

    CpqRackCommonEnclosureEntry ::= SEQUENCE {
        cpqRackCommonEnclosureRack                 INTEGER,
        cpqRackCommonEnclosureIndex                INTEGER,
        cpqRackCommonEnclosureModel                DisplayString,
        cpqRackCommonEnclosureAssetTag             DisplayString,
        cpqRackCommonEnclosurePartNumber           DisplayString,
        cpqRackCommonEnclosureSparePartNumber      DisplayString,
        cpqRackCommonEnclosureSerialNum            DisplayString,
        cpqRackCommonEnclosureFWRev                DisplayString,
        cpqRackCommonEnclosureName                 DisplayString,
        cpqRackCommonEnclosureNeighborNamePrev     DisplayString,
        cpqRackCommonEnclosureNeighborNameNext     DisplayString,
        cpqRackCommonEnclosureHeight               INTEGER,
        cpqRackCommonEnclosureWidth                INTEGER,
        cpqRackCommonEnclosureDepth                INTEGER,
        cpqRackCommonEnclosureTrapSequenceNum      INTEGER,
        cpqRackCommonEnclosureCondition            INTEGER,
        cpqRackCommonEnclosureHasServerBlades      INTEGER,
        cpqRackCommonEnclosureHasPowerSupplies     INTEGER,
        cpqRackCommonEnclosureHasNetConnectors     INTEGER,
        cpqRackCommonEnclosureHasTempSensors       INTEGER,
        cpqRackCommonEnclosureHasFans              INTEGER,
        cpqRackCommonEnclosureHasFuses             INTEGER,
        cpqRackCommonEnclosureMgmtUID              INTEGER,
        cpqRackCommonEnclosureSerialNumPrev        DisplayString,
        cpqRackCommonEnclosureSerialNumNext        DisplayString,
        cpqRackCommonEnclosureAddress              INTEGER,
        cpqRackCommonEnclosureProductId            DisplayString,
        cpqRackCommonEnclosureProductIdPrev        DisplayString,
        cpqRackCommonEnclosureProductIdNext        DisplayString,
        cpqRackCommonEnclosureUUID                 DisplayString,
        cpqRackCommonEnclosureUUIDPrev             DisplayString,
        cpqRackCommonEnclosureUUIDNext             DisplayString
    }

    cpqRackCommonEnclosureRack OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this rack."
        ::= { cpqRackCommonEnclosureEntry 1 }

    cpqRackCommonEnclosureIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this enclosure in the rack."
        ::= { cpqRackCommonEnclosureEntry 2 }

    cpqRackCommonEnclosureModel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The model name of the enclosure.

            The string will be empty if the enclosure does not report the
            model information."
        ::= { cpqRackCommonEnclosureEntry 3 }

    cpqRackCommonEnclosureAssetTag OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The customer changeable asset identifier of the enclosure.

            The string will be empty if the system does not report this
            function or if the asset tag has not been set."
        ::= { cpqRackCommonEnclosureEntry 4 }

    cpqRackCommonEnclosurePartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The part number of the enclosure.

            The string will be empty if the enclosure does not report this
            function."
        ::= { cpqRackCommonEnclosureEntry 5 }

    cpqRackCommonEnclosureSparePartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The spare part number of the enclosure.

            The string will be empty if the enclosure does not report this
            function."
        ::= { cpqRackCommonEnclosureEntry 6 }

    cpqRackCommonEnclosureSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the enclosure.

            The string will be empty if the enclosure does not report the
            serial number."
        ::= { cpqRackCommonEnclosureEntry 7 }

    cpqRackCommonEnclosureFWRev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The firmware revision of the enclosure.

            The string will be empty if the enclosure does not report the
            firmware revision or does not contain firmware."
        ::= { cpqRackCommonEnclosureEntry 8 }

    cpqRackCommonEnclosureName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the enclosure.

            The string will be empty if the enclosure does not report the
            name or it could not be determined."
        ::= { cpqRackCommonEnclosureEntry 9 }

    cpqRackCommonEnclosureNeighborNamePrev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the enclosure immediately preceding or above this
            enclosure.

            The string will be empty if the neighbor enclosure name could not be
            determined or there is no enclosure preceding this one."
        ::= { cpqRackCommonEnclosureEntry 10 }

    cpqRackCommonEnclosureNeighborNameNext OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the enclosure immediately following or below this
            enclosure.

            The string will be empty if the neighbor enclosure name could not be
            determined or there is no enclosure following this one."
        ::= { cpqRackCommonEnclosureEntry 11 }

    cpqRackCommonEnclosureHeight OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The height dimension of the rack space taken by the
            enclosure expressed in millimeters.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackCommonEnclosureEntry 12 }

    cpqRackCommonEnclosureWidth OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The width dimension of the rack space taken by the
            enclosure expressed in millimeters.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackCommonEnclosureEntry 13 }

    cpqRackCommonEnclosureDepth OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The depth dimension of the rack space taken by the
            enclosure expressed in millimeters.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackCommonEnclosureEntry 14 }

    cpqRackCommonEnclosureTrapSequenceNum OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The trap sequence number for the enclosure.

            This is used by the management application trap processing.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackCommonEnclosureEntry 15 }

    cpqRackCommonEnclosureCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The overall condition of the enclosure.

            This is the aggregate of the temperature sensors, fans, and
            fuses within the enclosure.

            This value will be one of the following:

            other(1)
              No temperature sensors, fans, or fuses in the enclosure or the
              state could no be determined.

            ok(2)
              All temperature sensors, fans, and fuses are within the normal
              operating range.

            degraded(3)
              One or more temperature sensors, fans, or fuses are outside of
              the normal operating range.  None are failed.

            failed(4)
              The temperature sensor exceeded the critical threshold value,
              a required fan has failed, or a fuse has been tripped.

            The system will automatically shutdown if the failed(4) condition
            results, so it is unlikely that this value will ever be returned
            by the agent."
        ::= { cpqRackCommonEnclosureEntry 16 }

    cpqRackCommonEnclosureHasServerBlades OBJECT-TYPE
        SYNTAX  INTEGER {
            false(1),
            true(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The enclosure can contain server blades.

            This will be true(2) is the enclosure can house server blades.  The
            cpqRackServerEnclosureTable will contain server enclosure specific
            information.

            Match the cpqRackCommonEnclosureSerialNum in this table to the
            serial number in the cpqRackServerEnclosureTable to get complete
            information on the server enclosure."
        ::= { cpqRackCommonEnclosureEntry 17 }

    cpqRackCommonEnclosureHasPowerSupplies OBJECT-TYPE
        SYNTAX  INTEGER {
            false(1),
            true(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The enclosure can contain power supplies.

            This will be true(2) is the enclosure can house power supplies.  The
            cpqRackEnclosurePowerTable will contain power enclosure specific
            information.

            Match the cpqRackCommonEnclosureSerialNum in this table to the
            serial number in the cpqRackEnclosurePowerTable to get complete
            information on the power enclosure."
        ::= { cpqRackCommonEnclosureEntry 18 }

    cpqRackCommonEnclosureHasNetConnectors OBJECT-TYPE
        SYNTAX  INTEGER {
            false(1),
            true(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The enclosure contains network connectivity.

            This will be true(2) is the enclosure contains network connectivity.
            The cpqRackCommonEnclosureNetConnectorTable will contain network
            connectivity specific information.

            Match the cpqRackCommonEnclosureSerialNum in this table to the
            serial number in the cpqRackCommonEnclosureNetConnectorTable to get complete
            information on the network connector enclosure."
        ::= { cpqRackCommonEnclosureEntry 19 }

    cpqRackCommonEnclosureHasTempSensors OBJECT-TYPE
        SYNTAX  INTEGER {
            false(1),
            true(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The enclosure contains temperature sensors.

            This will be true(2) is the enclosure contains
            temperature sensors. The cpqRackCommonEnclosureTempTable will
            contain temperature sensor specific information.

            Match the cpqRackCommonEnclosureSerialNum in this table to the
            serial number in the cpqRackCommonEnclosureTempTable to get complete
            information on the enclosure."
        ::= { cpqRackCommonEnclosureEntry 20 }

    cpqRackCommonEnclosureHasFans OBJECT-TYPE
        SYNTAX  INTEGER {
            false(1),
            true(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The enclosure contains fans.

            This will be true(2) is the enclosure contains fans.
            The cpqRackCommonEnclosureFanTable will contain the fan
            specific information.

            Match the cpqRackCommonEnclosureSerialNum in this table to the
            serial number in the cpqRackCommonEnclosureFanTable to get complete
            information on the enclosure."
        ::= { cpqRackCommonEnclosureEntry 21 }

    cpqRackCommonEnclosureHasFuses OBJECT-TYPE
        SYNTAX  INTEGER {
            false(1),
            true(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The enclosure contains fuses.

            This will be true(2) is the enclosure contains fuses.
            The cpqRackCommonEnclosureFuseTable will contain the fuse
            specific information.

            Match the cpqRackCommonEnclosureSerialNum in this table to the
            serial number in the cpqRackCommonEnclosureFuseTable to get complete
            information on the enclosure."
        ::= { cpqRackCommonEnclosureEntry 22 }

    cpqRackCommonEnclosureMgmtUID OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),            -- Unknown device or could not be determined
            none(2),             -- No Unit Identifier LED present
            ledOn(3),            -- Unit Identifier LED is On
            ledOff(4)            -- Unit Identifier LED is Off
            }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            "The Unit Identifier LED.

            This value will be one of the following:

            other(1)
              The state of the LED could not be determined.  Setting the
              LED state is not allowed.

            none(2)
              The LED is not present.  Setting LED state is not allowed.

            ledOn(3)
              The LED is present and ON.  The LED can be turned off
              by setting the cpqRackCommonEnclosureMgmtUID to ledOff(4).

            ledOff(4)
              The LED is present and OFF.  The LED can be turned on
              by setting the cpqRackCommonEnclosureMgmtUID to ledOn(3)."
        ::= { cpqRackCommonEnclosureEntry 23 }

    cpqRackCommonEnclosureSerialNumPrev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the enclosure immediately preceding or
            above this enclosure.

            The string will be empty if the neighbor enclosure serial number
            could not be determined or there is no enclosure preceding this one."
        ::= { cpqRackCommonEnclosureEntry 24 }

    cpqRackCommonEnclosureSerialNumNext OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the enclosure immediately following or
            below this enclosure.

            The string will be empty if the neighbor enclosure serial number
            could not be determined or there is no enclosure following this one."
        ::= { cpqRackCommonEnclosureEntry 25 }

    cpqRackCommonEnclosureAddress OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The unique address of the enclosure within the rack.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackCommonEnclosureEntry 26 }

    cpqRackCommonEnclosureProductId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The product id string of the enclosure.

            The string will be empty if the enclosure does not report the
            product id string."
        ::= { cpqRackCommonEnclosureEntry 27 }

    cpqRackCommonEnclosureProductIdPrev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The product id string of the enclosure immediately preceding or
            above this enclosure.

            The string will be empty if the enclosure does not report the
            product id string."
        ::= { cpqRackCommonEnclosureEntry 28 }

    cpqRackCommonEnclosureProductIdNext OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The product id string of the enclosure immediately following or
            below this enclosure.

            The string will be empty if the enclosure does not report the
            product id string."
        ::= { cpqRackCommonEnclosureEntry 29 }

    cpqRackCommonEnclosureUUID OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The universal unique identifier string of the enclosure.

            The string will be empty if the enclosure does not report the
            UUID string."
        ::= { cpqRackCommonEnclosureEntry 30 }

    cpqRackCommonEnclosureUUIDPrev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The universal unique identifier string of the enclosure
            immediately preceding or above this enclosure.

            The string will be empty if the enclosure does not report the
            UUID string or if there is no preceding enclosure."
        ::= { cpqRackCommonEnclosureEntry 31 }

    cpqRackCommonEnclosureUUIDNext OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The universal unique identifier string of the enclosure
            immediately following or below this enclosure.

            The string will be empty if the enclosure does not report the
            UUID string or if there is no following enclosure."
        ::= { cpqRackCommonEnclosureEntry 32 }


-- ****************************************************************************
--   Rack Enclosure Common Temperature Sensor Table
--   ==============================================
--
-- The compaq enterprise                     (1.3.6.1.4.1.232)
--      cpqRackInfo Group                    (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group              (1.3.6.1.4.1.232.22.2)
--        cpqRackEnclosure Group             (1.3.6.1.4.1.232.22.2.3)
--         cpqRackCommonEnclosure Group      (1.3.6.1.4.1.232.22.2.3.1)
--          cpqRackCommonEnclosureTempTable  (1.3.6.1.4.1.232.22.2.3.1.2)
--
-- ****************************************************************************

    cpqRackCommonEnclosureTempTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqRackCommonEnclosureTempEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of rack enclosure temperature sensor information."
        ::= { cpqRackCommonEnclosure 2 }

    cpqRackCommonEnclosureTempEntry OBJECT-TYPE
        SYNTAX  CpqRackCommonEnclosureTempEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A rack enclosure temperature sensor description."
        INDEX   { cpqRackCommonEnclosureTempRack,
                  cpqRackCommonEnclosureTempChassis,
                  cpqRackCommonEnclosureTempSensorIndex }
        ::= { cpqRackCommonEnclosureTempTable 1 }

    CpqRackCommonEnclosureTempEntry ::= SEQUENCE {
        cpqRackCommonEnclosureTempRack                      INTEGER,
        cpqRackCommonEnclosureTempChassis                   INTEGER,
        cpqRackCommonEnclosureTempSensorIndex               INTEGER,
        cpqRackCommonEnclosureTempSensorEnclosureName       DisplayString,
        cpqRackCommonEnclosureTempLocation                  DisplayString,
        cpqRackCommonEnclosureTempCurrent                   INTEGER,
        cpqRackCommonEnclosureTempThreshold                 INTEGER,
        cpqRackCommonEnclosureTempCondition                 INTEGER,
        cpqRackCommonEnclosureTempType                      INTEGER,
        cpqRackCommonEnclosureTempSensorEnclosureSerialNum  DisplayString
    }

    cpqRackCommonEnclosureTempRack OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this rack."
        ::= { cpqRackCommonEnclosureTempEntry 1 }

    cpqRackCommonEnclosureTempChassis OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this enclosure in the rack."
        ::= { cpqRackCommonEnclosureTempEntry 2 }

    cpqRackCommonEnclosureTempSensorIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this temperature sensor within
            this enclosure in the rack."
        ::= { cpqRackCommonEnclosureTempEntry 3 }

    cpqRackCommonEnclosureTempSensorEnclosureName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the enclosure.

            The string will be empty if the enclosure does not report the
            name or it could not be determined."
        ::= { cpqRackCommonEnclosureTempEntry 4 }

    cpqRackCommonEnclosureTempLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The location description of the temperature sensor within the
            enclosure.

            The string will be empty if the location could not be
            determined."
        ::= { cpqRackCommonEnclosureTempEntry 5 }

    cpqRackCommonEnclosureTempCurrent OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is the current temperature sensor reading in degrees
            celsius.

            If this value cannot be determined by software, then a value
            of -1 will be returned."
        ::= { cpqRackCommonEnclosureTempEntry 6 }

    cpqRackCommonEnclosureTempThreshold OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is the threshold temperature sensor setting
            in degrees celsius.  This is the temperature in which the
            sensor will be considered to be in a tripped state this
            causing some action to occur depending on the type of
            the sensor.  The action of temperature sensor threshold
            will be indicated by the cpqRackCommonEnclosureTempType
            item.  If the type is blowout(5), then the temperature sensor
            will cause the fans to speed up.  If the type is caution(9),
            then the temperature sensor is in a degraded state.  If the
            type is critical(15), then the enclosure will be considered
            as in a failed state.

            If this value cannot be determined by software, then a value
            of -1 will be returned."
        ::= { cpqRackCommonEnclosureTempEntry 7 }

    cpqRackCommonEnclosureTempCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The Temperature sensor condition.

            This value will be one of the following:

            other(1)
              Temperature could not be determined.

            ok(2)
              The temperature sensor is within the normal operating range.

            degraded(3)
              The temperature sensor is outside of the normal operating range.

            failed(4)
              The temperature sensor detects a condition that could
              possibly damage the system.

            The system will automatically shutdown if the failed(4) condition
            results, so it is unlikely that this value will ever be returned
            by the agent."
        ::= { cpqRackCommonEnclosureTempEntry 8 }

    cpqRackCommonEnclosureTempType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            blowout(5),
            caution(9),
            critical(15)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This specifies the type of this instance of temperature
            sensor.

            This value will be one of the following:

            other(1)
              Temperature threshold type could not be determined.

            blowout(5)
              If a blowout(5) temperature sensor reaches its threshold,
              the fan or fans in the area of the temperature sensor will
              increase in speed in an attempt to reduce the temperature
              before a caution or critical threshold is reached.

            caution(9)
              If a caution(9) temperature sensor reaches its threshold, the
              cpqRackCommonEnclosureTempCondition will be set to degraded(3)
              and the system will either continue or shutdown depending
              on the user preferences.

            critical(15)
              If a critical(15) temperature sensor reaches its threshold,
              the cpqHeTemperatureCondition will be set to failed(4)
              and the system will shutdown."
        ::= { cpqRackCommonEnclosureTempEntry 9 }

    cpqRackCommonEnclosureTempSensorEnclosureSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the enclosure containing this temperature
            sensor.

            The string will be empty if the enclosure does not report the
            serial number or it could not be determined."
        ::= { cpqRackCommonEnclosureTempEntry 10 }


-- ****************************************************************************
--   Rack Enclosure Common Fan Table
--   ===============================
--
-- The compaq enterprise                     (1.3.6.1.4.1.232)
--      cpqRackInfo Group                    (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group              (1.3.6.1.4.1.232.22.2)
--        cpqRackEnclosure Group             (1.3.6.1.4.1.232.22.2.3)
--         cpqRackCommonEnclosure Group      (1.3.6.1.4.1.232.22.2.3.1)
--          cpqRackCommonEnclosureFanTable   (1.3.6.1.4.1.232.22.2.3.1.3)
--
-- ****************************************************************************

    cpqRackCommonEnclosureFanTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqRackCommonEnclosureFanEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of rack enclosure fan information."
        ::= { cpqRackCommonEnclosure 3 }

    cpqRackCommonEnclosureFanEntry OBJECT-TYPE
        SYNTAX  CpqRackCommonEnclosureFanEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A rack enclosure fan description."
        INDEX   { cpqRackCommonEnclosureFanRack,
                  cpqRackCommonEnclosureFanChassis,
                  cpqRackCommonEnclosureFanIndex }
        ::= { cpqRackCommonEnclosureFanTable 1 }

    CpqRackCommonEnclosureFanEntry ::= SEQUENCE {
        cpqRackCommonEnclosureFanRack                   INTEGER,
        cpqRackCommonEnclosureFanChassis                INTEGER,
        cpqRackCommonEnclosureFanIndex                  INTEGER,
        cpqRackCommonEnclosureFanEnclosureName          DisplayString,
        cpqRackCommonEnclosureFanLocation               DisplayString,
        cpqRackCommonEnclosureFanPartNumber             DisplayString,
        cpqRackCommonEnclosureFanSparePartNumber        DisplayString,
        cpqRackCommonEnclosureFanPresent                INTEGER,
        cpqRackCommonEnclosureFanRedundant              INTEGER,
        cpqRackCommonEnclosureFanRedundantGroupId       INTEGER,
        cpqRackCommonEnclosureFanCondition              INTEGER,
        cpqRackCommonEnclosureFanEnclosureSerialNum     DisplayString
    }

    cpqRackCommonEnclosureFanRack OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this rack."
        ::= { cpqRackCommonEnclosureFanEntry 1 }

    cpqRackCommonEnclosureFanChassis OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this enclosure in the rack."
        ::= { cpqRackCommonEnclosureFanEntry 2 }

    cpqRackCommonEnclosureFanIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this fan within this
            enclosure in the rack."
        ::= { cpqRackCommonEnclosureFanEntry 3 }

    cpqRackCommonEnclosureFanEnclosureName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the enclosure.

            The string will be empty if the enclosure does not report the
            name or it could not be determined."
        ::= { cpqRackCommonEnclosureFanEntry 4 }

    cpqRackCommonEnclosureFanLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The location description of the fan within the enclosure.

            The string will be empty if the location could not be
            determined."
        ::= { cpqRackCommonEnclosureFanEntry 5 }

    cpqRackCommonEnclosureFanPartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The part number of the enclosure fan.

            The string will be empty if the part number could not be
            determined."
        ::= { cpqRackCommonEnclosureFanEntry 6 }

    cpqRackCommonEnclosureFanSparePartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The spare part number of the enclosure fan.

            The string will be empty if the part number could not be
            determined."
        ::= { cpqRackCommonEnclosureFanEntry 7 }

    cpqRackCommonEnclosureFanPresent OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            absent(2),
            present(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This specifies if the fan described is present in the system."
        ::= { cpqRackCommonEnclosureFanEntry 8 }

    cpqRackCommonEnclosureFanRedundant OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            notRedundant(2),
            redundant(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This specifies if the fan is in a redundant configuration."
        ::= { cpqRackCommonEnclosureFanEntry 9 }

    cpqRackCommonEnclosureFanRedundantGroupId OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This specifies the group number for redundant fans within this
            enclosure."
        ::= { cpqRackCommonEnclosureFanEntry 10 }

    cpqRackCommonEnclosureFanCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The condition of the fan.

            This value will be one of the following:

            other(1)
              Fan status detection is not supported.

            ok(2)
              The fan is operating properly.

            degraded(2)
              A redundant fan is not operating properly.

            failed(4)
              A non-redundant fan is not operating properly."
        ::= { cpqRackCommonEnclosureFanEntry 11 }

    cpqRackCommonEnclosureFanEnclosureSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the enclosure containing the fan.

            The string will be empty if the enclosure does not report the
            serial number or it could not be determined."
        ::= { cpqRackCommonEnclosureFanEntry 12 }


-- ****************************************************************************
--   Rack Enclosure Common Fuse Table
--   ================================
--
-- The compaq enterprise                     (1.3.6.1.4.1.232)
--      cpqRackInfo Group                    (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group              (1.3.6.1.4.1.232.22.2)
--        cpqRackEnclosure Group             (1.3.6.1.4.1.232.22.2.3)
--         cpqRackCommonEnclosure Group      (1.3.6.1.4.1.232.22.2.3.1)
--          cpqRackCommonEnclosureFuseTable  (1.3.6.1.4.1.232.22.2.3.1.4)
--
-- ****************************************************************************

    cpqRackCommonEnclosureFuseTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqRackCommonEnclosureFuseEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of rack enclosure fuse information."
        ::= { cpqRackCommonEnclosure 4 }

    cpqRackCommonEnclosureFuseEntry OBJECT-TYPE
        SYNTAX  CpqRackCommonEnclosureFuseEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A rack enclosure fuse description."
        INDEX   { cpqRackCommonEnclosureFuseRack,
                  cpqRackCommonEnclosureFuseChassis,
                  cpqRackCommonEnclosureFuseIndex }
        ::= { cpqRackCommonEnclosureFuseTable 1 }

    CpqRackCommonEnclosureFuseEntry ::= SEQUENCE {
        cpqRackCommonEnclosureFuseRack             INTEGER,
        cpqRackCommonEnclosureFuseChassis          INTEGER,
        cpqRackCommonEnclosureFuseIndex            INTEGER,
        cpqRackCommonEnclosureFuseEnclosureName    DisplayString,
        cpqRackCommonEnclosureFuseLocation         DisplayString,
        cpqRackCommonEnclosureFusePresent          INTEGER,
        cpqRackCommonEnclosureFuseCondition        INTEGER
    }

    cpqRackCommonEnclosureFuseRack OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this rack."
        ::= { cpqRackCommonEnclosureFuseEntry 1 }

    cpqRackCommonEnclosureFuseChassis OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this enclosure in the rack."
        ::= { cpqRackCommonEnclosureFuseEntry 2 }

    cpqRackCommonEnclosureFuseIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies the fuse within this enclosure."
        ::= { cpqRackCommonEnclosureFuseEntry 3 }

    cpqRackCommonEnclosureFuseEnclosureName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the enclosure.

            The string will be empty if the enclosure does not report the
            name or it could not be determined."
        ::= { cpqRackCommonEnclosureFuseEntry 4 }

    cpqRackCommonEnclosureFuseLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The location description of the fuse within the enclosure.

            The string will be empty if the location could not be
            determined."
        ::= { cpqRackCommonEnclosureFuseEntry 5 }

    cpqRackCommonEnclosureFusePresent OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            absent(2),
            present(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This specifies if the fuse described is present in the system."
        ::= { cpqRackCommonEnclosureFuseEntry 6 }

    cpqRackCommonEnclosureFuseCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The condition of the fuse.

            This value will be one of the following:

            other(1)
              Fuse status detection is not supported.

            ok(2)
              The fuse is operating properly.

            failed(4)
              A fuse has been tripped or is not operating properly."
        ::= { cpqRackCommonEnclosureFuseEntry 7 }

-- ****************************************************************************
--   Rack Enclosure Common FRU Table
--   ===============================
--
-- The compaq enterprise                     (1.3.6.1.4.1.232)
--      cpqRackInfo Group                    (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group              (1.3.6.1.4.1.232.22.2)
--        cpqRackEnclosure Group             (1.3.6.1.4.1.232.22.2.3)
--         cpqRackCommonEnclosure Group      (1.3.6.1.4.1.232.22.2.3.1)
--          cpqRackCommonEnclosureFruTable   (1.3.6.1.4.1.232.22.2.3.1.5)
--
-- ****************************************************************************

    cpqRackCommonEnclosureFruTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqRackCommonEnclosureFruEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of rack enclosure field replaceable units information."
        ::= { cpqRackCommonEnclosure 5 }

    cpqRackCommonEnclosureFruEntry OBJECT-TYPE
        SYNTAX  CpqRackCommonEnclosureFruEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A rack enclosure field replaceable unit description."
        INDEX   { cpqRackCommonEnclosureFruRack,
                  cpqRackCommonEnclosureFruChassis,
                  cpqRackCommonEnclosureFruIndex }
        ::= { cpqRackCommonEnclosureFruTable 1 }

    CpqRackCommonEnclosureFruEntry ::= SEQUENCE {
        cpqRackCommonEnclosureFruRack                 INTEGER,
        cpqRackCommonEnclosureFruChassis              INTEGER,
        cpqRackCommonEnclosureFruIndex                INTEGER,
        cpqRackCommonEnclosureFruEnclosureName        DisplayString,
        cpqRackCommonEnclosureFruDescription          DisplayString,
        cpqRackCommonEnclosureFruLocation             DisplayString,
        cpqRackCommonEnclosureFruAssemblyPartNumber   DisplayString,
        cpqRackCommonEnclosureFruSparePartNumber      DisplayString,
        cpqRackCommonEnclosureFruAutoRev              DisplayString,
        cpqRackCommonEnclosureFruSerialNum            DisplayString
    }

    cpqRackCommonEnclosureFruRack OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this rack."
        ::= { cpqRackCommonEnclosureFruEntry 1 }

    cpqRackCommonEnclosureFruChassis OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this enclosure in the rack."
        ::= { cpqRackCommonEnclosureFruEntry 2 }

    cpqRackCommonEnclosureFruIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies the FRU within this enclosure."
        ::= { cpqRackCommonEnclosureFruEntry 3 }

    cpqRackCommonEnclosureFruEnclosureName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the enclosure.

            The string will be empty if the enclosure does not report the
            name or it could not be determined."
        ::= { cpqRackCommonEnclosureFruEntry 4 }

    cpqRackCommonEnclosureFruDescription OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A description of the FRU component.

            The string will be empty if the enclosure does not report the
            description information."
        ::= { cpqRackCommonEnclosureFruEntry 5 }

    cpqRackCommonEnclosureFruLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The location description of the FRU within the enclosure.

            The string will be empty if the location could not be
            determined."
        ::= { cpqRackCommonEnclosureFruEntry 6 }

    cpqRackCommonEnclosureFruAssemblyPartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The assembly part number of the FRU within the enclosure.

            The string will be empty if the enclosure does not report this
            information."
        ::= { cpqRackCommonEnclosureFruEntry 7 }

    cpqRackCommonEnclosureFruSparePartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The spare part number of the FRU within the enclosure.

            The string will be empty if the enclosure does not report this
            information."
        ::= { cpqRackCommonEnclosureFruEntry 8 }

    cpqRackCommonEnclosureFruAutoRev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The auto revision number of the FRU within the enclosure.

            The string will be empty if the enclosure does not report this
            information."
        ::= { cpqRackCommonEnclosureFruEntry 9 }

    cpqRackCommonEnclosureFruSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the FRU within the enclosure.

            The string will be empty if the enclosure does not report the
            serial number."
        ::= { cpqRackCommonEnclosureFruEntry 10 }

-- ****************************************************************************
--   Rack Enclosure for Servers Table
--   ================================
--
-- The compaq enterprise                 (1.3.6.1.4.1.232)
--      cpqRackInfo Group                (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group          (1.3.6.1.4.1.232.22.2)
--        cpqRackEnclosure Group         (1.3.6.1.4.1.232.22.2.3)
--         cpqRackServerEnclosure Group  (1.3.6.1.4.1.232.22.2.3.2)
--          cpqRackServerEnclosureTable  (1.3.6.1.4.1.232.22.2.3.2.1)
--
-- ****************************************************************************

    cpqRackServerEnclosureTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqRackServerEnclosureEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of rack enclosure information for servers."
        ::= { cpqRackServerEnclosure 1 }

    cpqRackServerEnclosureEntry OBJECT-TYPE
        SYNTAX  CpqRackServerEnclosureEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A server enclosure description."
        INDEX   { cpqRackServerEnclosureRack,
                  cpqRackServerEnclosureIndex }
        ::= { cpqRackServerEnclosureTable 1 }

    CpqRackServerEnclosureEntry ::= SEQUENCE {
        cpqRackServerEnclosureRack                 INTEGER,
        cpqRackServerEnclosureIndex                INTEGER,
        cpqRackServerEnclosureName                 DisplayString,
        cpqRackServerEnclosureMaxNumBlades         INTEGER,
        cpqRackServerEnclosureMaxNumBladesX        INTEGER,
        cpqRackServerEnclosureMaxNumBladesY        INTEGER
    }

    cpqRackServerEnclosureRack OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this rack."
        ::= { cpqRackServerEnclosureEntry 1 }

    cpqRackServerEnclosureIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this server enclosure in the rack."
        ::= { cpqRackServerEnclosureEntry 2 }

    cpqRackServerEnclosureName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the server enclosure.

            The string will be empty if the enclosure does not report the
            name or it could not be determined."
        ::= { cpqRackServerEnclosureEntry 3 }

    cpqRackServerEnclosureMaxNumBlades OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The maximum number of server blades the enclosure can contain.

            The string will be empty if the enclosure does not report the
            name or it could not be determined."
        ::= { cpqRackServerEnclosureEntry 4 }

    cpqRackServerEnclosureMaxNumBladesX OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The maximum number of server blades in x-direction (from left to right)
            the enclosure can contain."

        ::= { cpqRackServerEnclosureEntry 5 }

    cpqRackServerEnclosureMaxNumBladesY OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The maximum number of server blades in y-direction (from top to bottom)
            the enclosure can contain."

        ::= { cpqRackServerEnclosureEntry 6 }


-- ****************************************************************************
--   Rack Enclosure for Power Supplies Table
--   =======================================
--
-- The compaq enterprise                 (1.3.6.1.4.1.232)
--      cpqRackInfo Group                (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group          (1.3.6.1.4.1.232.22.2)
--        cpqRackEnclosure Group         (1.3.6.1.4.1.232.22.2.3)
--         cpqRackPowerEnclosure Group   (1.3.6.1.4.1.232.22.2.3.3)
--          cpqRackPowerEnclosureTable   (1.3.6.1.4.1.232.22.2.3.3.1)
--
-- ****************************************************************************

    cpqRackPowerEnclosureTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqRackPowerEnclosureEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of rack power enclosure information."
        ::= { cpqRackPowerEnclosure 1 }

    cpqRackPowerEnclosureEntry OBJECT-TYPE
        SYNTAX  CpqRackPowerEnclosureEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A rack power enclosure description."
        INDEX   { cpqRackPowerEnclosureRack,
                  cpqRackPowerEnclosureIndex }
        ::= { cpqRackPowerEnclosureTable 1 }

    CpqRackPowerEnclosureEntry ::= SEQUENCE {
        cpqRackPowerEnclosureRack                  INTEGER,
        cpqRackPowerEnclosureIndex                 INTEGER,
        cpqRackPowerEnclosureName                  DisplayString,
        cpqRackPowerEnclosureMgmtBoardSerialNum    DisplayString,
        cpqRackPowerEnclosureRedundant             INTEGER,
        cpqRackPowerEnclosureLoadBalanced          INTEGER,
        cpqRackPowerEnclosureInputPwrType          INTEGER,
        cpqRackPowerEnclosurePwrFeedMax            INTEGER,
        cpqRackPowerEnclosureCondition             INTEGER
    }

    cpqRackPowerEnclosureRack OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this rack."
        ::= { cpqRackPowerEnclosureEntry 1 }

    cpqRackPowerEnclosureIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this power enclosure in the rack."
        ::= { cpqRackPowerEnclosureEntry 2 }

    cpqRackPowerEnclosureName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the power enclosure.

            The string will be empty if the enclosure does not report the
            name or it could not be determined."
        ::= { cpqRackPowerEnclosureEntry 3 }

    cpqRackPowerEnclosureMgmtBoardSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the enclosure.

            The string will be empty if the enclosure does not report the
            serial number."
        ::= { cpqRackPowerEnclosureEntry 4 }

    cpqRackPowerEnclosureRedundant OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            notRedundant(2),
            redundant(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This indicates if the power supply enclosure is in a redundant
            state."
        ::= { cpqRackPowerEnclosureEntry 5 }

    cpqRackPowerEnclosureLoadBalanced OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            notLoadBalanced(2),
            loadBalanced(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This indicates if the power supply enclosure is in a load
            balanced state."
        ::= { cpqRackPowerEnclosureEntry 6 }

    cpqRackPowerEnclosureInputPwrType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            singlePhase(2),
            threePhase(3),
            directCurrent(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This indicates type of input facility power."
        ::= { cpqRackPowerEnclosureEntry 7 }

    cpqRackPowerEnclosurePwrFeedMax OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This is the maximum facility power in watts.

            The maximum facility power being fed to this power enclosure.

            The value will be -1 if the power enclosure does not report the
            value or if the value is not known."
        ::= { cpqRackPowerEnclosureEntry 8 }

    cpqRackPowerEnclosureCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This indicates current condition of the power enclosure.

            other(1)
              The power enclosure condition could not be determined.

            ok(2)
              The power enclosure is operating normally.

            degraded(3)
              The power enclosure is in a degraded state.  The power subsystem
              may not be load balanced or may have lost redundancy."
        ::= { cpqRackPowerEnclosureEntry 9 }


-- ****************************************************************************
--   Rack Server Blade Table
--   =======================
--
-- The compaq enterprise                 (1.3.6.1.4.1.232)
--      cpqRackInfo Group                (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group          (1.3.6.1.4.1.232.22.2)
--        cpqRackServer Group            (1.3.6.1.4.1.232.22.2.4)
--         cpqRackServerBlade Group      (1.3.6.1.4.1.232.22.2.4.1)
--          cpqRackServerBladeTable      (1.3.6.1.4.1.232.22.2.4.1.1)
--
-- ****************************************************************************

    cpqRackServerBladeTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqRackServerBladeEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of rack server blade information."
        ::= { cpqRackServerBlade 1 }

    cpqRackServerBladeEntry OBJECT-TYPE
        SYNTAX  CpqRackServerBladeEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A rack server blade description."
        INDEX   { cpqRackServerBladeRack,
                  cpqRackServerBladeChassis,
                  cpqRackServerBladeIndex }
        ::= { cpqRackServerBladeTable 1 }

    CpqRackServerBladeEntry ::= SEQUENCE {
        cpqRackServerBladeRack               INTEGER,
        cpqRackServerBladeChassis            INTEGER,
        cpqRackServerBladeIndex              INTEGER,
        cpqRackServerBladeName               DisplayString,
        cpqRackServerBladeEnclosureName      DisplayString,
        cpqRackServerBladePartNumber         DisplayString,
        cpqRackServerBladeSparePartNumber    DisplayString,
        cpqRackServerBladePosition           INTEGER,
        cpqRackServerBladeHeight             INTEGER,
        cpqRackServerBladeWidth              INTEGER,
        cpqRackServerBladeDepth              INTEGER,
        cpqRackServerBladePresent            INTEGER,
        cpqRackServerBladeHasFuses           INTEGER,
        cpqRackServerBladeEnclosureSerialNum DisplayString,
        cpqRackServerBladeSlotsUsed          INTEGER,
        cpqRackServerBladeSerialNum          DisplayString,
        cpqRackServerBladeProductId          DisplayString,
        cpqRackServerBladeUid                DisplayString,
        cpqRackServerBladeSlotsUsedX         INTEGER,
        cpqRackServerBladeSlotsUsedY         INTEGER
    }

    cpqRackServerBladeRack OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this rack."
        ::= { cpqRackServerBladeEntry 1 }

    cpqRackServerBladeChassis OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this enclosure in the rack."
        ::= { cpqRackServerBladeEntry 2 }

    cpqRackServerBladeIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this server blade within the enclosure."
        ::= { cpqRackServerBladeEntry 3 }

    cpqRackServerBladeName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the server blade.

            The string will be empty if it could not be determined."
        ::= { cpqRackServerBladeEntry 4 }

    cpqRackServerBladeEnclosureName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the enclosure which contains the blade.

            The string will be empty if the enclosure does not report the
            name or it could not be determined."
        ::= { cpqRackServerBladeEntry 5 }

    cpqRackServerBladePartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The part number of the server blade.

            The string will be empty if the part number could not be
            determined."
        ::= { cpqRackServerBladeEntry 6 }

    cpqRackServerBladeSparePartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The spare part number of the server blade.

            The string will be empty if the part number could not be
            determined."
        ::= { cpqRackServerBladeEntry 7 }

    cpqRackServerBladePosition OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The position or slot number of the server blade within the
            server enclosure.

            This will be -1 if the server enclosure does not report the
            information or it could not be determined."
        ::= { cpqRackServerBladeEntry 8 }

    cpqRackServerBladeHeight OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The height dimension of the rack space taken by the server
            blade expressed in millimeters.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackServerBladeEntry 9 }

    cpqRackServerBladeWidth OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The width dimension of the rack space taken by the server
            blade expressed in millimeters.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackServerBladeEntry 10 }

    cpqRackServerBladeDepth OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The depth dimension of the rack space taken by the server
            blade expressed in millimeters.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackServerBladeEntry 11 }

    cpqRackServerBladePresent OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            absent(2),
            present(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This specifies if the server blade described is present in the
            enclosure."
        ::= { cpqRackServerBladeEntry 12 }

    cpqRackServerBladeHasFuses OBJECT-TYPE
        SYNTAX  INTEGER {
            false(1),
            true(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The server blade contains fuses.

            This will be true(2) is the server blade contains fuses.
            The cpqRackCommonEnclosureFuseTable will contain the fuse
            specific information.

            Match the cpqRackServerBladeEnclosureSerialNum in this table to the
            serial number in the cpqRackCommonEnclosureFanTable to get complete
            information on the fuses."
        ::= { cpqRackServerBladeEntry 13 }

    cpqRackServerBladeEnclosureSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the enclosure which contains the blade.

            The string will be empty if the enclosure does not report the
            serial number or it could not be determined."
        ::= { cpqRackServerBladeEntry 14 }

    cpqRackServerBladeSlotsUsed OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The number of slot positions occupied by this server blade.  This
            is used to indicate a server blade which may obscure an adjacent
            blade slot.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackServerBladeEntry 15 }

    cpqRackServerBladeSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the server blade.

            The string will be empty if the system does not report the
            serial number function."
        ::= { cpqRackServerBladeEntry 16 }

    cpqRackServerBladeProductId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The product id string of the server blade.

            The string will be empty if the system does not report the
            product id function."
        ::= { cpqRackServerBladeEntry 17 }

    cpqRackServerBladeUid OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The server blade unique identifier.

            The string will be empty if the blade does not report the
            UID or if it could not be determined."
        ::= { cpqRackServerBladeEntry 18 }

    cpqRackServerBladeSlotsUsedX OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The number of slot positions in x-direction (from left to right)
            occupied by this server blade.  This is used to indicate a server blade
            which may obscure an adjacent blade slot.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackServerBladeEntry 19 }

    cpqRackServerBladeSlotsUsedY OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The number of slot positions in y-direction (from top to bottom)
            occupied by this server blade.  This is used to indicate a server blade
            which may obscure an adjacent blade slot.

            This will be -1 if the rack does not report the information or
            it could not be determined."
        ::= { cpqRackServerBladeEntry 20 }


-- ****************************************************************************
--   Rack Power Supply Table
--   =======================
--
-- The compaq enterprise                 (1.3.6.1.4.1.232)
--      cpqRackInfo Group                (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group          (1.3.6.1.4.1.232.22.2)
--        cpqRackPower Group             (1.3.6.1.4.1.232.22.2.5)
--         cpqRackPowerSupply Group      (1.3.6.1.4.1.232.22.2.5.1)
--          cpqRackPowerSupplyTable      (1.3.6.1.4.1.232.22.2.5.1.1)
--
-- ****************************************************************************

    cpqRackPowerSupplyTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqRackPowerSupplyEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of rack power supply information."
        ::= { cpqRackPowerSupply 1 }

    cpqRackPowerSupplyEntry OBJECT-TYPE
        SYNTAX  CpqRackPowerSupplyEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A rack power supply description."
        INDEX   { cpqRackPowerSupplyRack,
                  cpqRackPowerSupplyChassis,
                  cpqRackPowerSupplyIndex }
        ::= { cpqRackPowerSupplyTable 1 }

    CpqRackPowerSupplyEntry ::= SEQUENCE {
        cpqRackPowerSupplyRack                  INTEGER,
        cpqRackPowerSupplyChassis               INTEGER,
        cpqRackPowerSupplyIndex                 INTEGER,
        cpqRackPowerSupplyEnclosureName         DisplayString,
        cpqRackPowerSupplySerialNum             DisplayString,
        cpqRackPowerSupplyPartNumber            DisplayString,
        cpqRackPowerSupplySparePartNumber       DisplayString,
        cpqRackPowerSupplyFWRev                 DisplayString,
        cpqRackPowerSupplyMaxPwrOutput          INTEGER,
        cpqRackPowerSupplyCurPwrOutput          INTEGER,
        cpqRackPowerSupplyPosition              INTEGER,
        cpqRackPowerSupplyIntakeTemp            INTEGER,
        cpqRackPowerSupplyExhaustTemp           INTEGER,
        cpqRackPowerSupplyStatus                INTEGER,
        cpqRackPowerSupplyInputLineStatus       INTEGER,
        cpqRackPowerSupplyPresent               INTEGER,
        cpqRackPowerSupplyCondition             INTEGER,
        cpqRackPowerSupplyEnclosureSerialNum    DisplayString
    }

    cpqRackPowerSupplyRack OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this rack."
        ::= { cpqRackPowerSupplyEntry 1 }

    cpqRackPowerSupplyChassis OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this power enclosure in the rack."
        ::= { cpqRackPowerSupplyEntry 2 }

    cpqRackPowerSupplyIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this power supply in the enclosure."
        ::= { cpqRackPowerSupplyEntry 3 }

    cpqRackPowerSupplyEnclosureName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the power supply enclosure in which this power supply
            resides.

            The string will be empty if the enclosure does not report the
            name or it could not be determined."
        ::= { cpqRackPowerSupplyEntry 4 }

    cpqRackPowerSupplySerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the power supply.

            The string will be empty if the power supply does not report the
            serial number."
        ::= { cpqRackPowerSupplyEntry 5 }

    cpqRackPowerSupplyPartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The part number of the power supply.

            The string will be empty if the power supply does not report this
            function."
        ::= { cpqRackPowerSupplyEntry 6 }

    cpqRackPowerSupplySparePartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The spare part number of the power supply.

            The string will be empty if the power supply does not report this
            function."
        ::= { cpqRackPowerSupplyEntry 7 }

    cpqRackPowerSupplyFWRev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The firmware revision of the power supply.

            The string will be empty if the power supply does not report the
            firmware revision."
        ::= { cpqRackPowerSupplyEntry 8 }

    cpqRackPowerSupplyMaxPwrOutput OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The maximum power output of the power supply in watts.

            The value will be -1 if the power supply does not report the
            value."
        ::= { cpqRackPowerSupplyEntry 9 }

    cpqRackPowerSupplyCurPwrOutput OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The current power output of the power supply in watts.

            The value will be -1 if the power supply does not report the
            value."
        ::= { cpqRackPowerSupplyEntry 10 }

    cpqRackPowerSupplyPosition OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The position of the power supply within the power enclosure.

            This will be -1 if the power enclosure does not report the
            power supply information or it could not be determined."
        ::= { cpqRackPowerSupplyEntry 11 }

    cpqRackPowerSupplyIntakeTemp OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The current air temperature at the intake of the power supply
            in degrees celsius.

            The value will be -1 if the power supply does not report the
            value."
        ::= { cpqRackPowerSupplyEntry 12 }

    cpqRackPowerSupplyExhaustTemp OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The current air temperature at the exhaust of the power supply
            in degrees celsius.

            The value will be -1 if the power supply does not report the
            value."
        ::= { cpqRackPowerSupplyEntry 13 }

    cpqRackPowerSupplyStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            noError(1),
            generalFailure(2),
            bistFailure(3),
            fanFailure(4),
            tempFailure(5),
            interlockOpen(6),
            epromFailed(7),
            vrefFailed(8),
            dacFailed(9),
            ramTestFailed(10),
            voltageChannelFailed(11),
            orringdiodeFailed(12),
            brownOut(13),
            giveupOnStartup(14),
            nvramInvalid(15),
            calibrationTableInvalid(16)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The status of the power supply."
        ::= { cpqRackPowerSupplyEntry 14 }

    cpqRackPowerSupplyInputLineStatus OBJECT-TYPE
        SYNTAX  INTEGER {
            noError(1),
            lineOverVoltage(2),
            lineUnderVoltage(3),
            lineHit(4),
            brownOut(5),
            linePowerLoss(6)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The status of line input power."
        ::= { cpqRackPowerSupplyEntry 15 }

    cpqRackPowerSupplyPresent OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            absent(2),
            present(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This specifies if the power supply described is present in the
            enclosure."
        ::= { cpqRackPowerSupplyEntry 16 }

    cpqRackPowerSupplyCondition OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            ok(2),
            degraded(3),
            failed(4)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The condition of the power supply.

            This value will be one of the following:

            other(1)
              The status could not be determined or not present.

            ok(2)
              The power supply is operating normally.

            degraded(3)
              A temperature sensor, fan or other power supply component is
              outside of normal operating range.

            failed(4)
              A power supply component detects a condition that could
              possibly damage the system."
        ::= { cpqRackPowerSupplyEntry 17 }

    cpqRackPowerSupplyEnclosureSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the power supply enclosure in which this
            power supply resides.

            The string will be empty if the enclosure does not report the
            serial number or it could not be determined."
        ::= { cpqRackPowerSupplyEntry 18 }


-- ****************************************************************************
--   Rack Network Connector Table
--   ============================
--
-- The compaq enterprise                 (1.3.6.1.4.1.232)
--      cpqRackInfo Group                (1.3.6.1.4.1.232.22)
--       cpqRackComponent Group          (1.3.6.1.4.1.232.22.2)
--        cpqRackNetwork Group           (1.3.6.1.4.1.232.22.2.6)
--         cpqRackNetConnector Group     (1.3.6.1.4.1.232.22.2.6.1)
--          cpqRackNetConnectorTable     (1.3.6.1.4.1.232.22.2.6.1.1)
--
-- ****************************************************************************

    cpqRackNetConnectorTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF CpqRackNetConnectorEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A table of rack network connector information."
        ::= { cpqRackNetConnector 1 }

    cpqRackNetConnectorEntry OBJECT-TYPE
        SYNTAX  CpqRackNetConnectorEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION
            "A rack network connector description."
        INDEX   { cpqRackNetConnectorRack,
                  cpqRackNetConnectorChassis,
                  cpqRackNetConnectorIndex }
        ::= { cpqRackNetConnectorTable 1 }

    CpqRackNetConnectorEntry ::= SEQUENCE {
        cpqRackNetConnectorRack                 INTEGER,
        cpqRackNetConnectorChassis              INTEGER,
        cpqRackNetConnectorIndex                INTEGER,
        cpqRackNetConnectorEnclosureName        DisplayString,
        cpqRackNetConnectorName                 DisplayString,
        cpqRackNetConnectorModel                DisplayString,
        cpqRackNetConnectorSerialNum            DisplayString,
        cpqRackNetConnectorPartNumber           DisplayString,
        cpqRackNetConnectorSparePartNumber      DisplayString,
        cpqRackNetConnectorFWRev                DisplayString,
        cpqRackNetConnectorType                 INTEGER,
        cpqRackNetConnectorLocation             DisplayString,
        cpqRackNetConnectorPresent              INTEGER,
        cpqRackNetConnectorHasFuses             INTEGER,
        cpqRackNetConnectorEnclosureSerialNum   DisplayString
    }

    cpqRackNetConnectorRack OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this rack."
        ::= { cpqRackNetConnectorEntry 1 }

    cpqRackNetConnectorChassis OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this server enclosure in the rack."
        ::= { cpqRackNetConnectorEntry 2 }

    cpqRackNetConnectorIndex OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "A number that uniquely specifies this network connector in the rack."
        ::= { cpqRackNetConnectorEntry 3 }

    cpqRackNetConnectorEnclosureName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the network connector enclosure.

            The string will be empty if the enclosure does not report the
            name or it could not be determined."
        ::= { cpqRackNetConnectorEntry 4 }

    cpqRackNetConnectorName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The name of the network connector.

            The string will be empty if the network connector does not report the
            name or it could not be determined."
        ::= { cpqRackNetConnectorEntry 5 }

    cpqRackNetConnectorModel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The model name of the network connector.

            The string will be empty if the network connector does not report the
            model information."
        ::= { cpqRackNetConnectorEntry 6 }

    cpqRackNetConnectorSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the network connector.

            The string will be empty if the network connector does not report the
            serial number."
        ::= { cpqRackNetConnectorEntry 7 }

    cpqRackNetConnectorPartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The part number of the network connector.

            The string will be empty if the enclosure does not report this
            function."
        ::= { cpqRackNetConnectorEntry 8 }

    cpqRackNetConnectorSparePartNumber OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The spare part number of the network connector.

            The string will be empty if the enclosure does not report this
            function."
        ::= { cpqRackNetConnectorEntry 9 }

    cpqRackNetConnectorFWRev OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The firmware revision of the network connector.

            The string will be empty if the network connector does not report the
            firmware revision."
        ::= { cpqRackNetConnectorEntry 10 }

    cpqRackNetConnectorType OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            passive(2),
            active(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The type of network connector within the enclosure."
        ::= { cpqRackNetConnectorEntry 11 }

    cpqRackNetConnectorLocation OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The location of the network connector within the enclosure."
        ::= { cpqRackNetConnectorEntry 12 }

    cpqRackNetConnectorPresent OBJECT-TYPE
        SYNTAX  INTEGER {
            other(1),
            absent(2),
            present(3)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "This specifies if the network connector described is present in the
            enclosure."
        ::= { cpqRackNetConnectorEntry 13 }

    cpqRackNetConnectorHasFuses OBJECT-TYPE
        SYNTAX  INTEGER {
            false(1),
            true(2)
            }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The network connector contains fuses.

            This will be true(2) is the network connector contains fuses.
            The cpqRackCommonEnclosureFuseTable will contain the fuse
            specific information.

            Match the cpqRackNetworkEnclosureSerialNum in this table to the
            serial number in the cpqRackCommonEnclosureFusTable to get complete
            information on the fuses."
        ::= { cpqRackNetConnectorEntry 14 }

    cpqRackNetConnectorEnclosureSerialNum OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The serial number of the enclosure containing the network connector.

            The string will be empty if the enclosure does not report the
            serial number or it could not be determined."
        ::= { cpqRackNetConnectorEntry 15 }


-- ****************************************************************************
--   Rack System Object Identification
--   =================================
--
-- The compaq enterprise                 (1.3.6.1.4.1.232)
--      cpqRackInfo Group                (1.3.6.1.4.1.232.22)
--       cpqRackSysObjID Group           (1.3.6.1.4.1.232.22.3)
--
-- ****************************************************************************

    cpqRackSystemObjectIdentification OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..64))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            "The hardware identification string.

            The string will reported by the rack firmware."
        ::= { cpqRackSysObjID 1 }


-- ****************************************************************************
--  Rack Information Trap Definitions
--  =================================
--
--  The SNMP trap messages must not be bigger than 484 octets (bytes).
--
--  Trap support in an SNMP agent implementation is optional.  An SNMP
--  agent implementation may support all, some, or none of the traps.
--  If traps are supported, The user should be provided with the option of
--  disabling traps.
-- **************************************************************************

    cpqRackNameChanged TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackSerialNum,
                     cpqRackTrapSequenceNum }
        DESCRIPTION
           "Rack name has changed.

            This trap signifies that an agent or utility has changed the name
            of the rack.  Each of the server blades in each of the enclosure
            within the rack will be updated to reflect the new rack name.

            It may take several minutes for the rack name change to be
            propagated throughout the entire rack.

            User Action: None."

        --#TYPE "Rack name changed (22001)"
        --#SUMMARY "The rack name has changed to %s."
        --#ARGUMENTS {2}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 22001

    cpqRackEnclosureNameChanged TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureModel,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The enclosure name has changed.

            This trap signifies that an agent or utility has changed the name
            of an enclosure within the rack.  Each of the components
            within the rack will be updated to reflect the new enclosure name.

            It may take several minutes for the enclosure name change to be
            propagated throughout the entire enclosure.

            User Action: None."

        --#TYPE "Enclosure name changed (22002)"
        --#SUMMARY "The enclosure name has changed to %s in rack %s."
        --#ARGUMENTS {4, 2}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 22002

    cpqRackEnclosureRemoved TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureModel,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The enclosure has been removed.

            This trap signifies that an enclosure has been removed from
            the rack.

            User Action: None."

        --#TYPE "Enclosure removed (22003)"
        --#SUMMARY "The enclosure %s has been removed from rack %s."
        --#ARGUMENTS {4, 2}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 22003

    cpqRackEnclosureInserted TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureModel,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The enclosure has been inserted.

            This trap signifies that an enclosure has been inserted into
            the rack.

            User Action: None."

        --#TYPE "Enclosure inserted (22004)"
        --#SUMMARY "The enclosure %s has been inserted into rack %s."
        --#ARGUMENTS {4, 2}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 22004

    cpqRackEnclosureTempFailed TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTempLocation,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The enclosure temperature status has been set to failed.

            This trap signifies that a enclosure temperature sensor has
            been tripped indicating an overheat condition.

            User Action: Shutdown the enclosure and possibly the rack
            as soon as possible.  Insure all fans are working properly and
            that air flow in the rack has not been blocked."

        --#TYPE "Enclosure temperature failed (22005)"
        --#SUMMARY "The enclosure %s temperature sensor in rack %s has been set to failed."
        --#ARGUMENTS {4, 2}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE NONOPERATIONAL

        ::= 22005

    cpqRackEnclosureTempDegraded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTempLocation,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The enclosure temperature status has been set to degraded.

            This trap signifies that an enclosure temperature sensor has
            been tripped indicating a possible overheat condition.

            User Action: Shutdown the enclosure and possibly the rack
            as soon as possible.  Insure all fans are working properly and
            that air flow in the rack has not been blocked."

        --#TYPE "Enclosure temperature degraded (22006)"
        --#SUMMARY "The enclosure %s temperature sensor in rack %s has been set to degraded."
        --#ARGUMENTS {4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22006

    cpqRackEnclosureTempOk TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTempLocation,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The enclosure temperature status has been set to ok.

            This trap signifies that an enclosure temperature sensor has
            returned to normal.

            User Action: None."

        --#TYPE "Enclosure temperature ok (22007)"
        --#SUMMARY "The enclosure %s temperature sensor in rack %s has been set to ok."
        --#ARGUMENTS {4, 2}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 22007

    cpqRackEnclosureFanFailed TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureFanLocation,
                     cpqRackCommonEnclosureFanSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The enclosure fan status has been set to failed.

            This trap signifies that an enclosure fan has failed and
            no other fans in the redundant fan group are operating.
            This may result in overheating of the enclosure.

            User Action: Replace the fan as soon as possible."

        --#TYPE "Enclosure fan failed (22008)"
        --#SUMMARY "The enclosure %s fan in rack %s has been set to failed."
        --#ARGUMENTS {4, 2}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE NONOPERATIONAL

        ::= 22008

    cpqRackEnclosureFanDegraded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureFanLocation,
                     cpqRackCommonEnclosureFanSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The enclosure fan status has been set to degraded.

            This trap signifies that an enclosure fan has failed but
            other fans in the redundant fan group are still operating.
            This may result in overheating of the enclosure.

            User Action: Replace the fan as soon as possible."

        --#TYPE "Enclosure fan degraded (22009)"
        --#SUMMARY "The enclosure %s fan in rack %s has been set to degraded."
        --#ARGUMENTS {4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22009

    cpqRackEnclosureFanOk TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureFanLocation,
                     cpqRackCommonEnclosureFanSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The enclosure fan status has been set to ok.

            This trap signifies that an enclosure fan has returned
            to normal operation.

            User Action: None."

        --#TYPE "Enclosure fan ok (22010)"
        --#SUMMARY "The enclosure %s fan in rack %s has been set to ok."
        --#ARGUMENTS {4, 2}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 22010


    cpqRackEnclosureFanRemoved TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureFanLocation,
                     cpqRackCommonEnclosureFanSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The enclosure fan has been removed.

            User Action: None."

        --#TYPE "Enclosure fan removed (22011)"
        --#SUMMARY "The enclosure %s fan in rack %s has been removed."
        --#ARGUMENTS {4, 2}
        --#SEVERITY MINOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22011

    cpqRackEnclosureFanInserted TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureFanLocation,
                     cpqRackCommonEnclosureFanSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The enclosure fan has been inserted.

            User Action: None."

        --#TYPE "Enclosure fan inserted (22012)"
        --#SUMMARY "The enclosure %s fan in rack %s has been inserted."
        --#ARGUMENTS {4, 2}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 22012

    cpqRackPowerSupplyFailed TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackPowerSupplyEnclosureName,
                     cpqRackPowerSupplySerialNum,
                     cpqRackPowerSupplyPosition,
                     cpqRackPowerSupplyFWRev,
                     cpqRackPowerSupplySparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The power supply status has been set to failed.

            This trap signifies that a power supply has failed.

            User Action: Replace the power supply as soon as possible."

        --#TYPE "Rack power supply failed (22013)"
        --#SUMMARY "The power supply %s in enclosure %s in rack %s has been set to failed."
        --#ARGUMENTS {6, 4, 2}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE NONOPERATIONAL

        ::= 22013

    cpqRackPowerSupplyDegraded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackPowerSupplyEnclosureName,
                     cpqRackPowerSupplySerialNum,
                     cpqRackPowerSupplyPosition,
                     cpqRackPowerSupplyFWRev,
                     cpqRackPowerSupplySparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The power supply status has been set to degraded.

            This trap signifies that a power supply has degraded.

            User Action: Replace the power supply as soon as possible."

        --#TYPE "Rack power supply degraded (22014)"
        --#SUMMARY "The power supply %s in enclosure %s in rack %s has been set to degraded."
        --#ARGUMENTS {6, 4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22014

    cpqRackPowerSupplyOk TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackPowerSupplyEnclosureName,
                     cpqRackPowerSupplySerialNum,
                     cpqRackPowerSupplyPosition,
                     cpqRackPowerSupplyFWRev,
                     cpqRackPowerSupplySparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The power supply status has been set to ok.

            This trap signifies that a power supply has returned to normal
            operation.

            User Action: None."

        --#TYPE "Rack power supply ok (22015)"
        --#SUMMARY "The power supply %s in enclosure %s in rack %s has been set to ok."
        --#ARGUMENTS {6, 4, 2}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 22015

    cpqRackPowerSupplyRemoved TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackPowerSupplyEnclosureName,
                     cpqRackPowerSupplySerialNum,
                     cpqRackPowerSupplyPosition,
                     cpqRackPowerSupplyFWRev,
                     cpqRackPowerSupplySparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The power supply has been removed.

            User Action: None."

        --#TYPE "Rack power supply removed (22016)"
        --#SUMMARY "The power supply %s in enclosure %s in rack %s has been removed."
        --#ARGUMENTS {6, 4, 2}
        --#SEVERITY MINOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22016

    cpqRackPowerSupplyInserted TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackPowerSupplyEnclosureName,
                     cpqRackPowerSupplySerialNum,
                     cpqRackPowerSupplyPosition,
                     cpqRackPowerSupplyFWRev,
                     cpqRackPowerSupplySparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The power supply has been inserted.

            User Action: None."

        --#TYPE "Rack power supply inserted (22017)"
        --#SUMMARY "The power supply %s in enclosure %s in rack %s has been inserted."
        --#ARGUMENTS {6, 4, 2}
        --#SEVERITY INFORMATIONAL
        --#TIMEINDEX 99
        --#STATE OPERATIONAL

        ::= 22017

    cpqRackPowerSubsystemNotRedundant TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackPowerEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The rack power subsystem is no longer in a redundant state.

            User Action: Replace any failed power supplies as soon as possible
            to return the system to a redundant state."

        --#TYPE "Rack power subsystem not redundant (22018)"
        --#SUMMARY "The power subsystem in enclosure %s in rack %s is no longer redundant."
        --#ARGUMENTS {4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22018

    cpqRackPowerSubsystemLineVoltageProblem TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackPowerSupplyEnclosureName,
                     cpqRackPowerSupplyPosition,
                     cpqRackPowerSupplyFWRev,
                     cpqRackPowerSupplyInputLineStatus,
                     cpqRackPowerSupplySparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The rack power supply detected an input line voltage problem.

            User Action: Check the power input for the power supply or replace
            any failed power supplies as soon as possible."

        --#TYPE "Rack power supply input voltage problem (22019)"
        --#SUMMARY "The rack power supply detected an input line voltage problem in power supply %s, enclosure %s, rack %s."
        --#ARGUMENTS {5, 4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22019

    cpqRackPowerSubsystemOverloadCondition TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackPowerEnclosureName,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "The rack power subsystem overload condition.

            User Action: Replace any failed power supplies as soon as possible
            to return the system to a redundant state."

        --#TYPE "Rack power subsystem overload condition (22020)"
        --#SUMMARY "The power subsystem in enclosure %s in rack %s is in an overload condition."
        --#ARGUMENTS {4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22020

    cpqRackPowerShedAutoShutdown TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackServerBladeEnclosureName,
                     cpqRackServerBladePosition,
                     cpqRackServerBladeSparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Server shutdown due to power shedding.

            The server blade was shutdown due to a lack of power.

            User Action: Check power connections or add power supplies."

        --#TYPE "Server shutdown due to power shedding (22021)"
        --#SUMMARY "The server shutdown due to lack of power blade %s, in enclosure %s, in rack %s."
        --#ARGUMENTS {5, 4, 2}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE NONOPERATIONAL

        ::= 22021

    cpqRackServerPowerOnFailedNotRedundant TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackServerBladeEnclosureName,
                     cpqRackServerBladePosition,
                     cpqRackServerBladeSparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Server power on prevented to preserve redundancy.

            There is not enough power to power on the server blade and
            maintain redundancy for the other blades in the enclosure.

            User Action: Check power connections or add power supplies."

        --#TYPE "Server power on prevented to preserve redundancy (22022)"
        --#SUMMARY "Server power on prevented to preserve redundancy in blade %s, in enclosure %s, in rack %s."
        --#ARGUMENTS {5, 4, 2}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE NONOPERATIONAL

        ::= 22022

    cpqRackServerPowerOnFailedNotEnoughPower TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackServerBladeEnclosureName,
                     cpqRackServerBladePosition,
                     cpqRackServerBladeSparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Inadequate power to power on.

            There is not enough power to power on the server blade.

            User Action: Check power connections or add power supplies."

        --#TYPE "Inadequate power to power on (22023)"
        --#SUMMARY "Inadequate power to power on blade %s, in enclosure %s, in rack %s."
        --#ARGUMENTS {5, 4, 2}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE NONOPERATIONAL

        ::= 22023

    cpqRackServerPowerOnFailedEnclosureNotFound TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackServerBladeEnclosureName,
                     cpqRackServerBladePosition,
                     cpqRackServerBladeSparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Inadequate power to power on.

            There is not enough power to power on the server blade.  The
            server enclosure micro-controller was not found.

            User Action: Check server enclosure connections or add power supplies."

        --#TYPE "Inadequate power to power on (22024)"
        --#SUMMARY "Inadequate power to power on blade %s, in enclosure %s, in rack %s."
        --#ARGUMENTS {5, 4, 2}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE NONOPERATIONAL

        ::= 22024

    cpqRackServerPowerOnFailedPowerChassisNotFound TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackServerBladeEnclosureName,
                     cpqRackServerBladePosition,
                     cpqRackServerBladeSparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Inadequate power to power on.

            There is not enough power to power on the server blade.  The
            power enclosure micro-controller was not found.

            User Action: Check power enclosure connections or add power supplies."

        --#TYPE "Inadequate power to power on (22025)"
        --#SUMMARY "Inadequate power to power on blade %s, in enclosure %s, in rack %s."
        --#ARGUMENTS {5, 4, 2}
        --#SEVERITY CRITICAL
        --#TIMEINDEX 99
        --#STATE NONOPERATIONAL

        ::= 22025

    cpqRackServerPowerOnManualOverride TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackServerBladeEnclosureName,
                     cpqRackServerBladePosition,
                     cpqRackServerBladeSparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Server power on via manual override.

            The server blade was powered on by a manual override.

            User Action: None."

        --#TYPE "Server power on via manual override (22026)"
        --#SUMMARY "Server power on via manual override on blade %s, in enclosure %s, in rack %s."
        --#ARGUMENTS {5, 4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22026

    cpqRackFuseOpen TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureFuseLocation,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Fuse open.

            The fuse has been tripped.

            User Action: Check enclosure and / or blade power connections and
            reset the fuse."

        --#TYPE "Fuse open (22027)"
        --#SUMMARY "Fuse open fuse %s, in enclosure %s, in rack %s."
        --#ARGUMENTS {5, 4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22027


    cpqRackServerBladeRemoved TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackServerBladeEnclosureName,
                     cpqRackServerBladeName,
                     cpqRackServerBladePosition,
                     cpqRackServerBladeSparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Server blade removed.

            The server blade has been removed from the enclosure.

            User Action: None."

        --#TYPE "Server blade removed (22028)"
        --#SUMMARY "Server blade %s removed from position %s, in enclosure %s, in rack %s."
        --#ARGUMENTS {5, 6, 4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22028

    cpqRackServerBladeInserted TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackServerBladeEnclosureName,
                     cpqRackServerBladeName,
                     cpqRackServerBladePosition,
                     cpqRackServerBladeSparePartNumber,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Server blade inserted.

            The server blade has been inserted into the enclosure.

            User Action: None."

        --#TYPE "Server blade inserted (22029)"
        --#SUMMARY "Server blade %s inserted into position %s, in enclosure %s, in rack %s."
        --#ARGUMENTS {5, 6, 4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22029

    cpqRackPowerChassisNotLoadBalanced TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Power subsystem not load balanced.

            The power subsystem is out of balance for this power enclosure.

            User Action: Check the power enclosure and power supplies.  Replace
            any failed or degraded power supplies.  Add additional power supplies
            if needed."

        --#TYPE "Power subsystem not load balanced (22030)"
        --#SUMMARY "Power subsystem not load balanced in enclosure %s, in rack %s."
        --#ARGUMENTS {4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22030

    cpqRackPowerChassisDcPowerProblem TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Power subsystem DC power problem.

            There is a power subsystem DC power problem for this power enclosure.

            User Action: Check the power enclosure and power supplies.  Replace
            any failed or degraded power supplies."

        --#TYPE "Power subsystem DC power problem (22031)"
        --#SUMMARY "Power subsystem DC power problem in enclosure %s, in rack %s."
        --#ARGUMENTS {4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22031

    cpqRackPowerChassisAcFacilityPowerExceeded TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Power subsystem AC facility input power exceeded.

            There is a power subsystem Power subsystem AC facility input power
            exceeded for this power enclosure.

            User Action: Check the power enclosure and power supplies.  Replace
            any failed or degraded power supplies."

        --#TYPE "Power subsystem AC facility input power exceeded (22032)"
        --#SUMMARY "Power subsystem AC facility input power exceeded in enclosure %s, in rack %s."
        --#ARGUMENTS {4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22032



    cpqRackPowerUnknownPowerConsumption TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Unknown power consumption.

            There is an unknown power consumer drawing power.

            User Action: Check the power enclosure and power supplies.  Replace
            any failed or degraded power supplies."

        --#TYPE "Unknown power consumption (22033)"
        --#SUMMARY "Unknown power consumption in rack %s."
        --#ARGUMENTS {2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22033

    cpqRackPowerChassisLoadBalancingWireMissing TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Power subsystem load balancing wire missing.

            The power subsystem load balancing wire missing.

            User Action: Connect the load balancing wire."

        --#TYPE "Power subsystem load balancing wire missing (22034)"
        --#SUMMARY "Power subsystem load balancing wire missing for enclosure %s, in rack %s."
        --#ARGUMENTS {4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22034

    cpqRackPowerChassisTooManyPowerChassis TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Power subsystem has too may power enclosures.

            The maximum number of power enclosures has been exceeded.

            User Action: Remove the extra power enclosure."

        --#TYPE "Power subsystem has too may power enclosures (22035)"
        --#SUMMARY "Power subsystem has too may power enclosures %s, in rack %s."
        --#ARGUMENTS {4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22035

    cpqRackPowerChassisConfigError TRAP-TYPE
        ENTERPRISE compaq
        VARIABLES  { sysName,
                     cpqHoTrapFlags,
                     cpqRackName,
                     cpqRackUid,
                     cpqRackCommonEnclosureName,
                     cpqRackCommonEnclosureSerialNum,
                     cpqRackCommonEnclosureSparePartNumber,
                     cpqRackCommonEnclosureTrapSequenceNum }
        DESCRIPTION
           "Power subsystem improperly configured.

            The power subsystem has been improperly configured.

            User Action: Check the cabling of the power enclosure."

        --#TYPE "Power subsystem improperly configured (22036)"
        --#SUMMARY "Power subsystem has been improperly configured in enclosure %s, in rack %s."
        --#ARGUMENTS {4, 2}
        --#SEVERITY MAJOR
        --#TIMEINDEX 99
        --#STATE DEGRADED

        ::= 22036

END

