#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2005 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

#-----------------------------
# Definiton for trap 3046
#-----------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3046*'
       MSGNODE=*
       DEScription='HP - Drive Array physical drive Status Change (3046)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Drive Array physical drive Status Change (TrapData: &(26:))'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The specific information about the alarm could not be parsed, so the original trap information is displayed. If the physical drive status is failed(3) or predictiveFailure(4), replace the drive.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3046 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Drive Array physical drive Status Other (3046)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Drive Array physical drive Status Other (Controller Location: &26 &27, Controller: &32, Drive: &37, Drive Location: &42 &43 &44 &45 &46, Type: &51, Model: &56 &57, Firmware: &62, SN: &67 &68, FailureCode: &73, Bus: &83)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3046 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Drive Array physical drive Status Ok (3046)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Drive Array physical drive Status Ok (Controller Location: &26 &27, Controller: &32, Drive: &37, Drive Location: &42 &43 &44 &45 &46, Type: &51, Model: &56 &57, Firmware: &62, SN: &67 &68, FailureCode: &73, Bus: &83)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3046 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Drive Array physical drive Status Failed (3046)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Drive Array physical drive Status Failed (Controller Location: &26 &27, Controller: &32, Drive: &37, Drive Location: &42 &43 &44 &45 &46, Type: &51, Model: &56 &57, Firmware: &62, SN: &67 &68, FailureCode: &73, Bus: &83)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3046 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Drive Array physical drive Status PredictiveFailure (3046)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Drive Array physical drive Status Predictive Failure (Controller Location: &26 &27, Controller: &32, Drive: &37, Drive Location: &42 &43 &44 &45 &46, Type: &51, Model: &56 &57, Firmware: &62, SN: &67 &68, FailureCode: &73, Bus: &83)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The S.M.A.R.T. hard drive or HP specific hard drive predicts imminent failure. The device or client issuing this alarm has a drive that exceeded one or more factory preset thresholds for functional degradation.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='As a result of normal wear and tear, the operation of a hard drive may gradually deteriorate. If certain thresholds are exceeded, the drive may not perform to specified levels, and may be subject to hardware failure sometime in the future.'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='Drives that exceed these thresholds need to be replaced, although true catastrophic failure has not yet occurred.'



#-----------------------------
# Definiton for trap 3047
#-----------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3047*'
	MSGNODE=*
	DEScription='HP - Drive Array spare drive Status Change (3047)'
	TYPE=MSG
DEFine MSGACTion NAME=(*,10)
	ACTION=sendkeep TEXT='HP - Drive Array spare drive Status Change (TrapData: &(26:))'
        SEVERITY=E
	ATTRIB=default
	COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The specific information about the alarm could not be parsed, so the original trap information is displayed.  The 4th variable represents the drive status: other(1), invalid(2), failed(3), inactive(4), building(5), active(6).'

# Two spaces for location

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3047 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
	MSGNODE=*
	DEScription='HP - Drive Array spare drive Status Other (3047)'
	TYPE=MSG
DEFine MSGACTion NAME=(*,10)
	ACTION=sendkeep TEXT='HP - Drive Array spare drive Status Other (Controller Location: &26 &27, Controller: &32, Drive: &37, Spare Location: &47 &48 &49 &50 &51, Bus: &56)'
        SEVERITY=I
	ATTRIB=default
	COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3047 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
	MSGNODE=*
	DEScription='HP - Drive Array spare drive Status Invalid (3047)'
	TYPE=MSG
DEFine MSGACTion NAME=(*,10)
	ACTION=sendkeep TEXT='HP - Drive Array spare drive Status Invalid (Controller Location: &26 &27, Controller: &32, Drive: &37, Spare Location: &47 &48 &49 &50 &51, Bus: &56)'
        SEVERITY=E
	ATTRIB=default
	COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3047 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
	MSGNODE=*
	DEScription='HP - Drive Array spare drive Status Failed (3047)'
	TYPE=MSG
DEFine MSGACTion NAME=(*,10)
	ACTION=sendkeep TEXT='HP - Drive Array spare drive Status Failed (Controller Location: &26 &27, Controller: &32, Drive: &37, Spare Location: &47, Bus: &52)'
        SEVERITY=E
	ATTRIB=default
	COLOR=red


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3047 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
	MSGNODE=*
	DEScription='HP - Drive Array spare drive Status Inactive (3047)'
	TYPE=MSG
DEFine MSGACTion NAME=(*,10)
	ACTION=sendkeep TEXT='HP - Drive Array spare drive Status Inactive (Controller Location: &26 &27, Controller: &32, Drive: &37, Spare Location: &47 &48 &49 &50 &51, Bus: &56)'
        SEVERITY=I
	ATTRIB=default
	COLOR=BLUE
DEFine MSGACTion NAME=(*,20)
        ACTION=ANNOTATE TEXT='This alarm signifies that the spare is in a ready state.  This alarm is typically issued if you install or replace a spare drive in a drive array. It is issued after you replace a failed spare drive with a new one.'
DEFine MSGACTion NAME=(*,30)
        ACTION=ANNOTATE TEXT='This alarm may also occur when a drive fails and the spare becomes active, the failed drive is replaced, and the spare eventually becomes inactive again.'
DEFine MSGACTion NAME=(*,40)
        ACTION=ANNOTATE TEXT='In fault tolerant configurations, when a drive fails and a spare drive is available, the storage subsystem begins building data onto that spare.'
DEFine MSGACTion NAME=(*,50)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced before restoration has completed, the process halts, and the data is restored to the replacement drive instead.'
DEFine MSGACTion NAME=(*,60)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced after the build process is complete, the system reconstructs the data to the replacement drive, and the spare will revert to its original inactive state. This keeps a spare drive available.'
DEFine MSGACTion NAME=(*,70)
        ACTION=ANNOTATE TEXT='If you have installed or replaced a failed drive in the drive array, then this alarm is to be expected.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3047 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
	MSGNODE=*
	DEScription='HP - Drive Array spare drive Status Building (3047)'
	TYPE=MSG
DEFine MSGACTion NAME=(*,10)
	ACTION=sendkeep TEXT='HP - Drive Array spare drive Status Building (Controller Location: &26 &27, Controller: &32, Drive: &37, Spare Location: &47 &48 &49 &50 &51, Bus: &56)'
        SEVERITY=I
	ATTRIB=default
	COLOR=blue
DEFine MSGACTion NAME=(*,20)
        ACTION=ANNOTATE TEXT='This alarm is issued when a spare drive is brought online to replace a failed drive, and the drive array subsystem begins to build data onto the spare.'
DEFine MSGACTion NAME=(*,30)
        ACTION=ANNOTATE TEXT='In fault tolerant configurations, when a spare drive is available, the storage subsystem begins building data onto that spare.'
DEFine MSGACTion NAME=(*,40)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced before restoration has completed, the process halts, and the data is restored to the replacement drive instead.' 
DEFine MSGACTion NAME=(*,50)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced after the build process is complete, the system reconstructs the data to the replacement drive, and the spare reverts to its original inactive state. This keeps a spare drive available.'
DEFine MSGACTion NAME=(*,60)
        ACTION=ANNOTATE TEXT='When a spare drive is available, this alarm is usually issued after the Drive Array Physical Drive Status Change - Failed alarm.  This alarm indicates that a drive has failed.'



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3047 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 6*'
	MSGNODE=*
	DEScription='HP - Drive Array spare drive Status Active (3047)'
	TYPE=MSG
DEFine MSGACTion NAME=(*,10)
	ACTION=sendkeep TEXT='HP - Drive Array spare drive Status Active (Controller Location: &26 &27, Controller: &32, Drive: &37, Spare Location: &47 &48 &49 &50 &51, Bus: &56)'
        SEVERITY=I
	ATTRIB=default
	COLOR=blue
DEFine MSGACTion NAME=(*,20)
        ACTION=ANNOTATE TEXT='A physical drive failed. The array successfully restored data onto a spare. That spare drive has now become active and replaces the failed drive.'
DEFine MSGACTion NAME=(*,30)
        ACTION=ANNOTATE TEXT='In fault tolerant configurations, when a spare drive is available, the storage subsystem begins building data onto that spare.'
DEFine MSGACTion NAME=(*,40)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced before restoration has completed, the process halts, and the data is restored to the replacement drive instead.'
DEFine MSGACTion NAME=(*,50)
        ACTION=ANNOTATE TEXT='If the failed drive is replaced after the build process is complete, the system reconstructs the data to the replacement drive, and the spare will revert to its original inactive state. This keeps a spare drive available.'
