#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6029*'
       MSGNODE=*
       DEScription='HP - Correctable Memory Log Entry'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - correctable memory log entry indicates a memory module needs to be replaced'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6030*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Power Supply: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Power Supply: DEGRADED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6031*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Power Supply: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Power Supply: FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6032*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Power Supply: REDUNDANCY LOST'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Power Supply: REDUNDANCY LOST'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='This may occur if a new hardware component has been added, requiring more power, thereby preventing the power supplies from acting in a redundant capacity.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='You may be able to add another power supply to restore redundancy.  Or verify all power supplies are functioning properly; one or more is possibly failed, degraded, or removed. If so, it should be replaced to restore redundancy.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6033*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Power Supply has been inserted'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Power Supply has been inserted'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6034*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Power Supply has been removed' 
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Power Supply has been removed'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6035*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Fan: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Fan: DEGRADED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='There may be a loss of redundancy until the degraded fan is replaced.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6036*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Fan: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Fan: FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='There may be a loss of redundancy until the failed fan is replaced. If this is not part of a redundant fan system, the server is not being properly cooled and the fan should be replaced as soon as possible.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6037*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Fan: REDUNDANCY LOST'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Fan: REDUNDANCY LOST'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Verify that all fans are installed and functioning properly.  One or more fans is possibly failed, degraded, or removed.  Note the fan number.  Replace the fan to restore redundancy.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6038*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Fan has been inserted'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Fan has been inserted'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6039*'
       MSGNODE=*
       DEScription='HP - Fault Tolerant Fan has been removed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Fault Tolerant Fan has been removed'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040*'
       MSGNODE=*
       DEScription='HP - Temperature: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location Other)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: Other)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location Unknown)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: Unknown)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location System)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: System)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location: System Board)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: System Board)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location: IO Board)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: IO Board)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location: CPU)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: CPU)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 7*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location: Memory)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: Memory)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 8*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location: Storage)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: Storage)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 9*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location: Removable Media)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: Removable Media)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 10*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location: Power Supply)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: Power Supply)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 11*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location: Ambient)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: Ambient)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 12*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location: Chassis)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: Chassis)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6040 * * * * * * * * * * * * * * * * * * * * * 13*'
       MSGNODE=*
       DEScription='HP - Temperature FAILED (Location: Bridge Card)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: FAILED (Chassis: &26, Location: Bridge Card)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
