#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

#
# SWCC Fibre Device Status Change
#

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.132.2.1*'
       MSGNODE=*
       DEScription='HP - SWCC Fibre Device Status Change'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC Fibre Device Status Change (Device Name: &21)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed FibreChannel devices. The variable cpqSwccFibreDevState indicates the current status, but that information could not be parsed.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='The last variable in the original alarm is cpqSwccFibreEventDescription which contains a textual description of the reason for the trap. The status variable may have values of other(1), ok(2), degraded(3), or failed(4).'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='Variables: sysName - the name of the host running the agent, cpqSwccFibreDevName - the name of the device which has changed state, cpqSwccFibreDevState - the current state of the device,' 
DEFine MSGACTion NAME=(*,50)
       ACTION=ANNOTATE TEXT='cpqSwccFibreEventDescription - a textual description of the reason for the trap.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.132.2.1 * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - SWCC Fibre Device Status Change: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC Fibre Device Status Change: OTHER (Device Name: &21)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed FibreChannel devices. Consult the original alarm for cpqSwccFibreEventDescription which contains a textual description of the reason for the trap.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.132.2.1 * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - SWCC Fibre Device Status Change: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC Fibre Device Status Change: OK (Device Name: &21)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed FibreChannel devices. Consult the original alarm for cpqSwccFibreEventDescription which contains a textual description of the reason for the trap.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.132.2.1 * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - SWCC Fibre Device Status Change: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC Fibre Device Status Change: DEGRADED (Device Name: &21)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed FibreChannel devices. Consult the original alarm for cpqSwccFibreEventDescription which contains a textual description of the reason for the trap.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.132.2.1 * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - SWCC Fibre Device Status Change: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC Fibre Device Status Change: FAILED (Device Name: &21)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed FibreChannel devices. Consult the original alarm for cpqSwccFibreEventDescription which contains a textual description of the reason for the trap.'

#
# SWCC Tape Controller Status Change
#

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 2 * * * * * * * * 1.3.6.1.4.1.232.132.2.1*'
       MSGNODE=*
       DEScription='HP - SWCC Tape Controller Status Change'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC Tape Controller Status Change (Device Name: &21)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed FibreChannel Tape Controller devices. The variable cpqSwccFibreDevState indicates the current status, but that information could not be parsed.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='The last variable in the original alarm is cpqSwccFibreEventDescription which contains a textual description of the reason for the trap. The status variable may have values of other(1), ok(2), degraded(3), or failed(4).'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='Variables: sysName - the name of the host running the agent, cpqSwccFibreDevName - the name of the device which has changed state, cpqSwccFibreDevState - the current state of the device,' 
DEFine MSGACTion NAME=(*,50)
       ACTION=ANNOTATE TEXT='cpqSwccFibreEventDescription - a textual description of the reason for the trap.'



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 2 * * * * * * * * 1.3.6.1.4.1.232.132.2.1 * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - SWCC Tape Controller Status Change: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC Tape Controller Status Change: OTHER (Device Name: &21)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed FibreChannel Tape Controller devices. Consult the original alarm for cpqSwccFibreEventDescription which contains a textual description of the reason for the trap.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 2 * * * * * * * * 1.3.6.1.4.1.232.132.2.1 * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - SWCC Tape Controller Status Change: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC Tape Controller Status Change: OK (Device Name: &21)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed FibreChannel Tape Controller devices. Consult the original alarm for cpqSwccFibreEventDescription which contains a textual description of the reason for the trap.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 2 * * * * * * * * 1.3.6.1.4.1.232.132.2.1 * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - SWCC Tape Controller Status Change: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC Tape Controller Status Change: DEGRADED (Device Name: &21)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed FibreChannel Tape Controller devices. Consult the original alarm for cpqSwccFibreEventDescription which contains a textual description of the reason for the trap.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 2 * * * * * * * * 1.3.6.1.4.1.232.132.2.1 * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - SWCC Tape Controller Status Change: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC Tape Controller Status Change: FAILED (Device Name: &21)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed FibreChannel Tape Controller devices. Consult the original alarm for cpqSwccFibreEventDescription which contains a textual description of the reason for the trap.'

#
# EMU Device Status Change
#

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.132.3.1*'
       MSGNODE=*
       DEScription='HP - SWCC EMU Device Status Change'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC EMU Device Status Change (Device Name: &21)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed devices. The variable cpqSwccEmuDevDevState indicates the current status, but that information could not be parsed.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='The last variable in the original alarm is cpqSwccEmuDevEventDescription which contains a textual description of the reason for the trap. The status variable may have values of other(1), ok(2), degraded(3), or failed(4).'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='Variables: sysName - the name of the host running the agent, cpqSwccEmuDevDevName - the name of the device which has changed state, cpqSwccEmuDevDevState - the current state of the device,' 
DEFine MSGACTion NAME=(*,50)
       ACTION=ANNOTATE TEXT='cpqSwccEmuDevEventDescription - a textual description of the reason for the trap.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.132.3.1 * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - SWCC EMU Dev Device Status Change: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC EMU/Device Status Change: OTHER (Device Name: &21)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed devices. Consult the original alarm for cpqSwccEmuDevEventDescription which contains a textual description of the reason for the trap.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.132.3.1 * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - SWCC EMU Dev Device Status Change: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC EMU/Device Status Change: OK (Device Name: &21)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed devices. Consult the original alarm for cpqSwccEmuDevEventDescription which contains a textual description of the reason for the trap.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.132.3.1 * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - SWCC EMU Dev Device Status Change: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC EMU/Device Status Change: DEGRADED (Device Name: &21)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed devices. Consult the original alarm for cpqSwccEmuDevEventDescription which contains a textual description of the reason for the trap.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.132.3.1 * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - SWCC EMU Dev Device Status Change: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC EMU/Device Status Change: FAILED (Device Name: &21)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The SWCC Agent has detected a change in state on one of the managed devices. Consult the original alarm for cpqSwccEmuDevEventDescription which contains a textual description of the reason for the trap.'


#
# KZPCC Controller Events
#

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.132.4.1*'
       MSGNODE=*
       DEScription='HP - SWCC KZPCC Controller - Physical Device Status Change'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC KZPCC Controller - Physical Device Status Change (System Name: &16, Subsystem Name: &21, Event Severity: &26)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Some event has happened to a KZPCC controller that a user maybe interested in knowing. The following variables are included in the trap to provide information to the user:'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='(1) cpqSwccKzpccSystemName - an octet string which will contain ASCII string identifying the name of the system the trap was generated from,'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='(2) cpqSwccKzpccSubsystemName - an octet string which will contain ASCII string identifying the name of the KZPCC controller (as defined by the system) the event occurred on,'
DEFine MSGACTion NAME=(*,50)
       ACTION=ANNOTATE TEXT='(3) cpqSwccKzpccEventSeverity - an enumerated integer that identifies the severity level of the event (1=informational, 2=warning, 3=error), and'
DEFine MSGACTion NAME=(*,60)
       ACTION=ANNOTATE TEXT='(4) cpqSwccKzpccEventDescription - an octet string which will contain an ASCII string describing the event that has occurred.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 2 * * * * * * * * 1.3.6.1.4.1.232.132.4.1*'
       MSGNODE=*
       DEScription='HP - SWCC KZPCC Controller - Virtual Device Status Change'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC KZPCC Controller - Virtual Device Status Change (System Name: &16, Subsystem Name: &21, Event Severity: &26)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Some event has happened to a KZPCC controller that a user maybe interested in knowing. The following variables are included in the trap to provide information to the user:'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='(1) cpqSwccKzpccSystemName - an octet string which will contain ASCII string identifying the name of the system the trap was generated from,'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='(2) cpqSwccKzpccSubsystemName - an octet string which will contain ASCII string identifying the name of the KZPCC controller (as defined by the system) the event occurred on,'
DEFine MSGACTion NAME=(*,50)
       ACTION=ANNOTATE TEXT='(3) cpqSwccKzpccEventSeverity - an enumerated integer that identifies the severity level of the event (1=informational, 2=warning, 3=error), and'
DEFine MSGACTion NAME=(*,60)
       ACTION=ANNOTATE TEXT='(4) cpqSwccKzpccEventDescription - an octet string which will contain an ASCII string describing the event that has occurred.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3 * * * * * * * * 1.3.6.1.4.1.232.132.4.1*'
       MSGNODE=*
       DEScription='HP - SWCC KZPCC Controller - Device Status Change'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SWCC KZPCC Controller - Device Status Change (System Name: &16, Subsystem Name: &21, Event Severity: &26)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Some event has happened to a KZPCC controller that a user maybe interested in knowing. The following variables are included in the trap to provide information to the user:'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='(1) cpqSwccKzpccSystemName - an octet string which will contain ASCII string identifying the name of the system the trap was generated from,'
DEFine MSGACTion NAME=(*,40)
       ACTION=ANNOTATE TEXT='(2) cpqSwccKzpccSubsystemName - an octet string which will contain ASCII string identifying the name of the KZPCC controller (as defined by the system) the event occurred on,'
DEFine MSGACTion NAME=(*,50)
       ACTION=ANNOTATE TEXT='(3) cpqSwccKzpccEventSeverity - an enumerated integer that identifies the severity level of the event (1=informational, 2=warning, 3=error), and'
DEFine MSGACTion NAME=(*,60)
       ACTION=ANNOTATE TEXT='(4) cpqSwccKzpccEventDescription - an octet string which will contain an ASCII string describing the event that has occurred.'



