DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 1 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Device Connected (1)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Device Connected (1)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a Connection Lost due to one of the following. 1. The serial cable connected to the UPS has been unplugged. 2. The Network cable connected to the UPS has been unplugged. Recommendations: 1. Insure all cables are'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='seated properly. 2. check you network to insure it is functioning properly. 3. If the UPS is serially connected insure that the Serial Relay Agent is installed and running.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 2 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Connection Lost (2)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Connection Lost (2)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A UPS device is reporting a Connection Lost due to one of the following. 1. The serial cable connected to the UPS has been unplugged. 2. The Network cable connected to the UPS has been unplugged. Recommendations: 1. Insure all cables are'
DEFine MSGACTion Name=(*,30)
ACTION=ANNOTATE TEXT='seated properly. 2. check you network to insure it is functioning properly. 3. If the UPS is serially connected insure that the Serial Relay Agent is installed and running.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 3 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - DNS Lookup Failed (3)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - DNS Lookup Failed (3)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='CRPM failed to find an IP address for the device hostname.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 4 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Connection Failed (4)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Connection Failed (4)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='CRPM failed to connect to a device.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Device Settings Changed (5)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Device Settings Changed (5)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Device settings have been changed by a user.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10001 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Temperature 1 Below Minimum (10001)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Temperature 1 Below Minimum (10001)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting temperature 1 below minimum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10002 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Temperature 1 Above Warning (10002)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Temperature 1 Above Warning (10002)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting temperature 1 above warning threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10003 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Temperature 1 Above Maximum (10003)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Temperature 1 Above Maximum (10003)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting temperature 1 above maximum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10004 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Temperature 1 Normal (10004)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Temperature 1 Normal (10004)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting temperature 1 has returned to a normal temperature.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10005 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Temperature 2 Below Minimum (10005)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Temperature 2 Below Minimum (10005)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting temperature 2 below minimum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10006 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Temperature 2 Above Warning (10006)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Temperature 2 Above Warning (10006)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting temperature 2 above warning threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10007 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Temperature 2 Above Maximum (10007)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Temperature 2 Above Maximum (10007)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting temperature 2 above maximum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10008 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Temperature 2 Normal (10008)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Temperature 2 Normal (10008)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting temperature 2 has returned to a normal temperature.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10011 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Voltage Below Minimum (10011)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Voltage Below Minimum (10011)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting voltage below minimum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10012 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Voltage Above Maximum (10012)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Voltage Above Maximum (10012)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting voltage above maximum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10013 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Voltage Normal (10013)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Voltage Normal (10013)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting voltage has returned to normal.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10021 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Humidity Below Minimum (10021)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Humidity Below Minimum (10021)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting humidity below minimum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10022 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Humidity Above Maximum (10022)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Humidity Above Maximum (10022)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting humidity above maximum threshold.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10023 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Humidity Normal (10023)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Humidity Normal (10023)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting humidity has returned to normal.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10031 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Smoke Detected (10031)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Smoke Detected (10031)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting smoke detected.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10032 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Smoke Cleared (10032)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Smoke Cleared (10032)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting smoke cleared.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10041 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Shock Detected (10041)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Shock Detected (10041)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting shock detected.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10042 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Shock Cleared (10042)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Shock Cleared (10042)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting shock cleared.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10051 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Aux 1 Alarm (10051)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Aux 1 Alarm (10051)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device has entered an alarm condition for auxiliary input 1.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10052 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Aux 1 Alarm Cleared (10052)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Aux 1 Alarm Cleared (10052)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting auxiliary input 1 alarm cleared.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10053 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Aux 2 Alarm (10053)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Aux 2 Alarm (10053)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device has entered an alarm condition for auxiliary input 2.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10054 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Aux 2 Alarm Cleared (10054)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Aux 2 Alarm Cleared (10054)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting auxiliary input 2 alarm cleared.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10101 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Input 1 Opened (10101)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Input 1 Opened (10101)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting input 1 has been opened.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10102 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Input 1 Closed (10102)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Input 1 Closed (10102)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting input 1 has been closed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10103 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Input 2 Opened (10103)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Input 2 Opened (10103)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting input 2 has been opened.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10104 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Input 2 Closed (10104)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Input 2 Closed (10104)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting input 2 has been closed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10105 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Input 3 Opened (10105)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Input 3 Opened (10105)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting input 3 has been opened.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10106 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Input 3 Closed (10106)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Input 3 Closed (10106)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting input 3 has been closed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10107 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Input 4 Opened (10107)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Input 4 Opened (10107)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting input 4 has been opened.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10108 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Input 4 Closed (10108)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Input 4 Closed (10108)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting input 4 has been closed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10111 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Lockset 1 Unlocked (10111)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Lockset 1 Unlocked (10111)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting lockset 1 has been unlocked.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10112 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - Lockset 1 Failed To Lock (10112)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Lockset 1 Failed To Lock (10112)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting lockset 1 has failed to lock.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10113 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Lockset 1 Error (10113)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Lockset 1 Error (10113)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting an error with lockset 1.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10114 * * * * * * * * 1.3.6.1.4.1.232.154.1.1.0*'
        MSGNODE=*
        DEScription='HP - CMC Lockset 1 Locked (10114)'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - CMC Lockset 1 Locked (10114)'
        SEVERITY=I
        ATTRIB=default
        COLOR=blue
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='A CMC device is reporting lockset 1 has been locked.'

