ProLiant GbE Interconnect Switch SNMP MIB Errata

The following are not supported in the MIB:

RFC1213
1. At ::= { mib-2 3 }
2. Egp ::= { mib-2 8 }
3. Transmission ::= { mib-2 10 }

RFC1215
1. EgpNeighborLoss

RFC1493
1. dot1dStatic ::= { dot1dBridge 5 }
2. dot1dTpFdbTable only applies to Default VLAN 1.
3. dot1dTpFdbTable ::= { dot1dTp 3 }

RFC1757 (RMON)
1. Hosts
2. HostTopN
3. Matrix
4. Filter
5. capture

RFC2233 (IF-MIB)
1. ifRcvAddressTable ::= { ifMIBObjects 4 }
2. ifTestTable ::= { ifMIBObjects 3 }


RFC2358 (Ethernet-Like MIB)
1. dot3StatsSQETestErrors ::= { dot3StatsEntry 6 }
2. dot3StatsInternalMacTransmitErrors ::= { dot3StatsEntry 10 }
3. dot3StatsInternalMacReceiveErrors ::= { dot3StatsEntry 16 }
4. dot3CollTable ::= { dot3 5 }
5. dot3TestTdr ::= { dot3Tests 1 }
6. dot3StatsMultipleCollisionFrames ::= { dot3StatsEntry 5 }
7. dot3StatsSQETestErrors ::= { dot3StatsEntry 6 }
8. dot3StatsInternalMacTransmitErrors ::= { dot3StatsEntry 10 }
9. dot3StatsCarrierSenseErrors ::= { dot3StatsEntry 11 }
10. dot3StatsFrameTooLongs ::= { dot3StatsEntry 13 }
11. dot3StatsInternalMacReceiveErrors ::= { dot3StatsEntry 16 }
12. dot3StatsEtherChipSet ::= { dot3StatsEntry 17 }
13. dot3StatsSymbolErrors ::= { dot3StatsEntry 18 }
14. dot3CollTable :: = { dot3 5 }
15. dot3Tests :: = { dot3 6 }
16. dot3Errors := {dot3 7 }
17. dot3ChipSets := {dot3 8 }
18. dot3StatsTable: dot3StatsEntry supports only the port interfaces.

RFC2674
1. pBridgeMIB ::= { dot1dBridge 6 }
* dot1dGmrp ::= { pBridgeMIBObjects 4 }
* dot1dUserPriorityRegenTable ::= { dot1dPriority 2 } is read-only.
* dot1dTrafficClassesEnabled ::= { dot1dExtBase 2 } is always true.
* dot1dGmrpStatus ::= { dot1dExtBase 3 } is always disabled.
2. qBridgeMIB ::= { dot1dBridge 7 }
* dot1qForwardAllTable ::= { dot1qTp 4 }
* dot1qForwardUnregisteredTable ::= { dot1qTp 5 }
* dot1qPortVlanStatisticsTable ::= { dot1qVlan 6 }
* dot1qPortVlanHCStatisticsTable ::= { dot1qVlan 7 }
* dot1qLearningConstraintsTable ::= { dot1qVlan 8 }
* dot1qConstraintSetDefault ::= { dot1qVlan 9 }
* dot1qConstraintTypeDefault ::= { dot1qVlan 10 }
3. dot1qStaticUnicastReceivePort ::= { dot1qStaticUnicastEntry 2 } always has to be 0.
4. dot1qStaticMulticastReceivePort ::= { dot1qStaticMulticastEntry 2 } always has to be 0.
5. dot1qStaticMulticastForbiddenEgressPorts ::= { dot1qStaticMulticastEntry 4 }  always has to be 0.
6. dot1qNextFreeLocalVlanIndex ::= { dot1qVlan 4 } always has to be 0.
7. dot1qStaticUnicastStatus and dot1qStaticMulticastStatus support setting value only to invalid(2), permanent(3), and deleteOnReset(4).

RFC2737 (Entity MIB)
1. entPhysicalModelName ::= { entPhysicalEntry 13 }

cpqAgent.mib - Common MIB for Basic Config
The following objects are defined as read-write/read-create, but we don't support write on these objects:

1. agentBscSwFileIndex
2. agentBscSwFileDscr
3. agentBscSwFileTransferType
4. agentBscSwFileLocateId
5. agentFileTransfer
6. agentRs232PortConfig -  read/write allowed on pGbE
7. agentOutOfBandBaudRateConfig- read/write/allowed on pGbE
8. agentBscSwFileIndex
9. agentBscSwFileDscr
10. agentBscSwFileTransferType
11. agentBscSwFileLocateId 
12. agentFileTransfer


These traps are generated:

	coldStart 
	warmStart 
	authenticationFailure 
	topologyChange
	newRoot 
	linkDown 
	linkUp
	entConfigChange
