@@QUES 060101 Y/N Q,290,453,301,291
Would you say that static routing tables can react automatically to changes in the internetwork topology?
|
2
|

|
That's right.
|
That's not so. The answer is No.
|
The answer is No.

@@QUES 060102 SXY Q,147,391,302,279
On which of the following do you think static routing works better?
|
Choose an option.
|
Large-scale networks
Small-scale networks
|

|
2
|
That's right.
|
Actually, static routing is much more suitable for small networks. The correct option is highlighted.
|
The correct option is highlighted.

@@QUES 060103 T/F Q,137,417,313,341
Do you think the following statement is true or false?

Information held in static routing tables is automatically conveyed to others as part of an update process.
|
2
|

|
That's right.
|
Actually, it isn't.
|
The statement is false.

@@QUES 060104 XYF Q,144,350,312,318
See if you can choose the correct option to fill in the blank.

Update messages are controlled by the  _  protocol.
|
Choose an option to fill the blank.
|
%010routed
%010routing
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The full statement is now shown.

@@QUES 060105 SXY Q,159,325,270,291
Where do you think router D will relay the packet to?
|
Choose an option.
|
Router C
Router B
Host Y
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 060106 SXY Q,134,321,331,288
What do you think router A will do?
|
Choose an option.
|
It will send the packets via router B
It will discard the packets because Host Y is unreachable 
It will store the packets for Host Y until the link is repaired
|
Router A is using static routing.
|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 060107 Y/N Q,171,289,269,267
Do you think it knows or can find any other route to Host Y?
|
1
|

|
You're right.
|
In fact, it does.
|
The answer is Yes.

@@QUES 060108 T/F Q,121,425,336,350
Do you think the following statement is true or false?

If a router's routing table does not have an entry for a specific destination it cannot communicate with that destination.
|
2
|

|
That's right.
|
Actually, it can.
|
The statement is false.

@@QUES 060201 SXY Q,129,308,342,288
Using 8 bits as the network address, what is the maximum number of networks that can be addressed?
|
Choose an option.
|
8
16
254
255
|

|
3
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.


@@QUES 060301 T/F Q,123,342,339,313
Do you think the following statement is true or false?

A distance vector algorithm know the exact topology of an internetwork.
|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 060302 T/F Q,139,362,314,318
Do you think the following statement is true or false?

Each router sends its entire routing table to its neighbors.
|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.


@@QUES 060303 DTF Q,117,424,358,372
Try to decide which option goes in which blank.

In essence,  _  algorithms send small updates everywhere, while  _  algorithms send larger updates only to neighboring routers.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
%010distance vector
%010link state
|

|
1
|
That's right.
|
In fact, it's the other way around.
|
Incorrect.
|
Incorrect.
|
The full statement is now shown.

@@QUES 060304 SXY Q,138,329,316,303
Which type of routing algorithm requires more CPU power and memory?
|
Choose an option.
|
Link state
Distance vector
|

|
1
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 060305 SXY Q,147,411,313,332
Which of the following types of routing algorithm is the slowest to converge?
|
Choose an option.
|
Link state
Distance vector
Balanced hybrid
|

|
2
|
That's right.
|
That's not it. The correct option is now highlighted.
|
The correct option is now highlighted.

@@QUES 060306 T/F Q,120,367,350,318
Do you think the following statement is true or false?

An Enhanced IGRP creates only one routing table that is used by all routed protocols.
|
2
|

|
That's right.
|
Actually, the statement is false.
|
The statement is false.

@@QUES 060101t SXY Q,0,0,353,331
Which type of routing requires the least amount of input from a network administrator?
|
Choose an option.
|
Static routing
Dynamic routing
Both types require the same input
|
2
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 060102t MXY Q,0,0,372,418
Which of the following statements about static routing is/are true?
|
Choose each appropriate item.
|
Static routers must be changed manually whenever an internetwork topology change requires it
Static routing is ideal for large-scale networks where the traffic is unpredictable
Information held in static routing tables is automatically conveyed to others as part of an update process
Static routing is generally used for security where it is inappropriate to reveal everything about an internetwork
|
1,4
|
28
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 060103t MXY Q,0,0,350,350
In a dynamic router, which of the following is/are controlled by the routing protocol?
|
Choose each appropriate item.
|
How updates are conveyed
What knowledge is conveyed
When the knowledge is conveyed
How to locate recipients of the updates
|
1,2,3,4
|
28
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 060104t SXY Q,0,0,280,319
Which type of routing uses routing update messages?
|
Choose an option.
|
Static routing
Dynamic routing
Default routing
|
2
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.

@@QUES 060105t XYF Q,0,0,335,350
If a router's routing table does not have an entry for a specific destination it can direct packets along  _  route.
|
Choose an option to fill the blank.
|
%010an open
%010a default
%010a dynamic
|
2
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted.
|
The full statement is now shown.



@@QUES 060201t MXY Q,0,0,333,338
Which of the following routing protocols use distance vector routing algorithms?
|
Choose each appropriate item.
|
RIP
OSPF
IGRP
Enhanced IGRP
|
1,3
|
28
|
Correct.
|
7 per correct decision
|
Partly right. The correct options are now highlighted.
|
You have not made any correct choices. The correct options are now highlighted.

@@QUES 060202t DTF Q,0,0,300,297
Convergence occurs more quickly with  _  routing algorithms converge more quickly than  _  routing algorithms.
|
Choose an option to fill the first blank.
|
Choose an option to fill the second blank.
|
%010distance vector
%010link state
|
2
|
Correct.
|
10
|
Incorrect. It's the other way around.
|
0
|
Incorrect.
|
0
|
Incorrect.
|
0
|
The full statement is now shown.

@@QUES 060203t SXY Q,0,0,326,306
Which of the following routing algorithms require the most CPU power and memory?
|
Choose an option.
|
Distance vector
Link state
Balanced hybrid
|
2
|
15
|
Correct.
|
Incorrect. The correct option is now highlighted. 
|
The correct option is now highlighted.

@@QUES 060204t SXY Q,0,0,350,350
Which of the following routing protocols use a balanced hybrid routing algorithm?
|
Choose an option.
|
OSPF
RIP
Enhanced IGRP
IGRP
|
3
|
20
|
Correct.
|
Incorrect. The correct option is now highlighted. 
|
The correct option is now highlighted.
