Chapter 7: Novell IPX Labs:
7.4.3 | In previous labs you have been working with the TCP/IP routed protocol or the Internet Protocol (IP). In this lab you will work with Novell's Internetwork Packet Exchange (IPX) routed protocol. OSI layer 3 protocols such as IP and IPX contain information in their packets to indicate what network the packet came from and what network it is going to.
Threaded Case Studies:
TCS | Threaded Case Study Overview
Overview | Washington Project: IPX Implementation
7.1.3 | Washington Project: IPX Addressing Issues
7.2.2 | Washington Project: IPX Addressing and Encapsulation Types
7.4.2 | Washington Project: Configuring Subinterfaces
Summary | Washington School District Project Task: Configuring Novell IPX
Engineering Journal:
7.1.3 | Engineering Journal: The show ipx interface Command
7.3.1.1 | Engineering Journal: The ipx routing Command
7.3.1.2 | Engineering Journal: The ipx maximum-paths Command
7.3.1.3 | Engineering Journal: Cisco's Enhanced IGRP
7.3.2 | Engineering Journal: Configurable RIP and SAP Update Timers and Packet Sizes
7.5.1 | Engineering Journal: Simple Network Management Protocol