|  | 6.8 | Verifying ACLs
| 6.8.1 | How to verify ACLs and interpret the output

The show ip interface command displays IP interface information and indicates whether any ACLs are set. The show access-lists command displays the contents of all ACLs. By entering the ACL name or number as an option for this command, you can see a specific list. Verifying ACLs
| Lab Activity
| In this lab you will work with Extended ACLs to regulate the traffic that is allowed to pass through the router based on the source and type of traffic. ACLs are an important tool to control which packets and what type of packets should be allowed to pass through a router from one network to another.

| Lab Activity
| This lab is a practice exercise which simulates a real-world example. You will work with multiple Extended Access Control Lists (ACLs) to simulate regulating the traffic that is allowed to pass through multiple routers to various servers and the Internet.