|  | 6.3 | Standard ACLs
| 6.3.2 |
Writing a valid standard ACL command using all available parameters

As you have learned, you use the standard version of the access-list global configuration command to define a standard ACL with a number. This command is used in global configuration command mode. The full syntax of the command is Router(config)# access-list access-list-number {deny | permit} source [source-wildcard ] [log] You use the no form of this command to remove a standard ACL. This is the syntax: Router(config)# no access-list access-list-number The table shows descriptions of the parameters used in this syntax.