|  | 6.5 | Named ACLs
| 6.5.3 | The permit command

You use the permit access-list configuration command to set conditions for a named standard ACL. The full syntax of this command is: permit {source [source-wildcard] | any}[log] You use the no form of this command to remove a condition from an ACL, using the following syntax: no permit {source [source-wildcard]| any} You use this command in access list configuration mode, following the ip access-list command, to define the conditions under which a packet passes the ACL. The following example is for a standard ACL named Internetfilter: ip access-list standard Internetfilter deny 192.5.34.0 0.0.0.255 permit 128.88.0.0 0.0.255.255 permit 36.0.0.0 0.255.255.255 !(Note:all other access implicitly denied) In this example, permit and deny statements have no number, and no removes the specific test from the named ACL: Router(config {std- | ext-}nacl)# {permit | deny} {ip ACL test conditions} {permit | deny} {ip ACL test conditions} no {permit | deny} {ip ACL text conditions} This example activates the IP named ACL on an interface: Router(config-if)# ip access-group {name | 1-199 {in | out}} A configuration output example is shown in the Figure.