|  | 7.5 | Monitoring and Managing an IPX Network
| 7.5.3 |
Writing a valid IOS command sequence for monitoring Novell IPX servers
The show ipx servers command lists the IPX servers discovered through SAP advertisements. The output of the show ipx servers command shows the following information: The service learned about the server from a SAP update The server name, network location, device address, and source socket number The ticks and hops for the route (taken from the routing table) The number of hops (taken from the SAP protocol) The interface through which to reach the server To list the IPX servers discovered through SAP advertisements, use the show ipx servers in user EXEC mode. The full syntax of this command is: show ipx servers [ sorted [name | net | type ]] This example is sample output from the show ipx servers command. The information in the table describes the fields shown in the example.