| Installing the Stealth Mod Chip: Carefully bend back the pins of the chip so that they are flat and even with the chip. Solder the wires to the chip following the diagram below.

For Pre-Wired Stealth Mod Chip Kits here is the Color Coded Diagram for you:

Pin 1: Red | Pin 8: Black
Pin 2: Not Used | Pin 7: Orange
Pin 3: Purple | Pin 6: Yellow
Pin 4: Blue | Pin 5: Green

Check which type of playstation you have by turning the unit upside down and looking at the label. It will say SCPH-XXXX. XXXX= Model #.

Choose your model below for installation information:

SCPH-100x | SCPH-550x | SCPH-700x | SCPH-750x | SCPH-900x