			IBM NetVista N2200w Service Pack 3 CD
                        -------------------------------------

This CD contains the following information:

Client Service Pack 3.0
_______________________
	*  Important installation notes
	*  What's new in SP 3.0
	*  Verifying  if your new system is up-to-date
	*  Installing the client update on your update server
        *  How to customize the installsp3.xml 
	*  Updating your N2200w 

Remote Management Software
__________________________
	*  Remote Device Administrator prerequisites
	*  RDA installation steps
	*  Getting Started with RDA
	*  Update Designer installation
	*  Getting Started with Update Designer
	*  Sample update files

Publications
____________
	*  NetVista N2200w,Thin Client for Windows-based Terminal Standard
	   1.5 Reference Service Pack 3.0
	*  Remote Device Administrator for use with the IBM NetVista N2200w
	   User's Manual
	*  Update Designer for use with the IBM NetVista N2200w User's Manual
	*  Support info on the web



CLIENT SERVICE PACK 3.0
_______________________

Important installation notes


        *When updating an OS image or downloading a configuration, the update file type you
         use is dependent on your version of the NetVista thin client.
		·	For WBT SP 1.1 or earlier, use .XML files.
		·	For WBT SP 2.0 or later use .BUD files.

	*If you are upgrading to Service Pack 3 from Service Pack 1.1 or earlier, you
         will need to use the .XML files at the initial upgrade. After the initial upgrade
         use .BUD files.


	*Use http or ftp as the transport protocol.  If using FTP, the server 
	  MUST support the PASV flag (passive FTP).  Microsoft Internet 
	  Information Server is known to support this flag.

	*Change //update_server to your update server host name or IP address.

	*Change /sp30 to the folder name you used to store the update files.
       
	*If your update server is using http as the transport protocol, ensure 
        that the http server directory permissions for the update directory
	(e.g. sp30) DO NOT have Execute turned on.

What's new in SP 3.0
	What follows is an overview of what is new in Service Pack 2.0.  
	For more detailed and the most up-to-date information,
	visit our website:

	http://www.ibm.com/pc/support
		* Select NetVista, then select NetVista thin client
		* Under Technical Information, click on "Hot News"
		* Select the following document: NetVista N2200w (8363-Wxx)
	 	  - Service packs

	
Citrix ICA v6 client
User Accounts (individual connection lists)
Japanese Keyboard support
NFUSE external viewer support (start the Citrix connection inside a web browser, but not embedded in the web page).
ISP Dial-In
AT Dial Strings


Verifying if your new system is up-to-date
	It is strongly recommended that before you start to configure your
	new N2200w system, first check to see if it is already loaded with 
	the latest WBT software. To do this:
	1.  Go through the Setup Wizard and wait for the system to restart.
	2.  After the system restarts, it will display the Terminal
	    Connection Manager.
	3.  Press <F2> key to activate the Terminal Properties dialog box
	4.  Click on the "System" tab and check the "Build Version 
            Information"
	5.  If the Build Number is 1087_1, your software is already up-to-date 
	    and you can skip software update steps and start configuring and
	    using your system. 
       	    If the Build Number is below 1087_1 or below, you need to update 
	    your system software.

Installing the Client Code on your server
	To update your client software you must first setup an update server:
	1.  Make sure you have a HTTP server or a FTP server, with anonymous
	    login support, as your update server.
	2.  Install the software update package from  the CD  into the
	    appropriate folder on the update server.
	
	The SP3.0 is packaged in the client directory on the CD. You must 
	first copy the contents into a subdirectory accessible by update 
	protocol on your update server.
	For example, if you are using Microsoft IIS with its default HTTP
	root directory, you can create a folder sp30 as follows:
		c:\inetpub\wwwroot\sp30 
	You  then copy  all the files in the client subdirectory into 
	this folder. With this example, the Update URL you  specify on
	your client systems is:
		http://update_server/sp30/installsp3.xml

	Where update_server should be substituted with the actual host name
	or the IP address of the update server. 

	3.  Edit the XML (installsp3.xml) file to reflect your server
	    environment.  You need to modify the update XML files with 
	    the address of the update server.

How to customize the installsp3.xml 
	You need to customize the installsp3.xml file based on:
		The transport protocol you choose to use (http or ftp)
		The server host name/IP address of your update server
		The directory path used to access the files

	installsp3.xml file:

	<?xml version="1.0" encoding="UTF-8"?>
	<!DOCTYPE Package SYSTEM "SoftwareUpdate.dtd">
	<!-- Upgrade to IBM WBT SP30-->
	<Package ID="1087">
	    <CopyFile>
 	      <Description>Copy getconfig.exe</Description>
     	      <Source>http://update_server/sp30/getconfig.exe</Source>
    	      <Destination>getconfig.exe</Destination>
	    </CopyFile>
 	   <Execute WaitForExit="Yes">
        	<Description>Save Current Configuration</Description>
        	<FileName>getconfig.exe</FileName>
     	        <CommandLine> </CommandLine>
 	   </Execute>
	    <CopyFile OSImage="Yes" OSImageSize="0xC50000">
	       <Description>Download Software Update for SP3.0</Description>
 	       <Source>http://update_server/sp30/nk_1087.bin</Source>
 	       <Destination>\Program Files\nk.bin</Destination>
 	   </CopyFile>
  	  <Reboot>Yes</Reboot>
	</Package>


Updating your N2200w
	1.  Press F2 to get into the Terminal Properties.  In the Terminal
	    Properties dialog box, click on the "Update" tab.
	2.  Enter the URL for the update server and update xml file. 
	    (e.g. http://update_server/sp30/installsp3.xml)
	3.  Click on the "Update Now . . . " button.
	4.  The system will restart and begin to update the system software.
	5.  After the update has been completed, the system will restart again.
	6.  After the system come back it will restore the save configuration, 
	    then restart again (you will only see a blank screen with a mouse 
            pointer briefly).
	7.  The system should now have the original configuration restored 
            with the new level of code.



REMOTE MANAGEMENT SOFTWARE
__________________________
	The Remote Device Administrator is a software suite that updates,
	manages, and monitors remote clients. The Remote Device 
	Administrator Server is a set of Active Server Pages that displays
	and updates device information.  The Update Designer is a user 
	interface that creates bud files that contain XML directive which are
	the instructions for remote updates. 
	** Remote Management is NOT supported for modem connected clients. **


Remote Device Administrator Server prerequisites
	Remote device administrator can be installed on either Windows NT 4.0 Server or 	Windows 2000 Server.  The prerequisites for the installation of RDA are:

	Internet Explorer 4.0 or later (included with Windows 2000 Server)
	Enabled SNMP Service
	Internet Information Server 4.0 or later (included with Windows 2000
	server)
	Microsoft MDAC (Microsoft Data Access Components) 2.1 or later 
	(included with 	Windows 2000 Server)	
	WMI (included with Windows 2000 Server)
	WMI SNMP Provider, found at
           http://msdn.microsoft.com/Downloads/sdks/wmi/download.asp

	For NT 4.0 installation prerequisites, you can download the following
	files:
	Internet Information Server is part of the NT Options Pack
	   http://www.microsoft.com/ntworkstation/downloads/Recommended
	   /ServicePacks/NT4OptPk/Default.asp
	Microsoft MDAC (Microsoft Data Access Components) 2.1 (mdac_typ)
	   http://www.microsoft.com/data/download_21242023.htm
	WMI and WMI SNMP Provider (wmint4.exe)
	   http://www.microsoft.com/downloads/release.asp?ReleaseID=18491

RDA installation steps
	The RDA installation steps documented in the Getting Started section
        of the  Remote Device Administrator for use with the IBM NetVista
        N2200w User's Manual show you step by step how to ensure that you
        have the prerequisites installed and configured before installing
        the RDA software.  Please refer to the manual before beginning
        the RDA installation.

Getting Started with RDA
	After installing RDA on your server, you can launch the RDA server 
        or Update Designer from the Start Programs menu.  To view devices 
        that have announced themselves to the server, you can search with
        blank parameters  and view all devices.  Device records only include
        the information which the client includes in the announce to the
        server.  To see all available client information, press the Refresh
        button at the bottom of the view devices screen for the device.  
        Refer to Starting the Remote Device Administrator Server in the 
        RDA User's Manual  or Update Tab in Configuring your Thin Client
        in the N2200w Reference Guide.

Update Designer installation
	Update Designer is typically installed as part of the RDA
        installation, but can be installed separately using the RDA setup
        program and only selecting the Update Designer to be installed.  
        The procedure for installing separately is documented in the RDA 
        User's Manual under Installing Update Designer Only.

Getting Started with Update Designer
	To launch and get started using Update Designer, see Using Update
        Designer in the Update Designer's User Manual.  For the steps to
        create a typical configuration update for a SP 2.0 client using 
        Update Designer, refer to Configuring Multiple Clients in the 
        N2200w Reference Guide.

Sample update files
	Sample .bud files are included on this CD in the \client subdirectory.  
	You can view these files with Update Designer, but you must copy them
	to your hard drive, in order for Update Designer to access them. 
	These files are samples of update files for :

	OS update	
	Internet Explorer Favorites Update
	BootCode Update


Publications
___________
The documents are included in PDF format.  If you do not have Adobe Acrobat Reader installed, the software is included on this CD for your convenience.
	

NetVista N2200w,Thin Client for Windows-based Terminal Standard 1.5 Reference Service Pack 3.0
	Start reading with this publication.  This publication provides an overview of the NetVista N2200w Product. 

Remote Device Administrator for use with the IBM NetVista N2200w User's Manual
	Remote Device Administrator is the remote management utility to be used in combination with Service Pack 3.0.  The included publication documents installation and use of the utility.  

Update Designer for use with the IBM NetVista N2200w User's Manual
	Update Designer is a GUI tool for creating XML files used in updates with the Service Pack 3.0 client software.  The included publication documents installation and use of the utility.  


Support info on the web
	For more detailed and the most up-to-date information, visit our website:

	http://www.ibm.com/pc/support
		* Select NetVista, then select NetVista thin client
		* On the left hand frame under Technical Information, click on "Hot News"
		* Select the following document: NetVista N2200w (8363-Wxx) - Service



Remote Management Limitations
	A complete list of current limitations and workarounds where applicable is available         on the support website.  
	
	Must close Update file (.bud) before client updates
        RDA not supported with IE modem Autodial
        RDA Multiple configurations can have the same name
        RDA: Fields for RDP do not show in connection configuration dialogue on client