# Software and hardware support of RAID levels

RAID level | ServeRAID software* release that supports the RAID level | Hardware levels that support the RAID level
0 | All | ServeRAID on the board, ServeRAID, ServeRAID-II, ServeRAID-3 family, ServeRAID-4 family, ServeRAID-5i.
1 | All | ServeRAID on the board, ServeRAID, ServeRAID-II, ServeRAID-3 family, ServeRAID-4 family, ServeRAID-5i, integrated RAID controller.
1E | All | ServeRAID on the board, ServeRAID, ServeRAID-II, ServeRAID-3 family, ServeRAID-4 family, ServeRAID-5i.
5 | All | ServeRAID on the board, ServeRAID, ServeRAID-II, ServeRAID-3 family, ServeRAID-4 family, ServeRAID-5i.
5E | ServeRAID 3.50 or later | ServeRAID-3 and ServeRAID-4 families.
x0 | ServeRAID 4.00 or later | ServeRAID-4 family and ServeRAID-5i.

* ServeRAID software refers to BIOS, firmware, device drivers, programs, and so forth.

Glossary | Contents

x-1061-SRM-00-03-EN