### Failed to connect to host name [ID] at port number [number].

Explanation: Could not communicate with the ServeRAID Manager on the remote system.

Action:

1. Verify the ServeRAID Manager is running on the remote system.
2. Verify the port number specified for the remote system in the Add remote system window matches the value specified on the remote system by going to the ServeRAID Manager running on that system by doing the following:
   1. Click File --> User preferences.
   2. Click Remote access settings.
   3. Verify the value for the port number.
3. Verify the following:
   1. The remote system is on.
   2. Both the local and remote systems are connected to the network.
   3. TCP/IP networking support is configured on both the local and remote systems.
   4. The network is functioning.
4. If you are trying to connect to a remote system that has multiple network cards, you must use a host name to connect to the system.