## Confirming your system configuration

1. Review the configuration in the right panel. It describes the new logical drives that the ServeRAID Manager will define when you click Apply. Additional notes and attentions regarding the configuration appear in the event viewer.

   Tip: You can expand the tree for another view of the configuration.

2. If you want to modify the configuration:

   - To modify arrays or hot-spare drives, click Modify arrays.

   - To modify logical drives, click Modify logical drives.

3. Click Apply when you are satisfied with the configuration.

4. Click Yes when the confirm pop-up window opens. If your firmware supports it, the ServeRAID Manager will start the synchronization process automatically. Your logical drives will always be initialized automatically.

   Note: If you have disabled automatic initialization, the ServeRAID Manager will not initialize the logical drives automatically.