2/7/2005


The NVSRAM in this folder is for the DS4300 storage server configurations 
with either the DS4300 storage server by itself or the DS4300 storage 
server with Fibre Channel drive expansion enclosures only attached. This 
is not the correct NVSRAM file for the DS4300 storage servers with the 
FC/SATA intermix premium feature, which will enable the support of the 
EXP700/ EXP710 and the EXP100 drive expansion enclosures behind a DS4300 
storage server. Please refer to the CD that is shipped with the FC/SATA 
intermix entitlement for the correct NVSRAM file for the DS4300 storage 
server with FC/SATA intermix premium feature. The maximum of drive 
axpansion enclosures that can be connected to the DS4300 storage server 
with this NVSRAM file installed is 7. 


In addition, this is also not the correct NVSRAM file for the DS4300 
storage server configurations that have only (up to eight) EXP100 drive 
expansion enclosures attached. Please refer to the NVSRAM file named 
N1722F600R18enc1.dlp in the "For_attachment_of_EXP100(SATA)_enclosures_only"
directory in this web-posting firmware package, instead.


Please contact IBM support for more information, if required.
  
  
Note: The FC/SATA drive type intermixing behind a DS4000 storage server 
requires the purchase of the FC/SATA intermix premium feature entitlement. 
Please contact your IBM resellers or representatives for more information.

