From: G7MRI


  Well guys i see that many people have been looking for mods for
  this radio so here is the out of band tx mod.


1. take off bottom and top covers.
2. connect a jumper from point TP2003 to ground. this is temporary
while preforming the programming steps. that point is in front and to
the edge of the lithium battery.
3. with the ft-840 off, press and hold the (SSB) & (AM) buttons at the
same time. turn on the rig, then release the buttons simultaneously.

4. the display  will show (02-ON). press the (AM) button to confirm
setting: it should read 7.000.00 LSB. turn rig off.
( If the rig does not show 02-on move the main freq knob to change it)

5. press and hold in the MEM , (DOWN) and (UP) buttons while turning
rig "on".
6. turn pwr off, and remove jumper.
7. if you have a problem, dump the backup memory by switching the back
up switch off per the manual.you can then redo the steps.

If you know of any mods please let me know and if you can find out what
01-ON/OFF   to   09-ON/OFF i think it goes to, what do the other settings do.

                          73's de John
                          G7MRI@GB7LWB.#27.GBR.EU
