#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8001 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage Systems Fan: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Storage Systems fan status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8001 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage Systems Fan: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage Systems fan status is OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8001 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage Systems Fan: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage Systems fan has FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8001 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage Systems Fan: NO FAN'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage Systems status: NO FAN'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8001 * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Storage Systems Fan: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage Systems fan status: DEGRADED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8002 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8002 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature status: OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8002 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature status: DEGRADED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8002 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature has FAILED and will shutdown'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8002 * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature status is NOT SUPPORTED'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8003 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature status is: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8003 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature is OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8003 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature status has DEGRADED and may shutdown'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8003 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature has FAILED and will shutdown'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8003 * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature status is NOT SUPPORTED'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8004 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status normal operating range: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='A HP - Storage System temperature status is: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8004 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='A HP - Storage System temperature is OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8004 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='A HP - Storage System temperature status has DEGRADED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8004 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature has FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8004 * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System temperature status is NOT SUPPORTED'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8005 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System side panel status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Storage System side panel has a status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8005 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System side panel status: SIDE PANEL IN PLACE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System SIDE PANEL IN PLACE'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8005 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System side panel status: SIDE PANEL REMOVED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System side panel has been REMOVED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8005 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System side panel status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System side panel is NOT SUPPORTED'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8006 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System side panel removed status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Storage System side panel has a status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8006 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System side panel removed status: SIDE PANEL IN PLACE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System SIDE PANEL IN PLACE'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8006 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System side panel removed status: SIDE PANEL REMOVED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System SIDE PANEL HAS BEEN REMOVED, improper cooling of drives may result'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8006 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System side panel removed status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Storage System side panel is NOT SUPPORTED'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8007*'
       MSGNODE=*
       DEScription='HP - Storage Systems power supply status'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage Systems power supply has become degraded'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
