DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10510 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SAL failed to clear the CEC logs during Machine check handling.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SAL failed to clear the CEC logs during Machine check handling.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Sal failed to clear the CEC logs during Machine check handling. The data field return an ASCII name of the CEC that failed to clear.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10516 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System FW was unable to access the XBC semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System FW was unable to access the XBC semaphore.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while getting the XBC semaphore.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10518 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System Firmware detected an error while trying to release the XBC Global Semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System Firmware detected an error while trying to release the XBC Global Semaphore.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while releasing the XBC Global Semaphore.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10519 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event System Firmware detected an Error while checking the owner of the XBC Global Semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event System Firmware detected an Error while checking the owner of the XBC Global Semaphore.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while checking the owner of the XBC Global Semaphore.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10520 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event An error occurred while forming the XBC semaphore address'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event An error occurred while forming the XBC semaphore address: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='An error occurred while forming the XBC semaphore address. Data Field: (xbc << 32) | (cell << 56)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10521 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error reading the XBC Global Semaphore'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error reading the XBC Global Semaphore: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error reading the XBC Global Semaphore. Data Field: (cell num << 56) | (xbc << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10523 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failure to get the XBC Global Semaphore address'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failure to get the XBC Global Semaphore address: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failure to get the XBC Global Semaphore address. Data Field: (cell num << 56) | (xbc << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10524 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to write the XBC Global Semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to write the XBC Global Semaphore.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to write the XBC Global Semaphore. Data Field: (cell num << 56) | (xbc << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10528 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to read the XBC Global Semaphore'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to read the XBC Global Semaphore: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to read the XBC Global Semaphore. Data Field: (cell num << 56) | (xbc << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10529 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to get the address of the XBC Global Semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to get the address of the XBC Global Semaphore.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to get the address of the XBC Global Semaphore. Data Field: (cell num << 56) | (xbc << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10530 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to write the XBC Global Semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to write the XBC Global Semaphore.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to write the XBC Global Semaphore. Data Field: (cell num << 56) | (xbc << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10532 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to release the XBC Global Semaphore.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to release the XBC Global Semaphore.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to release the XBC Global Semaphore. Data Field: (cell num << 56) | (xbc << 32)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10534 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fabric phases have been executed in an invalid order.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fabric phases have been executed in an invalid order.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Fabric phases have been executed in an invalid order'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10535 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Fabric phases have been executed in an invalid order. Data field indicates the expected phase.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Fabric phases have been executed in an invalid order. Data field indicates the expected phase.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Fabric phases have been executed in an invalid order. Data field indicates the expected phase.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10558 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to get an address when opening XBC to XBC links.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to get an address when opening XBC to XBC links.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to get an address when opening XBC to XBC links. Data field is return value from GetAlbAddrBlk function. Internal debug only.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10559 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to open a fabric link.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to open a fabric link.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Failed to open a fabric link. Data field: [31:0] - error status from OpenFabricLink [39:32] - XBC ID [51:44] - XBC port number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10560 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error when writing the XBC return route.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error when writing the XBC return route.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error when writing the XBC return route. Data field: [31:0] - error status from WriteRouteReg [39:32] - XBC ID [51:44] - XBC port number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10561 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error enabling the XBC return route'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error enabling the XBC return route: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error enabling the XBC return route. Data field: [31:0] - error status from WriteRouteEnable [39:32] - XBC ID [51:44] - XBC port number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10564 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Failed to disperse the routes across links.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Failed to disperse the routes across links.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='failed to disperse the routes across links. Data field: [31:0] - error status from GetDispersedOutboundPort [39:32] - XBC ID [51:44] - XBC port number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10565 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error setting up XBC-XBC link for routing across it.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error setting up XBC-XBC link for routing across it.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error setting up XBC-XBC link for routing across it. Data field: [31:0] - error status from SetupXbcToXbcLinks [39:32] - XBC ID [51:44] - XBC port number '

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10566 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error while routing the remote side of a route.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error while routing the remote side of a route.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error while routing the remote side of a route. Data field: [31:0] - error status from RouteRemoteXbcPort [39:32] - XBC ID [51:44] - XBC port number [59:52] - Destination cell number:'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10567 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error getting address while routing the remote XBC.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error getting address while routing the remote XBC.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error getting address while routing the remote XBC. Data field: [31:0] - error status from GetAlbAddrBlk [39:32] - XBC ID [51:44] - XBC port number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10568 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error geting the neighbor info.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error geting the neighbor info.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error geting the neighbor info. Data field: [31:0] - error status from AlbGetNeighborInfo [39:32] - XBC ID [51:44] - XBC port number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10569 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error finding the shortest route'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error finding the shortest route: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error finding the shortest route. Most likely a firmware error or data corruption. Data field: [31:0] - error status from VM_FindShortestRoute [39:32] - Destination XBC ID [59:52] - Destination Cell number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10570 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error writing the remote XBC routing register.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error writing the remote XBC routing register.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error writing the remote XBC routing register. Data field: [31:0] - error status from WriteRouteReg [39:32] - XBC ID [51:44] - XBC port number [59:52] - Destination cell number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10571 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error enabling the routes on the remote XBC.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error enabling the routes on the remote XBC.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='error enabling the routes on the remote XBC. Data field: [31:0] - error status from WriteRouteEnable [39:32] - XBC ID [51:44] - XBC port number [59:52] - Destination cell number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10572 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error writing the routing register on the local XBC.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error writing the routing register on the local XBC.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error writing the routing register on the local XBC. Data field: [31:0] - error status from WriteRouteReg [39:32] - XBC ID [51:44] - XBC port number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10573 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error writing the local XBC routing registers to reach a remote cell.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error writing the local XBC routing registers to reach a remote cell.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error writing the local XBC routing registers to reach a remote cell. Data field: [31:0] - error status from WriteRouteReg [39:32] - XBC ID [51:44] - XBC port number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10574 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Error enabling the local XBC routes.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Error enabling the local XBC routes.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Error enabling the local XBC routes. Data field: [31:0] - error status from WriteRouteEnable [39:32] - XBC ID [51:44] - XBC port number'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10617 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event SynchGraphs() failed during Arches Fabric Phase 4. Data field: return value from SynchGraphs().'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event SynchGraphs() failed during Arches Fabric Phase 4. Data field: return value from SynchGraphs().: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='SynchGraphs() failed during Arches Fabric Phase 4. Data field: return value from SynchGraphs()'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10619 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event VM_DeleteVertex() failed in SynchGraphs(). Data field: (vertex id 32) | (vertex type 56) | (return value from VM_DeleteVertex()).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event VM_DeleteVertex() failed in SynchGraphs(). Data field: (vertex id 32) | (vertex type 56) | (return value from VM_DeleteVertex()).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='VM_DeleteVertex() failed in SynchGraphs(). Data field: (vertex id << 32) | (vertex type << 56) | (return value from VM_DeleteVertex())'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10620 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event VM_DeleteEdge() failed in the Arches Fabric function SynchGraphs(). Data field:(vertex id1 32) | (vertex port1 48) | (vertex type1 56) | (vertex id2 0) | (vertex port2 16) | (vertex type2 24).'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event VM_DeleteEdge() failed in the Arches Fabric function SynchGraphs(). Data field:(vertex id1 32) | (vertex port1 48) | (vertex type1 56) | (vertex id2 0) | (vertex port2 16) | (vertex type2 24).: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='VM_DeleteEdge() failed in the Arches Fabric function SynchGraphs(). Data field:(vertex id1 << 32) | (vertex port1 << 48) | (vertex type1 << 56) | (vertex id2 << 0) | (vertex port2 << 16) | (vertex type2 << 24)'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10621 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected error when calling an Arches Fabric vertex module function. Data field: return value from vertex module function.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected error when calling an Arches Fabric vertex module function. Data field: return value from vertex module function.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unexpected error when calling an Arches Fabric vertex module function. Data field: return value from vertex module function'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10622 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Unexpected return from an Arches Fabric vertex module function while copying a cell s graph. Data field: return value from vertex module function.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Unexpected return from an Arches Fabric vertex module function while copying a cell s graph. Data field: return value from vertex module function.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Unexpected return from an Arches Fabric vertex module function while copying a cell s graph. Data field: return value from vertex module function'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10623 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The checksum update for the PDT has failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The checksum update for the PDT has failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The checksum update for the PDT has failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10625 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The checksum in the memory area of NVM is bad.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The checksum in the memory area of NVM is bad.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The checksum in the memory area of NVM is bad. Memory NVM will be cleared.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10626 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Checksum calculation failed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Checksum calculation failed.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Checksum calculation failed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10628 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Both SAL s copy and BMC copy of the token specified in the data field is bad.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Both SAL s copy and BMC copy of the token specified in the data field is bad.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The BMC copy and SAL copy of the token specified in the data field has been initialized from the default value for the token due to an IPMI error and SAL NVM error.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10629 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event Incompatible I/O Backplane or I/O cables installed.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event Incompatible I/O Backplane or I/O cables installed.: &(16:)'
        SEVERITY=E
        ATTRIB=default
        COLOR=red
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='Detected incompatibility between the cell board and the I/O backplane and/or I/O backplane cables.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *11 * * 6 10698 * * * 1.3.6.1.4.1.11.2.23.35.1*'
        MSGNODE=*
        DEScription='HP - Integrity Event The fPar identified by the event detail will be unusable.'
        TYPE=MSG
DEFine MSGACTion NAME=(*,10)
        ACTION=sendkeep TEXT='HP - Integrity Event The fPar identified by the event detail will be unusable.: &(16:)'
        SEVERITY=W
        ATTRIB=default
        COLOR=orange
DEFine MSGACTion Name=(*,20)
        ACTION=ANNOTATE TEXT='The fPar identified by the event detail will be unusable. Other events may preceed this event which will help to diagnose the failure. A possible cause is that the system exhausted unused NVRAM.'

