#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6041 * * * * * * * * * * * * * * * * 2 * * * * * * * * * 10*'
       MSGNODE=*
       DEScription='HP - Temperature: DEGRADED (Action: Continue - Location: Power Supply)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: DEGRADED (Action: Continue - Location: Power Supply)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6041 * * * * * * * * * * * * * * * * 3 * * * * * * * * * 10*'
       MSGNODE=*
       DEScription='HP - Temperature: DEGRADED (Action: Shutdown - Location: Power Supply)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: DEGRADED (Action: Shutdown - Location: Power Supply)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6041 * * * * * * * * * * * * * * * * 1 * * * * * * * * * 11*'
       MSGNODE=*
       DEScription='HP - Temperature: DEGRADED (Action: Other - Location: Ambient)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: DEGRADED (Action: Other - Location: Ambient)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6041 * * * * * * * * * * * * * * * * 2 * * * * * * * * * 11*'
       MSGNODE=*
       DEScription='HP - Temperature: DEGRADED (Action: Continue - Location: Ambient)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: DEGRADED (Action: Continue - Location: Ambient)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6041 * * * * * * * * * * * * * * * * 3 * * * * * * * * * 11*'
       MSGNODE=*
       DEScription='HP - Temperature: DEGRADED (Action: Shutdown - Location: Ambient)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: DEGRADED (Action: Shutdown - Location: Ambient)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6041 * * * * * * * * * * * * * * * * 1 * * * * * * * * * 12*'
       MSGNODE=*
       DEScription='HP - Temperature: DEGRADED (Action: Other - Location: Chassis)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: DEGRADED (Action: Other - Location: Chassis)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6041 * * * * * * * * * * * * * * * * 2 * * * * * * * * * 12*'
       MSGNODE=*
       DEScription='HP - Temperature: DEGRADED (Action: Continue - Location: Chassis)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: DEGRADED (Action: Continue - Location: Chassis)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6041 * * * * * * * * * * * * * * * * 3 * * * * * * * * * 12*'
       MSGNODE=*
       DEScription='HP - Temperature: DEGRADED (Action: Shutdown - Location: Chassis)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: DEGRADED (Action: Shutdown - Location: Chassis)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6041 * * * * * * * * * * * * * * * * 1 * * * * * * * * * 13*'
       MSGNODE=*
       DEScription='HP - Temperature: DEGRADED (Action: Other - Location: Bridge Card)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: DEGRADED (Action: Other - Location: Bridge Card)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6041 * * * * * * * * * * * * * * * * 2 * * * * * * * * * 13*'
       MSGNODE=*
       DEScription='HP - Temperature: DEGRADED (Action: Continue - Location: Bridge Card)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: DEGRADED (Action: Continue - Location: Bridge Card)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6041 * * * * * * * * * * * * * * * * 3 * * * * * * * * * 13*'
       MSGNODE=*
       DEScription='HP - Temperature: DEGRADED (Action: Shutdown - Location: Bridge Card)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Temperature Status: DEGRADED (Action: Shutdown - Location: Bridge Card)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042*'
       MSGNODE=*
       DEScription='HP - Temperature: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location Other)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: Other)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location Unknown)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: Unknown)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location: System)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: System)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location: System Board)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: System Board)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location: IO Board)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: IO Board)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location: CPU)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: CPU)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 7*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location: Memory)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: Memory)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 8*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location: Storage)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: Storage)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 9*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location: Removable Media)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: Removable Media)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 10*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location: Power Supply)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: Power Supply)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 11*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location: Ambient)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: Ambient)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 12*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location: Chassis)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: Chassis)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6042 * * * * * * * * * * * * * * * * * * * * * 13*'
       MSGNODE=*
       DEScription='HP - Temperature OK (Location: Bridge Card)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Temperature Status: OK (Location: Bridge Card)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
