#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************
#
# StorageWorks Enterprise Array Manager (STEAM) Management Information Base (MIB)
#

#---------------------------------------------------------------
# STEAM trap ID 1 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 1 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Disk Drive Failure'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Disk Drive Failure. Consult the original alarm for more information.'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A disk device has failed. The original trap contains the following variable information: HostName, SubsysName, DiskName, CabinetNumber, DiskPort, and DiskTarget.'


#---------------------------------------------------------------
# STEAM trap ID 2 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 2 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Disk Drive Recovered'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Disk Drive Recovered. Consult the original alarm for more information.'
       SEVERITY=Sx
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A disk device has recovered. The original trap contains the following variable information: HostName, SubsysName, DiskName, CabinetNumber, DiskPort, and DiskTarget.'

#---------------------------------------------------------------
# STEAM trap ID 3 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 3 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Power Supply Device Failure'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Power Supply Device Failure. Consult the original alarm for more information.'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The original trap contains the following variable information: HostName, SubsysName, CabinetNumber, and PowerSupplyLocation.'

#---------------------------------------------------------------
# STEAM trap ID 4 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 4 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Power Supply Recovered'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Power Supply Recovered. Consult the original alarm for more information.'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The power supply in the specified location has gone from bad to good. The original trap contains the following variable information: HostName, SubsysName, CabinetNumber, and PowerSupplyLocation.'


#---------------------------------------------------------------
# STEAM trap ID 5 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 5 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Fan Failure'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Fan Failure. Consult the original alarm for more information.'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The original trap contains the following variable information: HostName, SubsysName, CabinetNumber, and FanLocation.'

#---------------------------------------------------------------
# STEAM trap ID 6 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 6 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Fan Recovered'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Fan Recovered. Consult the original alarm for more information.'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The original trap contains the following variable information: HostName, SubsysName, CabinetNumber, and FanLocation.'


#---------------------------------------------------------------
# STEAM trap ID 7 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 7 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Cache Battery Failure'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Cache Battery Failure. Consult the original alarm for more information.'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The cache battery in specified location has failed. Replace cache battery or replenish charge. The original trap contains the following variable information: HostName, SubsysName, and CacheBatteryLocation.'


#---------------------------------------------------------------
# STEAM trap ID 8 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 8 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Cache Battery Low'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Cache Battery Low. Consult the original alarm for more information.'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The cache battery in specified location has LOW state. Replace cache battery or replenish charge. The original trap contains the following variable information: HostName, SubsysName, and CacheBatteryLocation.'


#---------------------------------------------------------------
# STEAM trap ID 9 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 9 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Cache Battery OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Cache Battery OK. Consult the original alarm for more information.'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The cache battery in the specified location has a good state. The original trap contains the following variable information: HostName, SubsysName, and CacheBatteryLocation.'

#---------------------------------------------------------------
# STEAM trap ID 10 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 10 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Temperature Over Threshold: Warning'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Temperature Over Threshold: Warning. Consult the original alarm for more information.'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The temperature sensor in the specified location has exceeded WARNING threshold limit. Lower environmental temperature or raise internal threshold limit depending upon application.'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The original trap contains the following variable information: HostName, SubsysName, CabinetNumber and TemperatureSensorLocation.'

#---------------------------------------------------------------
# STEAM trap ID 11 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 11 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Temperature Threshold Ok'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Temperature Threshold Ok. Consult the original alarm for more information.'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The temperature sensor in the specified location indicates below WARNING threshold limit. The original trap contains the following variable information: HostName, SubsysName, CabinetNumber and TemperatureSensorLocation.'


#---------------------------------------------------------------
# STEAM trap ID 12 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 12 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Communication Failure'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Communication Failure. Consult the original alarm for more information.'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='Communication with the subsystem has failed. Possible causes are data path interruption, communication LUN failure, 2 or more power supplies failed, 2 or more fans failed, temperature overlimit, or both controllers failed.'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The original trap contains the following variable information: HostName and SubsysName.'

#---------------------------------------------------------------
# STEAM trap ID 13 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 13 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Communication Recovered'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Communication Recovered. Consult the original alarm for more information.'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='Communication with the subsystem has recovered. The original trap contains the following variable information: HostName and SubsysName.'


#---------------------------------------------------------------
# STEAM trap ID 14 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 14 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Secondary Controller Failure'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Secondary Controller Failure. Consult the original alarm for more information.'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The Secondary Controller in the subsytem has failed. Possible causes are PCMCIA memory card ejected, controller physically removed, or actual hardware failure. The original trap contains the following variable information: HostName and SubsysName.'

#---------------------------------------------------------------
# STEAM trap ID 15 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 15 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Secondary Controller Recovered'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Controller Recovered. Consult the original alarm for more information.'
       SEVERITY=S
       ATTRIB=default
       COLOR=green


#---------------------------------------------------------------
# STEAM trap ID 16 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 16 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM LUN Failure'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM LUN Failure. Consult the original alarm for more information.'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The LUN has failed and is off-line. Possible cause is too many failed disk drives that make up the LUN or the OS can no longer communicate with the LUN for other reasons.'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The original trap contains the following variable information: HostName, SubsysName, and LunName.'


#---------------------------------------------------------------
# STEAM trap ID 17 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 17 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM LUN Reconstruction'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM LUN Reconstruction. Consult the original alarm for more information.'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The LUN has started the reconstruction process but is available for normal use. The original trap contains the following variable information: HostName, SubsysName, and LunName.'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='Possible causes are an available disk drive was created as a spare to be inserted into the set or an existing spare was automatically added to the set for reconstruction upon failure of a member disk device.'


#---------------------------------------------------------------
# STEAM trap ID 18 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 18 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM LUN Reduced'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM LUN Reduced. Consult the original alarm for more information.'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A LUN has become degraded due to a member disk device failure. Replace the failed disk device; add a spare to the system to cause a reconstruct. The original trap contains the following variable information: HostName, SubsysName, and LunName.'



#---------------------------------------------------------------
# STEAM trap ID 19 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 19 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM LUN Ok'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM LUN Ok. Consult the original alarm for more information.'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='A LUN has become optimal due to a successful completion of the reconstruction process. The original trap contains the following variable information: HostName, SubsysName, and LunName.'


#---------------------------------------------------------------
# STEAM trap ID 20 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 20 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM External Input Failure'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM External Input Failure. Consult the original alarm for more information.'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The user-defined External Input to the EMU indicates a failure. If the state is FAILURE, then one of the user-defined external input devices is reporting a problem.'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The original trap contains the following variable information: HostName, SubsysName, and CabinetNumber.'


#---------------------------------------------------------------
# STEAM trap ID 21 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 21 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM External Input Recovery'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM External Input Recovery. Consult the original alarm for more information.'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The user-defined External Input to the EMU indicates a recovery. The original trap contains the following variable information: HostName, SubsysName, and CabinetNumber.'

#---------------------------------------------------------------
# STEAM trap ID 22 from 1.3.6.1.4.1.36 enterprise
#---------------------------------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *36 * * 6 22 * * * 1.3.6.1.4.1.36.2.15.21.1.4*'
       MSGNODE=*
       DEScription='HP - STEAM Cache Battery State Unknown'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - STEAM Cache Battery State Unknown. Consult the original alarm for more information.'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The original trap contains the following variable information: HostName, SubsysName, and CacheBatteryLocation.'

