#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2005 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

# New alarms for version 7.40 of the HP Management Agents


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5022*'
       MSGNODE=*
       DEScription='HP - SAS/SATA Physical Drive Status Change (5022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Physical Drive Status Change (TrapData: &(26:))'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - SAS/SATA Physical Drive Status Change (5022): Other'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Physical Drive Status Other (HBA Location: &26 &27, Drive Location: &32 &33 &34 &35 &36, HBA: &41, Drive: &46, Type: &56, Model: &61 &62, Firmware: &67, S/N: &72, SAS Address: &77)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - SAS/SATA Physical Drive Status Change (5022): OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Physical Drive Status Ok (HBA Location: &26 &27, Drive Location: &32 &33 &34 &35 &36, HBA: &41, Drive: &46, Type: &56, Model: &61 &62, Firmware: &67, S/N: &72, SAS Address: &77)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - SAS/SATA Physical Drive Status Change (5022): PREDICTIVE FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Physical Drive Status PredictiveFailure (HBA Location: &26 &27, Drive Location: &32 &33 &34 &35 &36, HBA: &41, Drive: &46, Type: &56, Model: &61 &62, Firmware: &67, S/N: &72, SAS Address: &77)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Indicates that the physical drive has exceeded a threshold value for one of the predictive indicators. When convenient, you should bring down the server and run diagnostics to help identify the problem. The drive may need to be replaced.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - SAS/SATA Physical Drive Status Change (5022): OFFLINE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Physical Drive Status Offline (HBA Location: &26 &27, Drive Location: &32 &33 &34 &35 &36, HBA: &41, Drive: &46, Type: &56, Model: &61 &62, Firmware: &67, S/N: &72, SAS Address: &77)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Indicates that the physical drive is offline and can no longer return data.  No further status is available.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - SAS/SATA Physical Drive Status Change (5022): FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Physical Drive Status Failed (HBA Location: &26 &27, Drive Location: &32 &33 &34 &35 &36, HBA: &41, Drive: &46, Type: &56, Model: &61 &62, Firmware: &67, S/N: &72, SAS Address: &77)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Indicates that the physical drive has failed and can no longer return data.  When convenient, you should bring down the server and run diagnostics to help identify the problem. The drive may need to be replaced.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - SAS/SATA Physical Drive Status Change (5022): MISSING WAS OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Physical Drive Status MissingWasOK (HBA Location: &26 &27, Drive Location: &32 &33 &34 &35 &36, HBA: &41, Drive: &46, Type: &56, Model: &61 &62, Firmware: &67, S/N: &72, SAS Address: &77)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Indicates that a physical drive had a status of OK and is no longer present.  The drive has been removed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 7*'
       MSGNODE=*
       DEScription='HP - SAS/SATA Physical Drive Status Change (5022): MISSING WAS PREDICTIVE FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Physical Drive Status MissingWasPredictiveFailure (HBA Location: &26 &27, Drive Location: &32 &33 &34 &35 &36, HBA: &41, Drive: &46, Type: &56, Model: &61 &62, Firmware: &67, S/N: &72, SAS Address: &77)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Indicates that a physical drive had a status of PREDICTIVE FAILURE and is no longer present.  The drive has been removed.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 8*'
       MSGNODE=*
       DEScription='HP - SAS/SATA Physical Drive Status Change (5022): MISSING WAS OFFLINE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Physical Drive Status MissingWasOffline (HBA Location: &26 &27, Drive Location: &32 &33 &34 &35 &36, HBA: &41, Drive: &46, Type: &56, Model: &61 &62, Firmware: &67, S/N: &72, SAS Address: &77)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Indicates that a physical drive had a status of OFFLINE and is no longer present.  The drive has been removed.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 9*'
       MSGNODE=*
       DEScription='HP - SAS/SATA Physical Drive Status Change (5022): MISSING WAS FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Physical Drive Status MissingWasFailed (HBA Location: &26 &27, Drive Location: &32 &33 &34 &35 &36, HBA: &41, Drive: &46, Type: &56, Model: &61 &62, Firmware: &67, S/N: &72, SAS Address: &77)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='Indicates that a physical drive had a status of FAILED and is no longer present.  The drive has been removed.'






DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5023*'
       MSGNODE=*
DEScription='HP - SAS/SATA Logical Drive Status Change (5023)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Logical Drive Status Change (TrapData: &(26:))'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
DEScription='HP - SAS/SATA Logical Drive Status Change (5023): OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Logical Drive Status Change: OTHER (HBA Location: &26 &27, HBA Index: &32, Drive Index: &37, OS Name: &47)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The management agent does not recognize the status. You may need to upgrade your software.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
DEScription='HP - SAS/SATA Logical Drive Status Change (5023): OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Logical Drive Status Change: OK (HBA Location: &26 &27, HBA Index: &32, Drive Index: &37, OS Name: &47)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
DEScription='HP - SAS/SATA Logical Drive Status Change (5023): DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Logical Drive Status Change: DEGRADED (HBA Location: &26 &27, HBA Index: &32, Drive Index: &37, OS Name: &47)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
DEScription='HP - SAS/SATA Logical Drive Status Change (5023): REBUILDING'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Logical Drive Status Change: REBUILDING (HBA Location: &26 &27, HBA Index: &32, Drive Index: &37, OS Name: &47)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This alarm indicates that the logical drive is currently resynchronizing the data accross the physical drives in the logical drive.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
DEScription='HP - SAS/SATA Logical Drive Status Change (5023): FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SAS/SATA Logical Drive Status Change: FAILED (HBA Location: &26 &27, HBA Index: &32, Drive Index: &37, OS Name: &47)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This alarm indicates that more physical drives have failed than the fault tolerance mode of the logical drive can handle without data loss.'









