#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5001 * * * * * * 1*'
       MSGNODE=*                     
       DEScription='HP - SCSI Drive Controller Status(v2.0): OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - SCSI Drive Controller Status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5001 * * * * * * 2*'
       MSGNODE=*
DEScription='HP - SCSI Drive Controller Status(v2.0): OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SCSI Drive Controller Status: OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5001 * * * * * * 3*'
       MSGNODE=*
DEScription='HP - SCSI Drive Controller Status(v2.0): FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SCSI Drive Controller Status: FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5002 * * * * * * 1*'
       MSGNODE=*
DEScription='HP - Logical SCSI Drive Status(v2.0): OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Logical SCSI Drive Status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5002 * * * * * * 2*'
       MSGNODE=*
DEScription='HP - Logical SCSI Drive Status(v2.0): OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Logical SCSI Drive Status: OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5002 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Logical SCSI Drive Status(v2.0): FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Logical SCSI Drive Status: FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5002 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Logical SCSI Drive Status(v2.0): UNCONFIGURED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Logical SCSI Drive Status: UNCONFIGURED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5002 * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Logical SCSI Drive Status(v2.0): RECOVERING'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Logical SCSI Drive Status: RECOVERING'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5002 * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - Logical SCSI Drive Status(v2.0): READY FOR REBUILD'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Logical SCSI Drive Status: READY TO REBUILD'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5002 * * * * * * 7*'
       MSGNODE=*
       DEScription='HP - Logical SCSI Drive Status(v2.0): REBUILDING'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Logical SCSI Drive Status: REBUILDING'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5002 * * * * * * 8*'
       MSGNODE=*
       DEScription='HP - Logical SCSI Drive Status(v2.0): WRONG DRIVE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Logical SCSI Drive Status: WRONG DRIVE'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5002 * * * * * * 9*'
       MSGNODE=*
       DEScription='HP - Logical SCSI Drive Status(v2.0): BAD CONNECTION'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Logical SCSI Drive Status: BAD CONNECTION'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5003 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Physical SCSI Drive Status(v2.0): OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Physical SCSI Drive Status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5003 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Physical SCSI Drive Status(v2.0): OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Physical SCSI Drive Status: OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5003 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Physical SCSI Drive Status(v2.0): FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical SCSI Drive Status: FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5003 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Physical SCSI Drive Status(v2.0): NOT CONFIGURED '
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical SCSI Drive Status: NOT CONFIGURED'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5003 * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Physical SCSI Drive Status(v2.0): BAD CABLE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical SCSI Drive Status: BAD CABLE'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5003 * * * * * * 6*'
       MSGNODE=*
       DEScription='HP - Physical SCSI Drive Status(v2.0): MISSING WAS OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical SCSI Drive Status: MISSING WAS OK'
       SEVERITY=E
       ATTRIB=default
       COLOR=RED

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5003 * * * * * * 7*'
       MSGNODE=*
       DEScription='HP - Physical SCSI Drive Status(v2.0): MISSING WAS FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical SCSI Drive Status: MISSING WAS FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5003 * * * * * * 8*'
       MSGNODE=*
       DEScription='HP - Physical SCSI Drive Status(v2.0): PREDICTIVE FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical SCSI Drive Status: PREDICTIVE FAILURE'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5003 * * * * * * 9*'
       MSGNODE=*
       DEScription='HP - Physical SCSI Drive Status(v2.0): MISSING WAS PREDICTIVE FAILURE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical SCSI Drive Status: MISSING WAS PREDICTIVE FAILURE'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5003 * * * * * * 10*'
       MSGNODE=*
       DEScription='HP - Physical SCSI Drive Status(v2.0): OFFLINE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical SCSI Drive Status: OFFLINE'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5003 * * * * * * 11*'
       MSGNODE=*
       DEScription='HP - Physical SCSI Drive Status(v2.0): MISSING WAS OFFLINE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Physical SCSI Drive Status: MISSING WAS OFFLINE'
       SEVERITY=E
       ATTRIB=default
       COLOR=RED

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5004 * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - SCSI Tape Drive Status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - SCSI Tape Drive Status: OTHER'
       SEVERITY=I
       ATTRIB=DEFAULT
       COLOR=BLUE

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5004 * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - SCSI Tape Drive Status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - SCSI Tape Drive Status: OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5004 * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - SCSI Tape Drive Status: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SCSI Tape Drive Status: DEGRADED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5004 * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - SCSI Tape Drive Status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SCSI Tape Drive Status: FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5005 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - SCSI Drive Controller: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - SCSI Drive Controller Status: OTHER'
       SEVERITY=I
       ATTRIB=DEFAULT
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5005 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - SCSI Drive Controller: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - SCSI Drive Controller Status: OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5005 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*              
       DEScription='HP - SCSI Drive Controller: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - SCSI Drive Controller Status: FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
