#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

#
# Rack trap 22001 - Rack Name Changed
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22001*'
       MSGNODE=*
       DEScription='HP - Rack Name has changed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack name has changed to &26 (RackUID: &31, RackSN: &36, SeqNum: &41)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an agent or utility has changed the name of the rack.  Each of the server blades in each of the enclosure within the rack will be updated to reflect the new rack name.'
#
# Rack trap 22001 without RackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22001 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Name has changed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack name has changed to &26.'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an agent or utility has changed the name of the rack.  Each of the server blades in each of the enclosure within the rack will be updated to reflect the new rack name.'


#
# Rack trap 22002 - Enclosure Name Changed
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22002*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Name has changed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure name changed. (Enclosure: &36, Rack: &26, RackUID: &31, Enc SN: &41, Enc Model: &46 &47 &48, Enc Spare: &53, SeqNum: &58)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an agent or utility has changed the name of an enclosure within the rack. Each of the components within the rack will be updated to reflect the new enclosure name.'
#
# Rack trap 22002 - Enclosure Name Changed - without rack UID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22002 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Name has changed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure name changed. (Enclosure: &35, Rack: &26, Enc SN: &40, Enc Model: &45 &46 &47, Enc Spare: &52, SeqNum: &57)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an agent or utility has changed the name of an enclosure within the rack. Each of the components within the rack will be updated to reflect the new enclosure name.'


#
# Rack trap 22003 - Rack Enclosure Removed
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22003*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Removed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure &36 has been removed from Rack &26 (RackUID: &31, Enc Model: &41 &42 &43, Enc SN: &48, Enc Spare: &53, SeqNum: &58)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
#
# Rack trap 22003 - Rack Enclosure Removed without rack UID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22003 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Removed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure &36 has been removed from Rack &26 (Enc Model: &40 &41 &42, Enc SN: &47, Enc Spare: &52, SeqNum: &57)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue


#
# Rack trap 22004 - Rack Enclosure Inserted
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22004*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Inserted'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure &36 has been inserted into Rack &26 (RackUID: &31, Enc Model: &41 &42 &43, Enc SN: &48, Enc Spare: &53, SeqNum: &58)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
#
# Rack trap 22004 - Rack Enclosure inserted without rack UID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22004 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Removed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure &36 has been inserted into Rack &26 (Enc Model: &40 &41 &42, Enc SN: &47, Enc Spare: &52, SeqNum: &57)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue


#
# Rack Trap 22005 - Enclosure temperature failed
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22005*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Temperature Failed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Temperature Failed for Enclosure &36 in Rack &26 (RackUID: &31, Enc SN: &41, TempLocation: &46, Enc Spare: &51, SeqNum: &56)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that a enclosure temperature sensor has been tripped indicating an overheat condition. Shutdown the enclosure and possibly the rack as soon as possible.'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='Insure all fans are working properly and that air flow in the rack has not been blocked.'
#
# Rack Trap 22005 - Enclosure temperature failed without rack UID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22005 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Temperature Failed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Temperature Failed for Enclosure &35 in Rack &26 (Enc SN: &40, TempLocation: &45, Enc Spare: &50, SeqNum: &55)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that a enclosure temperature sensor has been tripped indicating an overheat condition. Shutdown the enclosure and possibly the rack as soon as possible.'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='Insure all fans are working properly and that air flow in the rack has not been blocked.'

#
# Rack Trap 22006 - Enclosure temperature degraded
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22006*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Temperature Degraded'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Temperature Degraded for Enclosure &36 in Rack &26 (RackUID: &31, Enc SN: &41, TempLocation: &46, Enc Spare: &51, SeqNum: &56)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an enclosure temperature sensor has been tripped indicating a possible overheat condition. Shutdown the enclosure and possibly the rack as soon as possible.'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='Insure all fans are working properly and that air flow in the rack has not been blocked.'

#
# Rack Trap 22006 - Enclosure temperature degraded without rack UID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22006 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Temperature Degraded'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Temperature Degraded for Enclosure &35 in Rack &26 (Enc SN: &40, TempLocation: &45, Enc Spare: &50, SeqNum: &55)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an enclosure temperature sensor has been tripped indicating a possible overheat condition. Shutdown the enclosure and possibly the rack as soon as possible.'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='Insure all fans are working properly and that air flow in the rack has not been blocked.'


#
# Rack Trap 22007 - Enclosure Temperature OK
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22007*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Temperature OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Temperature OK for Enclosure &36 in Rack &26 (RackUID: &31, Enc SN: &41, TempLocation: &46, Enc Spare: &51, SeqNum: &56)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
#
# Rack Trap 22007 - Enclosure temperature ok without rack UID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22007 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Temperature OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Temperature Degraded for Enclosure &35 in Rack &26 (Enc SN: &40, TempLocation: &45, Enc Spare: &50, SeqNum: &55)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

#
# Rack Trap 22008 - Enclosure fan failed
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22008*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Fan Failed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure Fan Failed for Enclosure &36 in Rack &26. (RackUID: &31, Enc SN: &41, Fan Location: &46, Fan Spare: &51, SeqNum: &56)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an enclosure fan has failed and no other fans in the redundant fan group are operating. This may result in overheating of the enclosure. Replace the fan as soon as possible.'
#
# Rack Trap 22008 - Enclosure fan failed without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22008 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Fan Failed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure Fan Failed for Enclosure &35 in Rack &26. (Enc SN: &40, Fan Location: &45, Fan Spare: &50, SeqNum: &55)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an enclosure fan has failed and no other fans in the redundant fan group are operating. This may result in overheating of the enclosure. Replace the fan as soon as possible.'


#
# Rack Trap 22009 - Enclosure fan degraded 
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22009*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Fan Degraded'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure Fan Degraded for Enclosure &36 in Rack &26. (RackUID: &31, Enc SN: &41, Fan Location: &46, Fan Spare: &51, SeqNum: &56)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an enclosure fan has failed but other fans in the redundant fan group are still operating. This may result in overheating of the enclosure. Replace the fan as soon as possible.'
#
# Rack Trap 22009 - Enclosure fan failed without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22009 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Fan Degraded'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure Fan Degraded for Enclosure &35 in Rack &26. (Enc SN: &40, Fan Location: &45, Fan Spare: &50, SeqNum: &55)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an enclosure fan has failed but other fans in the redundant fan group are still operating. This may result in overheating of the enclosure. Replace the fan as soon as possible.'

#
# Rack trap 22010 - Enclosure fan OK
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22010*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Fan OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure Fan OK for Enclosure &36 in Rack &26. (RackUID: &31, Enc SN: &41, Fan Location: &46, Fan Spare: &51, SeqNum: &56)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an enclosure fan has returned to normal operation.'
#
# Rack Trap 22010 - Enclosure fan ok without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22010 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Fan OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure Fan OK for Enclosure &35 in Rack &26. (Enc SN: &40, Fan Location: &45, Fan Spare: &50, SeqNum: &55)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that an enclosure fan has failed but other fans in the redundant fan group are still operating. This may result in overheating of the enclosure. Replace the fan as soon as possible.'

#
# Rack trap 22011 - Enclosure Fan Removed
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22011*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Fan Removed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure Fan Removed from Enclosure &36 in Rack &26. (RackUID: &31, Enc SN: &41, Fan Location: &46, Fan Spare: &51, SeqNum: &56)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
#
# Rack Trap 22011 - Enclosure fan removed without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22011 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Fan Removed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure Fan Removed from Enclosure &35 in Rack &26. (Enc SN: &40, Fan Location: &45, Fan Spare: &50, SeqNum: &55)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue


#
# Rack Trap 22012 - Enclosure fan inserted
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22012*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Fan Inserted'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure Fan Inserted into Enclosure &36 in Rack &26. (RackUID: &31, Enc SN: &41, Fan Location: &46, Fan Spare: &51, SeqNum: &56)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
#
# Rack Trap 22012 - Enclosure fan inserted without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22012 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Enclosure Fan Inserted'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Enclosure Fan Inserted into Enclosure &35 in Rack &26. (Enc SN: &40, Fan Location: &45, Fan Spare: &50, SeqNum: &55)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue


#
# Rack Trap 22013 - rack power supply failed
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22013*'
       MSGNODE=*
       DEScription='HP - Rack Power Supply Failed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Supply Failed (Power Supply: &46, PS Enclosure: &36, Rack: &26, RackUID: &31, PS SN: &41, PS Location: &46, PS Firmware: &51, PS Spare: &56, Enc SN: &61, SeqNum: &66)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
#
# Rack Trap 22013 - rack power supply failed without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22013 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Supply Failed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Supply Failed (Power Supply: &45, PS Enclosure: &35, Rack: &26, PS SN: &40, PS Location: &45, PS Firmware: &50, PS Spare: &55, Enc SN: &60, SeqNum: &65)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

#
# Rack Trap 22014 - rack power supply degraded
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22014*'
       MSGNODE=*
       DEScription='HP - Rack Power Supply Degraded'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Supply Degraded (Power Supply: &46, PS Enclosure: &36, Rack: &26, RackUID: &31, PS SN: &41, PS Location: &46, PS Firmware: &51, PS Spare: &56, Enc SN: &61, SeqNum: &66)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
#
# Rack Trap 22014 - rack power supply failed without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22014 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Supply Degraded'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Supply Degraded (Power Supply: &45, PS Enclosure: &35, Rack: &26, PS SN: &40, PS Location: &45, PS Firmware: &50, PS Spare: &55, Enc SN: &60, SeqNum: &65)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

#
# Rack Trap 22015 - rack power supply ok
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22015*'
       MSGNODE=*
       DEScription='HP - Rack Power Supply OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Supply OK (Power Supply: &46, PS Enclosure: &36, Rack: &26, RackUID: &31, PS SN: &41, PS Location: &46, PS Firmware: &51, PS Spare: &56, Enc SN: &61, SeqNum: &66)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green
#
# Rack Trap 22015 - rack power supply ok without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22015 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Supply OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Supply OK (Power Supply: &45, PS Enclosure: &35, Rack: &26, PS SN: &40, PS Location: &45, PS Firmware: &50, PS Spare: &55, Enc SN: &60, SeqNum: &65)'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

#
# Rack Trap 22016 - rack power supply removed
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22016*'
       MSGNODE=*
       DEScription='HP - Rack Power Supply Removed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Supply Removed (PS Enclosure: &36, Rack: &26, RackUID: &31, Power Supply: &46, PS SN: &41, PS Location: &46, PS Firmware: &51, PS Spare: &56, Enc SN: &61, SeqNum: &66)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
#
# Rack Trap 22016 - rack power supply removed without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22016 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Supply Removed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Supply Removed (PS Enclosure: &35, Rack: &26, Power Supply: &45, PS SN: &40, PS Location: &45, PS Firmware: &50, PS Spare: &55, Enc SN: &60, SeqNum: &65)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

#
# Rack Trap 22017 - rack power supply inserted
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22017*'
       MSGNODE=*
       DEScription='HP - Rack Power Supply Inserted'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Supply Inserted (PS Enclosure: &36, Rack: &26, RackUID: &31, Power Supply: &46, PS SN: &41, PS Location: &46, PS Firmware: &51, PS Spare: &56, Enc SN: &61, SeqNum: &66)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
#
# Rack Trap 22017 - rack power supply inserted without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22017 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Supply Inserted'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Supply Inserted (PS Enclosure: &35, Rack: &26, Power Supply: &45, PS SN: &40, PS Location: &45, PS Firmware: &50, PS Spare: &55, Enc SN: &60, SeqNum: &65)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

#
# Rack Trap 22018 - rack power subsystem not redundant
# 
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22018*'
       MSGNODE=*
       DEScription='HP - Rack Power Subsystem not Redundant'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Subsystem no longer redundant for Enclosure &36, Rack &26. (RackUID: &31, Enc SN: &41, SeqNum: &46)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
#
# Rack Trap 22018 - rack power subsystem not redundant without rackUID sent
# 
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22018 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Subsystem not Redundant'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Subsystem no longer redundant for Enclosure &35, Rack &26. (Enc SN: &40, SeqNum: &45)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

#
# Trap 22019
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22019*'
       MSGNODE=*
       DEScription='HP - Rack Power Subsystem Line Voltage Problem'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Subsystem Line Voltage Problem (Power Supply: &41, PS Enclosure &36, Rack &26, RackUID: &31, PS Firmware: &46, PS Line Status: &51, PS Spare: &56, Enc SN: &61, SeqNum: &66)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The rack power supply detected an input line voltage problem. Check the power input for the power supply or replace any failed power supplies as soon as possible.'

#
# Trap 22019 without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22019 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Subsystem Line Voltage Problem'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Subsystem Line Voltage Problem (Power Supply: &40, PS Enclosure &35, Rack &26, PS Firmware: &45, PS Line Status: &50, PS Spare: &55, Enc SN: &60, SeqNum: &65)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The rack power supply detected an input line voltage problem. Check the power input for the power supply or replace any failed power supplies as soon as possible.'

#
# Trap 22020
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22020*'
       MSGNODE=*
       DEScription='HP - Rack Power Subsystem Overload Condition'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Subsystem Overload Condition (PS Enclosure: &36, Rack: &26, RackUID: &31, Enc Spare: &41, Enc SN: &46, SeqNum: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The rack power subsystem overload condition. Replace any failed power supplies as soon as possible to return the system to a redundant state.'
#
# Trap 22020 without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22020 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Subsystem Overload Condition'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Subsystem Overload Condition (PS Enclosure: &35, Rack: &26, Enc Spare: &40, Enc SN: &45, SeqNum: &50)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The rack power subsystem overload condition. Replace any failed power supplies as soon as possible to return the system to a redundant state.'


#
# Trap 22021
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22021*'
       MSGNODE=*
       DEScription='HP - Rack Power Shed Auto Shutdown'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Server Shutdown due to lack of Power (Blade: &41, Blade Enclosure: &36, Rack: &26, RackUID: &31, Blade Spare: &46, Enc SN: &51, SeqNum: &56)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The server blade was shutdown due to a lack of power. Check power connections or add power supplies.'
#
# Trap 22021 - without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22021 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Shed Auto Shutdown'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Server Shutdown due to lack of Power (Blade: &40, Blade Enclosure: &35, Rack: &26, Blade Spare: &45, Enc SN: &50, SeqNum: &55)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The server blade was shutdown due to a lack of power. Check power connections or add power supplies.'

#
# Trap 22022
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22022*'
       MSGNODE=*
       DEScription='HP - Rack Server Power on Failed - not Redundant'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Server power on prevented to preserve reundancy (Blade: &41, Blade Enclosure: &36, Rack: &26, RackUID: &31, Blade Spare: &46, Enc SN: &51, SeqNum: &56)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is not enough power to power on the server blade and maintain redundancy for the other blades in the enclosure. Check power connections or add power supplies.'
#
# Trap 22022 without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22022 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Server Power on Failed - not Redundant'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Server power on prevented to preserve reundancy (Blade: &40, Blade Enclosure: &35, Rack: &26, Blade Spare: &45, Enc SN: &50, SeqNum: &55)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is not enough power to power on the server blade and maintain redundancy for the other blades in the enclosure. Check power connections or add power supplies.'

#
# Trap 22023
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22023*'
       MSGNODE=*
       DEScription='HP - Rack Server Power on Failed - not enough power'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack - Inadequate power to power on blade. (Blade: &41, Blade Enclosure: &36, Rack: &26, RackUID: &31, Blade Spare: &46, Enc SN: &51, SeqNum: &56)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is not enough power to power on the server blade. Check power connections or add power supplies.'
#
# Trap 22023 without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22023 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Server Power on Failed - not enough power'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack - Inadequate power to power on blade. (Blade: &40, Blade Enclosure: &35, Rack: &26, Blade Spare: &45, Enc SN: &50, SeqNum: &55)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is not enough power to power on the server blade. Check power connections or add power supplies.'

#
# Rack Trap 22024 - rack server power on failed
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22024*'
       MSGNODE=*
       DEScription='HP - Rack Server Power on Failed - enclosure not found'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack - Inadequate power to power on blade. (Blade: &41, Blade Enclosure: &36, Rack: &26, RackUID: &31, Blade Spare: &46, Enc SN: &51, SeqNum: &56)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is not enough power to power on the server blade. The server enclosure micro-controller was not found. Check server enclosure connections or add power supplies.'
#
# Rack Trap 22024 - rack server power on failed without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22024 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Server Power on Failed - enclosure not found'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack - Inadequate power to power on blade. (Blade: &40, Blade Enclosure: &35, Rack: &26, Blade Spare: &45, Enc SN: &50, SeqNum: &55)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is not enough power to power on the server blade. The server enclosure micro-controller was not found. Check server enclosure connections or add power supplies.'

#
# Rack Trap 22025 - rack server power on failed
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22025*'
       MSGNODE=*
       DEScription='HP - Rack Server Power on Failed - power chassis not found'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack - Inadequate power to power on blade. (Blade: &41, Blade Enclosure: &36, Rack: &26, RackUID: &31, Blade Spare: &46, Enc SN: &51, SeqNum: &56)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is not enough power to power on the server blade. The power enclosure micro-controller was not found. Check power enclosure connections or add power supplies.'
#
# Rack Trap 22025 - rack server power on failed without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22025 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Server Power on Failed - power chassis not found'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack - Inadequate power to power on blade. (Blade: &40, Blade Enclosure: &35, Rack: &26, Blade Spare: &45, Enc SN: &50, SeqNum: &55)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is not enough power to power on the server blade. The power enclosure micro-controller was not found. Check power enclosure connections or add power supplies.'

#
# Rack trap 22026 - server power on manual override
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22026*'
       MSGNODE=*
       DEScription='HP - Rack Server Power on Manual Override'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Server Power on via Manual Override. (Blade: &41, Blade Enclosure: &36, Rack: &26, RackUID: &31, Blade Spare: &46, Enc SN: &51, SeqNum: &56)'
       SEVERITY=w
       ATTRIB=default
       COLOR=orange
#
# Rack trap 22026 - server power on manual override without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22026 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Server Power on Manual Override'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Server Power on via Manual Override. (Blade: &40, Blade Enclosure: &35, Rack: &26, Blade Spare: &45, Enc SN: &50, SeqNum: &55)'
       SEVERITY=w
       ATTRIB=default
       COLOR=orange

#
# Rack trap 22027 - rack fuse open
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22027*'
       MSGNODE=*
       DEScription='HP - Rack Fuse Open'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Fuse Open. (Fuse: &41, Enclosure: &36, Rack: &26, RackUID: &31, Enc Spare: &46, Enc SN: &51, SeqNum: &56)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
#
# Rack trap 22027 - rack fuse open without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22027 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Fuse Open'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Fuse Open. (Fuse: &40, Enclosure: &35, Rack: &26, Enc Spare: &45, Enc SN: &50, SeqNum: &55)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

#
# Rack trap 22028 - server blade removed
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22028*'
       MSGNODE=*
       DEScription='HP - Rack Server Blade Removed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Server Blade Removed. (Blade: &41, Blade Enclosure: &36, Rack: &26, RackUID: &31, Blade Position: &46, Blade Spare: &51, Enc SN: &56, SeqNum: &61)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
#
# Rack trap 22028 - server blade removed without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22028 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Server Blade Removed'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Server Blade Removed. (Blade: &40, Blade Enclosure: &35, Rack: &26, Blade Position: &45, Blade Spare: &50, Enc SN: &55, SeqNum: &60)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

#
# Rack trap 22029 - server blade inserted
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22029*'
       MSGNODE=*
       DEScription='HP - Rack Server Blade Inserted'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Server Blade Inserted. (Blade: &41, Blade Enclosure: &36, Rack: &26, RackUID: &31, Blade Position: &46, Blade Spare: &51, Enc SN: &56, SeqNum: &61)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
# 
# Rack trap 22029 - server blade inserted without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22029 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Server Blade Inserted'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Server Blade Inserted. (Blade: &40, Blade Enclosure: &35, Rack: &26, Blade Position: &45, Blade Spare: &50, Enc SN: &55, SeqNum: &60)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

#
# Rack Trap 22030 - power chassis not load balanced
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22030*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis not load balanced'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis not load balanced. (Enclosure: &36, Rack: &26, RackUID: &31, Enc SN: &41, Enc Spare: &46, SeqNum: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The power subsystem is out of balance for this power enclosure. Check the power enclosure and power supplies.  Replace any failed or degraded power supplies.  Add additional power supplies if needed.'
#
# Rack Trap 22030 - power chassis not load balanced without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22030 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis not load balanced'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis not load balanced. (Enclosure: &35, Rack: &26, Enc SN: &40, Enc Spare: &45, SeqNum: &50)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The power subsystem is out of balance for this power enclosure. Check the power enclosure and power supplies.  Replace any failed or degraded power supplies.  Add additional power supplies if needed.'

#
# Rack trap 22031 - dc power problem
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22031*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis - DC Power Problem'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis DC Power Problem. (Enclosure: &36, Rack: &26, RackUID: &31, Enc SN: &41, Enc Spare: &46, SeqNum: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is a power subsystem DC power problem for this power enclosure. Check the power enclosure and power supplies.  Replace any failed or degraded power supplies.'
#
# Rack trap 22031 - dc power problem without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22031 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis - DC Power Problem'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis DC Power Problem. (Enclosure: &35, Rack: &26, Enc SN: &40, Enc Spare: &45, SeqNum: &50)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is a power subsystem DC power problem for this power enclosure. Check the power enclosure and power supplies.  Replace any failed or degraded power supplies.'

#
# Rack Trap 22032 - ac facility power exceeded
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22032*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis - AC Facility Power Exceeded'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis AC Facility Power Exceeded. (Enclosure: &36, Rack: &26, RackUID: &31, Enc SN: &41, Enc Spare: &46, SeqNum: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is a Power subsystem AC facility input power exceeded for this power enclosure. Check the power enclosure and power supplies.  Replace any failed or degraded power supplies.'
#
# Rack Trap 22032 - ac facility power exceeded without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22032 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis - AC Facility Power Exceeded'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis AC Facility Power Exceeded. (Enclosure: &35, Rack: &26, Enc SN: &40, Enc Spare: &45, SeqNum: &50)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is a Power subsystem AC facility input power exceeded for this power enclosure. Check the power enclosure and power supplies.  Replace any failed or degraded power supplies.'

#
# Rack Trap 22033 - unknown power consumption
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22033*'
       MSGNODE=*
       DEScription='HP - Rack Power Unknown Power Consumption'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Unknown Power Consumption. (Rack: &26, RackUID: &31, Enc SN: &36, SeqNum: &41)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is an unknown power consumer drawing power. Check the power enclosure and power supplies.  Replace any failed or degraded power supplies.'
#
# Rack Trap 22033 - unknown power consumption without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22033 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Unknown Power Consumption'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Unknown Power Consumption. (Rack: &26, Enc SN: &35, SeqNum: &40)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='There is an unknown power consumer drawing power. Check the power enclosure and power supplies.  Replace any failed or degraded power supplies.'

#
# Rack Trap 22034 - load balancing wire missing
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22034*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis Load Balancing Wire Missing'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis Load Balancing Wire Missing. (Enclosure: &36, Rack: &26, RackUID: &31, Enc SN: &41, Enc Spare: &46, SeqNum: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The power subsystem load balancing wire is missing. Connect the load balancing wire.'
#
# Rack Trap 22034 - load balancing wire missing without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22034 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis Load Balancing Wire Missing'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis Load Balancing Wire Missing. (Enclosure: &35, Rack: &26, Enc SN: &40, Enc Spare: &45, SeqNum: &50)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The power subsystem load balancing wire is missing. Connect the load balancing wire.'

#
# Rack trap 22035 - too many power chassis
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22035*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis - Too Many Power Chassis'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis - Too Many Power Chassis. (Enclosure: &36, Rack: &26, RackUID: &31, Enc SN: &41, SeqNum: &46)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The maximum number of power enclosures has been exceeded. Remove the extra power enclosure.'
#
# Rack trap 22035 - too many power chassis without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22035 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis - Too Many Power Chassis'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis - Too Many Power Chassis. (Enclosure: &35, Rack: &26, Enc SN: &40, SeqNum: &45)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The maximum number of power enclosures has been exceeded. Remove the extra power enclosure.'

#
# Rack Trap 22036 - power chassis config error
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22036*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis Config Error'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis Config Error. (Enclosure: &36, Rack: &26, RackUID: &31, Enc SN: &41, Enc Spare: &46, SeqNum: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The power subsystem has been improperly configured. Check the cabling of the power enclosure.'
#
# Rack Trap 22036 - power chassis config error without rackUID sent
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 22036 * * * * * * * * * * * * * * * * * * * * * OID:*'
       MSGNODE=*
       DEScription='HP - Rack Power Chassis Config Error'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Rack Power Chassis Config Error. (Enclosure: &35, Rack: &26, Enc SN: &40, Enc Spare: &45, SeqNum: &50)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='The power subsystem has been improperly configured. Check the cabling of the power enclosure.'


