#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8008 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - A systems fan status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - System fan status: OTHER'
       SEVERITY=I
       ATTRIB=DEFAULT
       COLOR=BLUE

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8008 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - A systems fan status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Systems fan status is OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8008 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - A systems fan status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - System fan has FAILED'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8008 * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - system fan status: NO FAN'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - System does not support fan monitoring'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8008 * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - system fan status: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - system fan status: DEGRADED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8009 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - The Storage System temp failed status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Storage System Temperature Failed status has a status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8009 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - The Storage System temp failed status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Failed status is OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8009 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - The Storage System temp failed status: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Failed status has DEGRADED AND MAY SHUTDOWN'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8009 * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - The Storage System temp failed status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Failed status has FAILED AND MAY SHUTDOWN'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8009 * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - The Storage System temp failed status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Failed status is NOT SUPPORTED'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8010 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System temp degraded status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Storage System Temperature Degraded status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8010 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System temp degraded status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Degraded status is OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8010 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System temp degraded status: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Degraded status has DEGRADED AND MAY SHUTDOWN'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8010 * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System temp degraded status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Degraded status has FAILED AND MAY SHUTDOWN'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8010 * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Storage System temp degraded status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Degraded status is NOT SUPPORTED'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8011 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System temp ok status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Storage System Temperature Ok status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8011 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - The Storage System temp ok status: OK'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Ok status is OK'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8011 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - The Storage System temp ok status: DEGRADED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Ok status has DEGRADED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8011 * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - The Storage System temp ok status: FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System Temperature Ok status has FAILED AND MAY SHUTDOWN'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8011 * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - The Storage System temp ok status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Storage System Temperature Ok status is NOT SUPPORTED'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8012 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System side panel in place status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Storage System side panel in place status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8012 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System side panel in place status: SIDE PANEL IN PLACE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System side panel in place status is IN PLACE'
       SEVERITY=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8012 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System side panel in place status: SIDE PANEL REMOVED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage System side panel in place status has been REMOVED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8012 * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System side panel in place status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendoper TEXT='HP - Storage System side panel in place status is NOT SUPPORTED'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8013 * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System side panel removed status: OTHER'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)       
       ACTION=sendoper TEXT='HP - Storage System side panel removed status: OTHER'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8013 * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System side panel removed status: SIDE PANEL IN PLACE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)       
       ACTION=sendkeep TEXT='HP - Storage System side panel removed status IS IN PLACE'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue
       
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8013 * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System side panel removed status: SIDE PANEL REMOVED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)       
       ACTION=sendkeep TEXT='HP - Storage System side panel removed status has been installed improperly and improper cooling of drives may result' 
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8013 * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System side panel removed status: NOT SUPPORTED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)       
       ACTION=sendoper TEXT='HP - Storage System side panel removed status is NOT SUPPORTED'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8014*'
       MSGNODE=*
       DEScription='HP - The Storage Systems redundant power supply degrading'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Storage Systems redundant power supply degraded status is DEGRADED'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
