#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 5 * * * * * * * * 1.3.6.1.4.1.232.141.2.3*'
       MSGNODE=*
       DEScription='HP - Clustered RAID Logical Drive Information Trap: Status OPTIMAL'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Clustered RAID Logical Drive Status: OPTIMAL (Logical Drive Index &21)'
       SEVerity=S
       ATTRIB=default
       COLOR=GREEN
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='A logical drive has become optimal due to a successful completion of the reconstruction process.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 6 * * * * * * * * 1.3.6.1.4.1.232.141.2.3*'
       MSGNODE=*
       DEScription='HP - Clustered RAID Logical Drive Failed Trap'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Clustered RAID Logical Drive Status: FAILED (Logical Drive Index &21)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The logical drive has failed and is off-line.  Possible cause is too many failed disk drives that make up the LUN or the OS can no longer communicate with the LUN for other reasons.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 7 * * * * * * * * 1.3.6.1.4.1.232.141.2.3*'
       MSGNODE=*
       DEScription='HP - Clustered RAID Logical Drive RECONSTRUCTING Trap'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Clustered RAID Logical Drive Status: RECONSTRUCTING (Logical Drive Index &21)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The LUN has started the reconstruction process but is available for normal use.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='Possible causes are an available disk drive was created as a spare to be inserted into the set or an existing spare was automatically added to the set for reconstruction upon failure of a member disk device.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8 * * * * * * * * 1.3.6.1.4.1.232.141.2.3*'
       MSGNODE=*
       DEScription='HP - Clustered RAID Logical Drive Reduced Trap'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Clustered RAID Logical Drive Status: REDUCED (Logical Drive Index &21)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='A logical drive has become degraded due to a member disk device failure.  Replace the failed disk device; add a spare to the system to cause a reconstruct.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 9 * * * * * * * * 1.3.6.1.4.1.232.141.2.3*'
       MSGNODE=*
       DEScription='HP - Clustered RAID Logical Drive Initializing Trap'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Clustered RAID Logical Drive Status: INITIALIZING (Logical Drive Index &21)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue



DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 10 * * * * * * * * 1.3.6.1.4.1.232.141.2.5*'
       MSGNODE=*
       DEScription='HP - Clustered RAID Physical Drive RECOVERED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Clustered RAID Physical Drive Status: RECOVERED (Controller Index &21, Drive Index &26)'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 11 * * * * * * * * 1.3.6.1.4.1.232.141.2.5*'
       MSGNODE=*
       DEScription='HP - Clustered RAID Physical Drive FAILED'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Clustered RAID Physical Drive Status: FAILED (Controller Index &21, Drive Index &26)'
       SEVerity=E
       ATTRIB=default
       COLOR=RED

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 12 * * * * * * * * 1.3.6.1.4.1.232.141.2.5*'
       MSGNODE=*
       DEScription='HP - Clustered RAID Physical Drive RECONSTRUCTING'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Clustered RAID Physical Drive Status: RECONSTRUCTING (Drive Index &21)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='A disk member of a logical drive has begun the reconstruction process and will be available for use when reconstruction is complete.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 13 * * * * * * * * 1.3.6.1.4.1.232.141.2.5*'
       MSGNODE=*
       DEScription='HP - Clustered RAID Physical Drive AVAILABLE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Clustered RAID Physical Drive Status: AVAILABLE (Drive Index &21)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='A disk drive has been physically added or set to the Available state. It can be used as a RAIDset member or as a Spare.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 14 * * * * * * * * 1.3.6.1.4.1.232.141.2.5*'
       MSGNODE=*
       DEScription='HP - Clustered RAID Physical Drive SPARE'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - Clustered RAID Physical Drive has been made a spare (Drive Index &21)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='A disk drive has been set to Spare status from Available and may be used in a RAID 1, RAID 0+1 or RAID 5 logical disk should a member device fail in one of those RAID sets.'



