#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************

#-------------------------------
# Definition for trap 8022
#-------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8022*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status Change (8022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status Change.  Consult the original event for more information. (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The agent has detected a change in the fan status of a storage system.  The variable cpqSsBackplaneFanStatus indicates the current fan status, but that information could not be parsed.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='The last variable in the trap is cpqSsBackplaneFanStatus.  The status variable may have values of other(1), notInstalled(2), ok(3), degraded(4), or failed(5).'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status Change: OTHER (8022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status Change: OTHER (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status Change: Not Installed (8022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status Change: Not Installed (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status Change: OK (8022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status Change: OK (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=I
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status Change: DEGRADED (8022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status Change: DEGRADED (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8022 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Storage System Fan Status Change: FAILED (8022)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Fan Status Change: FAILED (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

#----------------------------------------
# Definition for trap 8023
#----------------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8023*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status Change (8023)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status Change.  Consult the original event for more information. (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The agent has detected a change in the status of the temperature in a storage system.  The variable cpqSsBackplaneTempStatus indicates the current status, but that information could not be parsed.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='The last variable in the trap is cpqSsBackplaneTempStatus.  The status variable may have values of other(1), noTemp(2), ok(3), degraded(4), or failed(5).'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status Change: OTHER (8023)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status Change: OTHER (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status Change: No Temp (8023)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status Change: No Temp (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status Change: OK (8023)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status Change: OK (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=I
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status Change: DEGRADED (8023)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status Change: DEGRADED (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8023 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Storage System Temperature Status Change: FAILED (8023)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Temperature Status Change: FAILED (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red



#--------------------------------
# Definition for trap 8024
#--------------------------------

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8024*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status Change (8024)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status Change.  Consult the original event for more information. (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion NAME=(*,20)
       ACTION=ANNOTATE TEXT='The agent has detected a change in the power supply status of a storage system.  The variable cpqSsBackplaneFtpsStatus indicates the current status, but that information could not be parsed.'
DEFine MSGACTion NAME=(*,30)
       ACTION=ANNOTATE TEXT='The last variable in the trap is cpqSsBackplaneFtpsStatus.  The status variable may have values of other(1), noFltTolPower(2), ok(3), degraded(4), or failed(5).'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8024 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status Change: OTHER (8024)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status Change: OTHER (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8024 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status Change: No Fault Tolerant Power (8024)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status Change: No Fault Tolerant Power (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=I
       ATTRIB=default
       COLOR=blue

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8024 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status Change: OK (8024)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status Change: OK (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=I
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8024 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status Change: DEGRADED (8024)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status Change: DEGRADED (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=W
       ATTRIB=default
       COLOR=orange

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 8024 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - Storage System Power Supply Status Change: FAILED (8024)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep 
       TEXT='HP - Storage System Power Supply Status Change: FAILED (Chassis Name: &26, Chassis Time: &31, Backplane Index: &36, Backplane Vendor: &41,  Backplane Model: &46, Backplane S/N: &51)'
       SEVERITY=E
       ATTRIB=default
       COLOR=red

