#* **************************************************************************
#*
#*                  Insight Integration for CA Unicenter
#*
#*      Copyright 1996,2003 Hewlett-Packard Development Company, L.P.
#*
#*      Hewlett-Packard Company shall not be liable for technical or
#*      editorial errors or omissions contained herein. The information in
#*      this document is provided "as is" without warranty of any kind and
#*      is subject to change without notice. The warranties for HP products
#*      are set forth in the express limited warranty statements
#*      accompanying such products. Nothing herein should be construed as
#*      constituting an additional warranty.
#*
#*      Confidential computer software. Valid license from HP required for
#*      possession, use or copying. Consistent with FAR 12.211 and 12.212,
#*      Commercial Computer Software, Computer Software Documentation, and
#*      Technical Data for Commercial Items are licensed to the U.S.
#*      Government under vendor's standard commercial license.
#*
#* **************************************************************************
#*                                                                        
#* PROPRIETARY NOTE:                                                      
#*     This document contains information confidential and proprietary to 
#*     Hewlett-Packard and shall not be reproduced or transferred to other
#*     documents or disclosed to others or used for any purpose other than 
#*     that for which it was obtained without the expressed written consent
#*     of Hewlett-Packard Company.
#*                                                                        
#* **************************************************************************
#
# Fibre Channel Array traps from version 5.40 to 6.40 of the management agents
#

#
# FCA trap 16026
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16026*'
       MSGNODE=*
       DEScription='HP - External Tape Library Status Change (16026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Library Status Change (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41, Data: &(46:))'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external tape library.  The last variable (cpqFcTapeLibraryStatus) indicates the current tape library status.'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The tape library may have the following status: other(1), ok(2), degraded(3), failed(4), or offline(5). User Action: If the tape library is failed or offline, check the tape library front panel and all connections.'


DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16026 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - External Tape Library Status Other(16026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Library Status Other (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41, Model: &46 &47, Firmware: &52, SN: &57, Location: &62 &63)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external tape library.  User Action: If the tape library is failed or offline, check the tape library front panel and all connections.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16026 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - External Tape Library Status Ok(16026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Library Status Ok (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41, Model: &46 &47, Firmware: &52, SN: &57, Location: &62 &63)'
       SEVerity=S
       ATTRIB=default
       COLOR=green

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16026 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - External Tape Library Status Degraded(16026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Library Status Degraded (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41, Model: &46 &47, Firmware: &52, SN: &57, Location: &62 &63)'
       SEVerity=W
       ATTRIB=default
       COLOR=orange
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external tape library.  User Action: If the tape library is failed or offline, check the tape library front panel and all connections.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16026 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - External Tape Library Status Failed (16026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Library Status Failed (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41, Model: &46 &47, Firmware: &52, SN: &57, Location: &62 &63)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external tape library.  User Action: If the tape library is failed or offline, check the tape library front panel and all connections.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16026 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 5*'
       MSGNODE=*
       DEScription='HP - External Tape Library Status Offline (16026)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Library Status Offline (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41, Model: &46 &47, Firmware: &52, SN: &57, Location: &62 &63)'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the status of an external tape library.  User Action: If the tape library is failed or offline, check the tape library front panel and all connections.'


#
# FCA trap 16027
#
DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16027*'
       MSGNODE=*
       DEScription='HP - External Tape Library Door Status Change (16027)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Library Door Status Change (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41, Data: &(46:))'
       SEVerity=E
       ATTRIB=default
       COLOR=red
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the door status of a Compaq External Tape library.  The last variable (cpqFcTapeLibraryDoorStatus) indicates the current tape library door status.'
DEFine MSGACTion Name=(*,30)
       ACTION=ANNOTATE TEXT='The tape library door may have the following status: other(1), notSupported(2), closed(3), or open(4). User Action: If the tape library door is open, close the tape library door.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16027 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 1*'
       MSGNODE=*
       DEScription='HP - External Tape Library Door Status Other (16027)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Library Door Status Other (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41, Model: &46 47, Firmware: &52, SN: &57, Location: &62 &63)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the door status of an External Tape library.  User Action: If the tape library door is open, close the tape library door.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16027 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 2*'
       MSGNODE=*
       DEScription='HP - External Tape Library Door Status NotSupported (16027)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Library Door Status NotSupported (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41, Model: &46 47, Firmware: &52, SN: &57, Location: &62 &63)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the door status of an External Tape library.  User Action: If the tape library door is open, close the tape library door.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16027 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 3*'
       MSGNODE=*
       DEScription='HP - External Tape Library Door Status Closed (16027)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Library Door Status Closed (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41, Model: &46 47, Firmware: &52, SN: &57, Location: &62 &63)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the door status of an External Tape library.  User Action: If the tape library door is open, close the tape library door.'

DEFine MSGREcord MSGID='* SNMPTRAP: * * *232 * * 6 16027 * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * * 4*'
       MSGNODE=*
       DEScription='HP - External Tape Library Door Status Open (16027)'
       TYPE=MSG
DEFine MSGACTion NAME=(*,10)
       ACTION=sendkeep TEXT='HP - External Tape Library Door Status Open (Controller Index: &26, Bus: &31, SCSI ID: &36, LUN: &41, Model: &46 47, Firmware: &52, SN: &57, Location: &62 &63)'
       SEVerity=I
       ATTRIB=default
       COLOR=blue
DEFine MSGACTion Name=(*,20)
       ACTION=ANNOTATE TEXT='This trap signifies that the agent has detected a change in the door status of an External Tape library.  User Action: If the tape library door is open, close the tape library door.'


