  	                          Installation Notes 
        	                         for 
                     Insight Manager for HP OpenView NNM on Windows
                    ------------------------------------------------

Version : 3.2 
Dated   : August 1, 2005


Installation Procedure
----------------------

The below mentioned step by step procedure needs to be followed to install the
Insight Integration for HP OpenView Network Node Manager revision 3.2.  

Installation is supported on Windwos 2000, Windows 2003 and Windows XP.
HP OpenView NNM versions 6.3x, 6.4, and 7.x are supported.


1. Login as Administrator.

2. Verify that there is at least 10 MB of free disk space in the file system
   where HP OpenView NNM is installed. Copy the imovwin30.zip file to any 
   directory on the drive. 
  
3. Stop the HP OpenView GUI if it is running. Close all ovw sessions. Click on
   the "NNM Services Stop" icon in the program menu or run the command
   "%OV_BIN%\ovstop" at the command prompt. 
  
4. Unzip imovwin32.zip to extract all the required files to the temporary
   directory.

5. Open a command prompt and change to the directory where the files were
   extracted (imovwin32 by default).

6. Run "cpqinstall.cmd" to install the Insight Integration. 
  
7. This application requires either Netscape Communicator (ver 4.78 or above),
   Internet Explorer (ver 5.5 or above), or Mozilla (version 1.2 or above) to be
   configured as the default browser to view the device home page of the 
   web enabled HP Management Agents.

  

Deleting Integration Objects/Symbols
------------------------------------

For deleting the integration specific objects and symbols, the below 
mentioned steps should be followed:

1. start ovw.

2. For each of the maps, the below mentioned steps should be followed,
    - Open the map.
    - Select "Map->Properties..." menu item.
    - Select the Applications tab in the Map Properties dialog.
    - Select "Insight Integration for HP OpenView NNM" from the "Configurable Applications:"
      section in the "Map Properties" dialog box.
    - Click "Configure For This Map ..." button.
    - Select "Proceed with deleting Insight Manager Symbols & Objects from this map" option.
    - Select "True" option in the "Configuration" dialog box.
    - Click "Verify" button in the "Configuration" dialog box.
    - Click "OK" button in the "Configuration" dialog box.

3. Exit ovw.


Configuring Insight Integration Applications
--------------------------------------------

For launching Systems Insight Manager, the steps mentioned below should be 
followed :

1.  Open the map.
2.  Select "Map->Properties..."menu item.
3.  Select the Applications tab in the Map Properties dialog.
4.  Select "Insight Integration for HP OpenView NNM" from the "Configurable Applications:"
    section in the "Map Properties" dialog box.
5.  Click "Configure For this Map..." button.
6.  Select "Enter the IP address for launching Insight Manager" option.
7.  Enter the IP Address of machine where Systems Insight Manager is installed.
8.  Click "Verify" button in the "Configuration" dialog box.
9.  Click "OK" button in the "Configuratiom" dialog box.
10. Select "Monitor->HP..." menu item and click on "Insight Manager Home".


Documentation
-------------

The documentation for this product (the user guide) is a PDF file located 
in the \docs directory.
	
	

